// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		label-mac-device = &eth0;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001919>;

	phy-mode = "sgmii";
	phy-handle = <&phy0>;

	nvmem-cells = <&macaddr_factory_1002>;
	nvmem-cell-names = "mac-address";
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,mib-poll-interval = <500>;

		qca,ar8327-initvals = <
			0x04 0x80080080 /* PORT0 PAD MODE CTRL */
			0x08 0x00000000 /* PORT5 PAD MODE CTRL */
			0x0c 0x00000000 /* PORT6 PAD MODE CTRL */
			0x10 0x00000080 /* POWER_ON_STRAP */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x00000200 /* PORT6_STATUS */
			>;
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0 0 0 0 0>;

		nvmem-cells = <&precal_factory_5000>;
		nvmem-cell-names = "pre-calibration";
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;
		m25p,fast-read;

		mtdparts: partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "Bootloader";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "nvram";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				label = "Factory";
				reg = <0x050000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					cal_factory_1000: cal@1000 {
						reg = <0x1000 0x440>;
					};

					macaddr_factory_1002: macaddr@1002 {
						reg = <0x1002 0x6>;
					};

					precal_factory_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
		};
	};
};

&wmac {
	/* Does not work due to lack of QCN5502 support in ath9k. */
	status = "disabled";

	nvmem-cells = <&cal_factory_1000>;
	nvmem-cell-names = "calibration";
};
