From: George Moussalem <george.moussalem@outlook.com>
Date: Tue, 07 Jan 2025 17:34:13 +0400
Subject: [PATCH] phy: qualcomm: qcom-uniphy-pcie 28lp add support for IPQ5018

The Qualcomm UNIPHY PCIe PHY 28lp is found on both IPQ5332 and IPQ5018.
Adding the PHY init sequence, pipe clock rate, and compatible for IPQ5018.

Signed-off-by: George Moussalem <george.moussalem@outlook.com>
---
--- a/drivers/phy/qualcomm/phy-qcom-uniphy-pcie-28lp.c
+++ b/drivers/phy/qualcomm/phy-qcom-uniphy-pcie-28lp.c
@@ -76,6 +76,40 @@ struct qcom_uniphy_pcie {
 
 #define phy_to_dw_phy(x)	container_of((x), struct qca_uni_pcie_phy, phy)
 
+static const struct qcom_uniphy_pcie_regs ipq5018_regs[] = {
+	{
+		.offset = SSCG_CTRL_REG_4,
+		.val = 0x1cb9,
+	}, {
+		.offset = SSCG_CTRL_REG_5,
+		.val = 0x023a,
+	}, {
+		.offset = SSCG_CTRL_REG_3,
+		.val = 0xd360,
+	}, {
+		.offset = SSCG_CTRL_REG_1,
+		.val = 0x1,
+	}, {
+		.offset = SSCG_CTRL_REG_2,
+		.val = 0xeb,
+	}, {
+		.offset = CDR_CTRL_REG_4,
+		.val = 0x3f9,
+	}, {
+		.offset = CDR_CTRL_REG_5,
+		.val = 0x1c9,
+	}, {
+		.offset = CDR_CTRL_REG_2,
+		.val = 0x419,
+	}, {
+		.offset = CDR_CTRL_REG_1,
+		.val = 0x200,
+	}, {
+		.offset = PCS_INTERNAL_CONTROL_2,
+		.val = 0xf101,
+	},
+};
+
 static const struct qcom_uniphy_pcie_regs ipq5332_regs[] = {
 	{
 		.offset = PHY_CFG_PLLCFG,
@@ -89,6 +123,14 @@ static const struct qcom_uniphy_pcie_reg
 	},
 };
 
+static const struct qcom_uniphy_pcie_data ipq5018_data = {
+	.lane_offset	= 0x800,
+	.phy_type	= PHY_TYPE_PCIE_GEN2,
+	.init_seq	= ipq5018_regs,
+	.init_seq_num	= ARRAY_SIZE(ipq5018_regs),
+	.pipe_clk_rate	= 125000000,
+};
+
 static const struct qcom_uniphy_pcie_data ipq5332_data = {
 	.lane_offset	= 0x800,
 	.phy_type	= PHY_TYPE_PCIE_GEN3,
@@ -212,6 +254,9 @@ static inline int phy_pipe_clk_register(
 
 static const struct of_device_id qcom_uniphy_pcie_id_table[] = {
 	{
+		.compatible = "qcom,ipq5018-uniphy-pcie-phy",
+		.data = &ipq5018_data,
+	}, {
 		.compatible = "qcom,ipq5332-uniphy-pcie-phy",
 		.data = &ipq5332_data,
 	}, {
