From 2a2858bc1420f940eb70464fafe2db08bce2be8a Mon Sep 17 00:00:00 2001
From: Tomi Valkeinen <tomi.valkeinen@ideasonboard.com>
Date: Fri, 29 Sep 2023 16:24:14 +0300
Subject: [PATCH 0773/1085] media: rp1: cfe: Add missing remaps

8-bit bayer formats are missing remap definitions. Add them.

Signed-off-by: Tomi Valkeinen <tomi.valkeinen@ideasonboard.com>
---
 drivers/media/platform/raspberrypi/rp1_cfe/cfe_fmts.h | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/media/platform/raspberrypi/rp1_cfe/cfe_fmts.h
+++ b/drivers/media/platform/raspberrypi/rp1_cfe/cfe_fmts.h
@@ -85,24 +85,28 @@ static const struct cfe_fmt formats[] =
 		.code = MEDIA_BUS_FMT_SBGGR8_1X8,
 		.depth = 8,
 		.csi_dt = 0x2a,
+		.remap = { V4L2_PIX_FMT_SBGGR16, V4L2_PIX_FMT_PISP_COMP1_BGGR },
 	},
 	{
 		.fourcc = V4L2_PIX_FMT_SGBRG8,
 		.code = MEDIA_BUS_FMT_SGBRG8_1X8,
 		.depth = 8,
 		.csi_dt = 0x2a,
+		.remap = { V4L2_PIX_FMT_SGBRG16, V4L2_PIX_FMT_PISP_COMP1_GBRG },
 	},
 	{
 		.fourcc = V4L2_PIX_FMT_SGRBG8,
 		.code = MEDIA_BUS_FMT_SGRBG8_1X8,
 		.depth = 8,
 		.csi_dt = 0x2a,
+		.remap = { V4L2_PIX_FMT_SGRBG16, V4L2_PIX_FMT_PISP_COMP1_GRBG },
 	},
 	{
 		.fourcc = V4L2_PIX_FMT_SRGGB8,
 		.code = MEDIA_BUS_FMT_SRGGB8_1X8,
 		.depth = 8,
 		.csi_dt = 0x2a,
+		.remap = { V4L2_PIX_FMT_SRGGB16, V4L2_PIX_FMT_PISP_COMP1_RGGB },
 	},
 	{
 		.fourcc = V4L2_PIX_FMT_SBGGR10P,
