From 6484f966af53447deefcd4b805c201d8624981cb Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Mon, 29 May 2023 23:32:44 +0200
Subject: [PATCH] ARM: dts: ixp4xx: Boot NSLU2 from harddrive

This enforces harddrive boot on the NSLU2. The flash is too small
to hold any rootfs these days.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 arch/arm/boot/dts/intel/ixp/intel-ixp42x-linksys-nslu2.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/intel/ixp/intel-ixp42x-linksys-nslu2.dts
+++ b/arch/arm/boot/dts/intel/ixp/intel-ixp42x-linksys-nslu2.dts
@@ -21,7 +21,7 @@
 	};
 
 	chosen {
-		bootargs = "console=ttyS0,115200n8 root=/dev/mtdblock2 rw rootfstype=squashfs,jffs2 rootwait";
+		bootargs = "console=ttyS0,115200n8 root=/dev/sda1 rw rootwait";
 		stdout-path = "uart0:115200n8";
 	};
 
