From a6ae420439dc47a58550a6e61e596e9dd1562caf Mon Sep 17 00:00:00 2001
From: Rick Wertenbroek <rick.wertenbroek@gmail.com>
Date: Wed, 6 Nov 2024 14:03:13 +0100
Subject: [PATCH] arm64: dts: rockchip: enable USB3 on NanoPC-T6

Enable the USB3 port on FriendlyELEC NanoPC-T6.

Signed-off-by: Rick Wertenbroek <rick.wertenbroek@gmail.com>
Link: https://lore.kernel.org/r/20241106130314.1289055-1-rick.wertenbroek@gmail.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 .../boot/dts/rockchip/rk3588-nanopc-t6.dtsi   | 36 +++++++++++++++++++
 1 file changed, 36 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
@@ -160,6 +160,20 @@
 		vin-supply = <&vcc5v0_sys>;
 	};
 
+	vbus5v0_usb: vbus5v0-usb-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio4 RK_PB0 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&usb5v_pwren>;
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-name = "vbus5v0_usb";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
 	vcc3v3_pcie2x1l0: vcc3v3-pcie2x1l0-regulator {
 		compatible = "regulator-fixed";
 		enable-active-high;
@@ -577,6 +591,10 @@
 			rockchip,pins = <1 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
 		};
 
+		usb5v_pwren: usb5v_pwren {
+			rockchip,pins = <4 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
 		usbc0_int: usbc0-int {
 			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_up>;
 		};
@@ -976,6 +994,14 @@
 	status = "okay";
 };
 
+&u2phy1 {
+	status = "okay";
+};
+
+&u2phy1_otg {
+	status = "okay";
+};
+
 &u2phy2_host {
 	status = "okay";
 };
@@ -1015,6 +1041,11 @@
 	};
 };
 
+&usbdp_phy1 {
+	phy-supply = <&vbus5v0_usb>;
+	status = "okay";
+};
+
 &usb_host0_ehci {
 	status = "okay";
 };
@@ -1035,6 +1066,11 @@
 	};
 };
 
+&usb_host1_xhci {
+	dr_mode = "host";
+	status = "okay";
+};
+
 &usb_host1_ehci {
 	status = "okay";
 };
