#
# Copyright (C) 2018 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
adtran,bsap1800-v2|\
adtran,bsap1840)
	ucidef_add_gpio_switch "wifi1_ext_a" "5GHz External Antenna A" "534" "1"
	ucidef_add_gpio_switch "wifi1_int_a" "5GHz Internal Antenna A" "535"
	ucidef_add_gpio_switch "wifi1_ext_b" "5GHz External Antenna B" "536" "1"
	ucidef_add_gpio_switch "wifi1_int_b" "5GHz Internal Antenna B" "537"
	ucidef_add_gpio_switch "wifi1_ext_c" "5GHz External Antenna C" "538" "1"
	ucidef_add_gpio_switch "wifi1_int_c" "5GHz Internal Antenna C" "539"
	ucidef_add_gpio_switch "wifi0_ext_a" "2.4GHz External Antenna A" "527" "1"
	ucidef_add_gpio_switch "wifi0_int_a" "2.4GHz Internal Antenna A" "528"
	ucidef_add_gpio_switch "wifi0_ext_b" "2.4GHz External Antenna B" "529" "1"
	ucidef_add_gpio_switch "wifi0_int_b" "2.4GHz Internal Antenna B" "530"
	ucidef_add_gpio_switch "wifi0_ext_c" "2.4GHz External Antenna C" "531" "1"
	ucidef_add_gpio_switch "wifi0_int_c" "2.4GHz Internal Antenna C" "532"
	;;
asus,pl-ac56)
	ucidef_add_gpio_switch "plc_enable" "PLC enable" "526" "1"
	;;
comfast,cf-e5|\
telco,t1)
	ucidef_add_gpio_switch "lte_power" "LTE Power" "526" "1"
	ucidef_add_gpio_switch "lte_wakeup" "LTE Wakeup" "523" "1"
	ucidef_add_gpio_switch "lte_poweroff" "LTE Poweroff" "513" "1"
	ucidef_add_gpio_switch "lte_reset" "LTE Reset" "524" "1"
	;;
devolo,dlan-pro-1200plus-ac)
	ucidef_add_gpio_switch "plc_enable" "PLC enable" "525" "0"
	;;
devolo,magic-2-wifi)
	ucidef_add_gpio_switch "plc_pairing" "PLC pairing" "523" "1"
	ucidef_add_gpio_switch "plc_enable" "PLC enable" "525" "1"
	;;
dlink,dir-825-c1|\
dlink,dir-835-a1)
	ucidef_add_gpio_switch "wan_led_auto" "WAN LED Auto" "532" "0"
	;;
librerouter,librerouter-v1)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "513" "0"
	;;
teltonika,rut230-v1)
	ucidef_add_gpio_switch "DOUT" "DOUT" "524" "0"
	ucidef_add_gpio_switch "modem_pwr" "Modem power" "531" "1"
	ucidef_add_gpio_switch "modem_rst" "Modem reset" "530" "0"
	;;
teltonika,rut955)
	ucidef_add_gpio_switch "sim_sel" "SIM select" "542" "1"
	ucidef_add_gpio_switch "DOUT1" "DOUT1 (OC)" "543" "0"
	ucidef_add_gpio_switch "DOUT2" "DOUT2 (Relay)" "544" "0"
	ucidef_add_gpio_switch "modem_vbus" "Modem enable" "545" "1"
	ucidef_add_gpio_switch "modem_rst" "Modem reset" "546" "0"
	ucidef_add_gpio_switch "DOUT3" "DOUT3" "547" "0"
	;;
teltonika,rut955-h7v3c0)
	ucidef_add_gpio_switch "sim_sel" "SIM select" "542" "1"
	ucidef_add_gpio_switch "DOUT1" "DOUT1 (OC)" "543" "0"
	ucidef_add_gpio_switch "DOUT2" "DOUT2 (Relay)" "544" "0"
	ucidef_add_gpio_switch "modem_vbus" "Modem enable" "547" "1"
	ucidef_add_gpio_switch "modem_rst" "Modem reset" "548" "0"
	;;

tplink,archer-c25-v1)
	ucidef_add_gpio_switch "led_control" "LED control" "533" "0"
	ucidef_add_gpio_switch "led_reset" "LED reset" "531" "1"
	;;
tplink,cpe210-v1|\
tplink,cpe220-v2|\
tplink,cpe220-v3|\
tplink,cpe510-v1|\
tplink,wbs210-v1|\
tplink,wbs210-v2|\
tplink,wbs510-v1|\
tplink,wbs510-v2)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "532"
	;;
ubnt,aircube-ac|\
ubnt,nanobeam-ac-gen2|\
ubnt,nanostation-ac)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "515"
	;;
ubnt,aircube-isp)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "523"
	;;
ubnt,nanostation-m)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "520"
	;;
ubnt,nanostation-m-xw)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "514"
	;;
ubnt,uk-ultra)
	ucidef_add_gpio_switch "ant0_internal" "ANT0 Internal" "517" "1"
	ucidef_add_gpio_switch "ant1_internal" "ANT1 Internal" "518" "1"
	;;
zbtlink,zbt-wd323)
	ucidef_add_gpio_switch "io0" "IO#0" "512"
	ucidef_add_gpio_switch "io1" "IO#1" "513"
	ucidef_add_gpio_switch "io2" "IO#2" "514"
	ucidef_add_gpio_switch "io14" "IO#14" "526"
	;;
esac

board_config_flush

exit 0
