From e87e452cdc7109748217171c422cb53336939be4 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Thu, 25 Mar 2021 18:34:50 +0000
Subject: [PATCH] staging/bcm2835-camera: Add support for H264 levels 4.1 and
 4.2

Whilst the hardware can't achieve the limits of level 4.2 under
all situations, it can exceed level 4.0.

Allow selection of levels 4.1 and 4.2.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 .../vc04_services/bcm2835-camera/controls.c   | 19 +++++++++++++++++--
 1 file changed, 17 insertions(+), 2 deletions(-)

--- a/drivers/staging/vc04_services/bcm2835-camera/controls.c
+++ b/drivers/staging/vc04_services/bcm2835-camera/controls.c
@@ -704,6 +704,8 @@ static int ctrl_set_video_encode_profile
 		case V4L2_MPEG_VIDEO_H264_LEVEL_3_1:
 		case V4L2_MPEG_VIDEO_H264_LEVEL_3_2:
 		case V4L2_MPEG_VIDEO_H264_LEVEL_4_0:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_4_1:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_4_2:
 			dev->capture.enc_level = ctrl->val;
 			break;
 		default:
@@ -769,6 +771,17 @@ static int ctrl_set_video_encode_profile
 		case V4L2_MPEG_VIDEO_H264_LEVEL_4_0:
 			param.level = MMAL_VIDEO_LEVEL_H264_4;
 			break;
+		/*
+		 * Note that the hardware spec is level 4.0. Achieving levels
+		 * above that depend on exactly the resolution and frame rate
+		 * being requested.
+		 */
+		case V4L2_MPEG_VIDEO_H264_LEVEL_4_1:
+			param.level = MMAL_VIDEO_LEVEL_H264_41;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_4_2:
+			param.level = MMAL_VIDEO_LEVEL_H264_42;
+			break;
 		default:
 			/* Should never get here */
 			break;
@@ -1218,8 +1231,10 @@ static const struct bcm2835_mmal_v4l2_ct
 			 BIT(V4L2_MPEG_VIDEO_H264_LEVEL_3_0) |
 			 BIT(V4L2_MPEG_VIDEO_H264_LEVEL_3_1) |
 			 BIT(V4L2_MPEG_VIDEO_H264_LEVEL_3_2) |
-			 BIT(V4L2_MPEG_VIDEO_H264_LEVEL_4_0)),
-		.max = V4L2_MPEG_VIDEO_H264_LEVEL_4_0,
+			 BIT(V4L2_MPEG_VIDEO_H264_LEVEL_4_0) |
+			 BIT(V4L2_MPEG_VIDEO_H264_LEVEL_4_1) |
+			 BIT(V4L2_MPEG_VIDEO_H264_LEVEL_4_2)),
+		.max = V4L2_MPEG_VIDEO_H264_LEVEL_4_2,
 		.def = V4L2_MPEG_VIDEO_H264_LEVEL_4_0,
 		.step = 1,
 		.imenu = NULL,
