// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"
#include "arxxxx_fortinet_loader.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "fortinet,fap-220-b", "qca,ar7161";
	model = "Fortinet FAP-220-B";

	chosen {
		bootargs = "console=ttyS0,9600";
	};

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &eth1;
	};

	keys {
		compatible = "gpio-keys";
		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power-green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		status-green {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		status-yellow {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_YELLOW>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			panic-indicator;
		};

		mode-green {
			label = "green:mode";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		mode-yellow {
			label = "yellow:mode";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		wlan2g-green {
			label = "green:wlan2g";
			gpios = <&ath9k0 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan2g-yellow {
			label = "yellow:wlan2g";
			gpios = <&ath9k0 3 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0assoc";
		};

		wlan5g-green {
			label = "green:wlan5g";
			gpios = <&ath9k1 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g-yellow {
			label = "yellow:wlan5g";
			gpios = <&ath9k1 3 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1assoc";
		};
	};

	virtual_flash {
		devices = <&fwconcat0 &fwconcat1 &fwconcat2>;
	};
};

&pcie0 {
	status = "okay";

	ath9k0: wifi@11,0 { /* 2.4 GHz */
		compatible = "pci168c,0029";
		reg = <0x8800 0 0 0 0>;
		ieee80211-freq-limit = <2402000 2482000>;
		nvmem-cells = <&macaddr_uboot_3ff80 9>, <&cal_art_1000>;
		nvmem-cell-names = "mac-address", "calibration";
		#gpio-cells = <2>;
		gpio-controller;
	};

	ath9k1: wifi@12,0 { /* 5 GHz */
		compatible = "pci168c,0029";
		reg = <0x9000 0 0 0 0>;
		ieee80211-freq-limit = <2402000 2482000 4900000 5990000>;
		nvmem-cells = <&macaddr_uboot_3ff80 2>, <&cal_art_5000>;
		nvmem-cell-names = "mac-address", "calibration";
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0x0>;
	};
};

&eth0 {
	status = "okay";
	compatible = "syscon", "simple-mfd";
};

&eth1 {
	status = "okay";
	nvmem-cells = <&macaddr_uboot_3ff80 0>;
	nvmem-cell-names = "mac-address";

	pll-data = <0x00110000 0x00001099 0x00991099>;
	phy-handle = <&phy0>;
	phy-mode = "rgmii";
};

&usb1 {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&art {
	nvmem-layout {
		compatible = "fixed-layout";
		#address-cells = <1>;
		#size-cells = <1>;

		cal_art_1000: calibration@1000 {
			reg = <0x1000 0xeb8>;
		};

		cal_art_5000: calibration@5000 {
			reg = <0x5000 0xeb8>;
		};
	};
};
