--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -83,6 +83,16 @@ config WS_AP3825I
 	  This board is a Concurrent Dual-Band wireless access point with a
 	  Freescale P1020 SoC.
 
+config FIREBOX_T1X
+	bool "Watchguard Firebox T10/T15"
+	select DEFAULT_UIMAGE
+	select ARCH_REQUIRE_GPIOLIB
+	select GPIO_MPC8XXX
+	select PPC_ZIMAGE_LA3000000
+	help
+	  This option enables support for the Watchguard Firebox T10/T15 board.
+	  This board is a VPN Gateway-Router with a Freescale P1010 SoC.
+
 config MPC8540_ADS
 	bool "Freescale MPC8540 ADS"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -27,6 +27,7 @@ obj-$(CONFIG_PPC_P2020)   += p2020.o $(o
 obj-$(CONFIG_TWR_P102x)   += twr_p102x.o
 obj-$(CONFIG_WS_AP3710I)  += ws-ap3710i.o
 obj-$(CONFIG_WS_AP3825I)  += ws-ap3825i.o
+obj-$(CONFIG_FIREBOX_T1X) += firebox_t1x.o
 obj-$(CONFIG_CORENET_GENERIC)   += corenet_generic.o
 obj-$(CONFIG_FB_FSL_DIU)	+= t1042rdb_diu.o
 obj-$(CONFIG_RED_15W_REV1)	+= red15w_rev1.o
