#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "yuncore,cpe200", "mediatek,mt7628an-soc";
	model = "Yuncore CPE200";

	aliases {
		label-mac = &ethernet;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 38 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		mode {
			label = "mode";
			linux,input-type = <EV_SW>;
			linux,code = <BTN_0>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		lan {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 43 GPIO_ACTIVE_LOW>;
		};

		wan {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 39 GPIO_ACTIVE_LOW>;
		};
	};

	watchdog {
		compatible = "linux,wdt-gpio";
		gpios = <&gpio 37 GPIO_ACTIVE_HIGH>;
		hw_algo = "toggle";
		hw_margin_ms = <20000>;
		always-running;
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_factory_4: macaddr@4 {
						reg = <0x4 0x6>;
					};

					eeprom_factory_8000: eeprom@8000 {
						reg = <0x8000 0x600>;
					};

					macaddr_factory_8004: macaddr@8004 {
						reg = <0x8004 0x6>;
					};
				};
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&ethernet {
	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";
};

&esw {
	mediatek,portmap = <0x2f>;
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <5000000 6000000>;
		nvmem-cells = <&eeprom_factory_8000>, <&macaddr_factory_8004>;
		nvmem-cell-names = "eeprom", "mac-address";

		led {
			led-sources = <0>;
			led-active-low;
		};
	};
};

&state_default {
	gpio {
		groups = "pwm0", "i2c", "refclk", "wdt", "i2s", "spi cs1",
			 "spis", "gpio", "p0led_an", "p1led_an", "p2led_an",
			 "p3led_an", "p4led_an", "wled_kn", "p0led_kn",
			 "p1led_kn", "p2led_kn", "p3led_kn", "p4led_kn", "wled_an";
		function = "gpio";
	};
};
