From ce792f7abd4294ebba76f76d9d7aa90c7970de8e Mon Sep 17 00:00:00 2001
From: Samuel Holland <samuel@sholland.org>
Date: Thu, 4 Aug 2022 23:35:09 -0500
Subject: [PATCH 78/90] riscv: Add Allwinner D1 devicetrees

Signed-off-by: Samuel Holland <samuel@sholland.org>
---
 arch/riscv/dts/Makefile                       |   9 +
 .../riscv/dts/sun20i-d1-clockworkpi-v3.14.dts | 242 +++++
 .../dts/sun20i-d1-common-regulators.dtsi      |  51 +
 arch/riscv/dts/sun20i-d1-devterm-v3.14.dts    |  37 +
 .../dts/sun20i-d1-dongshan-nezha-stu.dts      | 114 +++
 .../dts/sun20i-d1-lichee-rv-86-panel-480p.dts |  29 +
 .../dts/sun20i-d1-lichee-rv-86-panel-720p.dts |  10 +
 .../dts/sun20i-d1-lichee-rv-86-panel.dtsi     |  92 ++
 arch/riscv/dts/sun20i-d1-lichee-rv-dock.dts   |  74 ++
 arch/riscv/dts/sun20i-d1-lichee-rv.dts        |  84 ++
 arch/riscv/dts/sun20i-d1-mangopi-mq-pro.dts   | 128 +++
 arch/riscv/dts/sun20i-d1-nezha.dts            | 171 ++++
 arch/riscv/dts/sun20i-d1.dtsi                 | 900 ++++++++++++++++++
 arch/riscv/dts/sunxi-u-boot.dtsi              |  68 ++
 include/dt-bindings/clock/sun20i-d1-r-ccu.h   |  19 +
 include/dt-bindings/reset/sun20i-d1-r-ccu.h   |  16 +
 16 files changed, 2044 insertions(+)
 create mode 100644 arch/riscv/dts/sun20i-d1-clockworkpi-v3.14.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-common-regulators.dtsi
 create mode 100644 arch/riscv/dts/sun20i-d1-devterm-v3.14.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-dongshan-nezha-stu.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-lichee-rv-86-panel-480p.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-lichee-rv-86-panel-720p.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-lichee-rv-86-panel.dtsi
 create mode 100644 arch/riscv/dts/sun20i-d1-lichee-rv-dock.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-lichee-rv.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-mangopi-mq-pro.dts
 create mode 100644 arch/riscv/dts/sun20i-d1-nezha.dts
 create mode 100644 arch/riscv/dts/sun20i-d1.dtsi
 create mode 100644 arch/riscv/dts/sunxi-u-boot.dtsi
 create mode 100644 include/dt-bindings/clock/sun20i-d1-r-ccu.h
 create mode 100644 include/dt-bindings/reset/sun20i-d1-r-ccu.h

--- a/arch/riscv/dts/Makefile
+++ b/arch/riscv/dts/Makefile
@@ -7,6 +7,15 @@ dtb-$(CONFIG_TARGET_OPENPITON_RISCV64) +
 dtb-$(CONFIG_TARGET_SIFIVE_UNLEASHED) += hifive-unleashed-a00.dtb
 dtb-$(CONFIG_TARGET_SIFIVE_UNMATCHED) += hifive-unmatched-a00.dtb
 dtb-$(CONFIG_TARGET_SIPEED_MAIX) += k210-maix-bit.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-clockworkpi-v3.14.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-devterm-v3.14.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-dongshan-nezha-stu.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-lichee-rv-86-panel-480p.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-lichee-rv-86-panel-720p.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-lichee-rv-dock.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-lichee-rv.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-mangopi-mq-pro.dtb
+dtb-$(CONFIG_TARGET_SUN20I_D1) += sun20i-d1-nezha.dtb
 
 include $(srctree)/scripts/Makefile.dts
 
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-clockworkpi-v3.14.dts
@@ -0,0 +1,242 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+/dts-v1/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+#include "sun20i-d1.dtsi"
+#include "sun20i-d1-common-regulators.dtsi"
+
+/ {
+	model = "ClockworkPi v3.14 (R-01)";
+	compatible = "clockwork,r-01-clockworkpi-v3.14", "allwinner,sun20i-d1";
+
+	aliases {
+		ethernet0 = &ap6256;
+		mmc0 = &mmc0;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	/*
+	 * This regulator is PWM-controlled, but the PWM controller is not
+	 * yet supported, so fix the regulator to its default voltage.
+	 */
+	reg_vdd_cpu: vdd-cpu {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd-cpu";
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+		vin-supply = <&reg_vcc>;
+	};
+
+	wifi_pwrseq: wifi-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&pio 6 11 GPIO_ACTIVE_LOW>; /* PG11/GPIO3 */
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpu>;
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&i2c0 {
+	pinctrl-0 = <&i2c0_pb10_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	axp221: pmic@34 {
+		compatible = "x-powers,axp228", "x-powers,axp221";
+		reg = <0x34>;
+		interrupt-parent = <&pio>;
+		interrupts = <4 9 IRQ_TYPE_LEVEL_LOW>; /* PE9/GPIO2 */
+		interrupt-controller;
+		#interrupt-cells = <1>;
+
+		ac_power_supply: ac-power {
+			compatible = "x-powers,axp221-ac-power-supply";
+		};
+
+		axp_adc: adc {
+			compatible = "x-powers,axp221-adc";
+			#io-channel-cells = <1>;
+		};
+
+		battery_power_supply: battery-power {
+			compatible = "x-powers,axp221-battery-power-supply";
+		};
+
+		regulators {
+			x-powers,dcdc-freq = <3000>;
+
+			reg_dcdc1: dcdc1 {
+				regulator-name = "sys-3v3";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_dcdc3: dcdc3 {
+				regulator-name = "sys-1v8";
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+			};
+
+			reg_aldo1: aldo1 {
+				regulator-name = "aud-3v3";
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_aldo2: aldo2 {
+				regulator-name = "disp-3v3";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_aldo3: aldo3 {
+				regulator-name = "vdd-wifi";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+			};
+
+			/* DLDO1 and ELDO1-3 are connected in parallel. */
+			reg_dldo1: dldo1 {
+				regulator-name = "vbat-wifi-a";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			/* DLDO2-DLDO4 are connected in parallel. */
+			reg_dldo2: dldo2 {
+				regulator-name = "vcc-3v3-ext-a";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_dldo3: dldo3 {
+				regulator-name = "vcc-3v3-ext-b";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_dldo4: dldo4 {
+				regulator-name = "vcc-3v3-ext-c";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_eldo1: eldo1 {
+				regulator-name = "vbat-wifi-b";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_eldo2: eldo2 {
+				regulator-name = "vbat-wifi-c";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+
+			reg_eldo3: eldo3 {
+				regulator-name = "vbat-wifi-d";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+			};
+		};
+
+		usb_power_supply: usb-power {
+			compatible = "x-powers,axp221-usb-power-supply";
+			status = "disabled";
+		};
+	};
+};
+
+&mmc0 {
+	broken-cd;
+	bus-width = <4>;
+	disable-wp;
+	vmmc-supply = <&reg_dcdc1>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&mmc1 {
+	bus-width = <4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	non-removable;
+	vmmc-supply = <&reg_dldo1>;
+	vqmmc-supply = <&reg_aldo3>;
+	pinctrl-0 = <&mmc1_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	ap6256: wifi@1 {
+		compatible = "brcm,bcm43456-fmac", "brcm,bcm4329-fmac";
+		reg = <1>;
+		interrupt-parent = <&pio>;
+		interrupts = <6 10 IRQ_TYPE_LEVEL_LOW>; /* PG10/GPIO4 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&pio {
+	vcc-pg-supply = <&reg_ldoa>;
+};
+
+&uart0 {
+	pinctrl-0 = <&uart0_pb8_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&uart1 {
+	uart-has-rtscts;
+	pinctrl-0 = <&uart1_pg6_pins>, <&uart1_pg8_rts_cts_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	bluetooth {
+		compatible = "brcm,bcm4345c5";
+		interrupt-parent = <&pio>;
+		interrupts = <6 17 IRQ_TYPE_LEVEL_HIGH>; /* PG17/GPIO6 */
+		device-wakeup-gpios = <&pio 6 16 GPIO_ACTIVE_HIGH>; /* PG16/GPIO7 */
+		shutdown-gpios = <&pio 6 18 GPIO_ACTIVE_HIGH>; /* PG18/GPIO5 */
+		max-speed = <1500000>;
+		vbat-supply = <&reg_dldo1>;
+		vddio-supply = <&reg_aldo3>;
+	};
+};
+
+&usb_otg {
+	dr_mode = "peripheral";
+	status = "okay";
+};
+
+&usbphy {
+	usb0_vbus_power-supply = <&ac_power_supply>;
+	status = "okay";
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-common-regulators.dtsi
@@ -0,0 +1,51 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2021-2022 Samuel Holland <samuel@sholland.org>
+
+/ {
+	reg_vcc: vcc {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+	};
+
+	reg_vcc_3v3: vcc-3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&reg_vcc>;
+	};
+};
+
+&lradc {
+	vref-supply = <&reg_aldo>;
+};
+
+&pio {
+	vcc-pb-supply = <&reg_vcc_3v3>;
+	vcc-pc-supply = <&reg_vcc_3v3>;
+	vcc-pd-supply = <&reg_vcc_3v3>;
+	vcc-pe-supply = <&reg_vcc_3v3>;
+	vcc-pf-supply = <&reg_vcc_3v3>;
+	vcc-pg-supply = <&reg_vcc_3v3>;
+};
+
+&reg_aldo {
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	vdd33-supply = <&reg_vcc_3v3>;
+};
+
+&reg_hpldo {
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	hpldoin-supply = <&reg_vcc_3v3>;
+};
+
+&reg_ldoa {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	ldo-in-supply = <&reg_vcc_3v3>;
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-devterm-v3.14.dts
@@ -0,0 +1,37 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+/dts-v1/;
+
+#include "sun20i-d1-clockworkpi-v3.14.dts"
+
+/ {
+	model = "Clockwork DevTerm (R-01)";
+	compatible = "clockwork,r-01-devterm-v3.14",
+		     "clockwork,r-01-clockworkpi-v3.14",
+		     "allwinner,sun20i-d1";
+
+	fan {
+		compatible = "gpio-fan";
+		gpios = <&pio 3 10 GPIO_ACTIVE_HIGH>; /* PD10/GPIO41 */
+		gpio-fan,speed-map = <0    0>,
+				     <6000 1>;
+		#cooling-cells = <2>;
+	};
+
+	i2c-gpio-0 {
+		compatible = "i2c-gpio";
+		sda-gpios = <&pio 3 14 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>; /* PD14/GPIO44 */
+		scl-gpios = <&pio 3 15 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>; /* PD15/GPIO45 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		adc@54 {
+			compatible = "ti,adc101c";
+			reg = <0x54>;
+			interrupt-parent = <&pio>;
+			interrupts = <4 12 IRQ_TYPE_LEVEL_LOW>; /* PE12/GPIO35 */
+			vref-supply = <&reg_dldo2>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-dongshan-nezha-stu.dts
@@ -0,0 +1,114 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+/dts-v1/;
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/leds/common.h>
+
+#include "sun20i-d1.dtsi"
+#include "sun20i-d1-common-regulators.dtsi"
+
+/ {
+	model = "Dongshan Nezha STU";
+	compatible = "100ask,dongshan-nezha-stu", "allwinner,sun20i-d1";
+
+	aliases {
+		ethernet0 = &emac;
+		mmc0 = &mmc0;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led-0 {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_STATUS;
+			gpios = <&pio 2 1 GPIO_ACTIVE_HIGH>; /* PC1 */
+		};
+	};
+
+	reg_usbvbus: usbvbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usbvbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		gpio = <&pio 3 19 GPIO_ACTIVE_HIGH>; /* PD19 */
+		enable-active-high;
+		vin-supply = <&reg_vcc>;
+	};
+
+	/*
+	 * This regulator is PWM-controlled, but the PWM controller is not
+	 * yet supported, so fix the regulator to its default voltage.
+	 */
+	reg_vdd_cpu: vdd-cpu {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd-cpu";
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+		vin-supply = <&reg_vcc>;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpu>;
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&emac {
+	pinctrl-0 = <&rgmii_pe_pins>;
+	pinctrl-names = "default";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii-id";
+	phy-supply = <&reg_vcc_3v3>;
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
+&mmc0 {
+	broken-cd;
+	bus-width = <4>;
+	disable-wp;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-0 = <&uart0_pb8_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "otg";
+	status = "okay";
+};
+
+&usbphy {
+	usb0_id_det-gpios = <&pio 3 21 GPIO_ACTIVE_HIGH>; /* PD21 */
+	usb0_vbus_det-gpios = <&pio 3 20 GPIO_ACTIVE_HIGH>; /* PD20 */
+	usb0_vbus-supply = <&reg_usbvbus>;
+	status = "okay";
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-lichee-rv-86-panel-480p.dts
@@ -0,0 +1,29 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+#include "sun20i-d1-lichee-rv-86-panel.dtsi"
+
+/ {
+	model = "Sipeed Lichee RV 86 Panel (480p)";
+	compatible = "sipeed,lichee-rv-86-panel-480p", "sipeed,lichee-rv",
+		     "allwinner,sun20i-d1";
+};
+
+&i2c2 {
+	pinctrl-0 = <&i2c2_pb0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	touchscreen@48 {
+		compatible = "focaltech,ft6236";
+		reg = <0x48>;
+		interrupt-parent = <&pio>;
+		interrupts = <6 14 IRQ_TYPE_LEVEL_LOW>; /* PG14 */
+		iovcc-supply = <&reg_vcc_3v3>;
+		reset-gpios = <&pio 6 15 GPIO_ACTIVE_LOW>; /* PG15 */
+		touchscreen-size-x = <480>;
+		touchscreen-size-y = <480>;
+		vcc-supply = <&reg_vcc_3v3>;
+		wakeup-source;
+	};
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-lichee-rv-86-panel-720p.dts
@@ -0,0 +1,10 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+#include "sun20i-d1-lichee-rv-86-panel.dtsi"
+
+/ {
+	model = "Sipeed Lichee RV 86 Panel (720p)";
+	compatible = "sipeed,lichee-rv-86-panel-720p", "sipeed,lichee-rv",
+		     "allwinner,sun20i-d1";
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-lichee-rv-86-panel.dtsi
@@ -0,0 +1,92 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+#include "sun20i-d1-lichee-rv.dts"
+
+/ {
+	aliases {
+		ethernet0 = &emac;
+		ethernet1 = &xr829;
+	};
+
+	/* PC1 is repurposed as BT_WAKE_AP */
+	/delete-node/ leds;
+
+	wifi_pwrseq: wifi-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&ccu CLK_FANOUT1>;
+		clock-names = "ext_clock";
+		reset-gpios = <&pio 6 12 GPIO_ACTIVE_LOW>; /* PG12 */
+		assigned-clocks = <&ccu CLK_FANOUT1>;
+		assigned-clock-rates = <32768>;
+		pinctrl-0 = <&clk_pg11_pin>;
+		pinctrl-names = "default";
+	};
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&emac {
+	pinctrl-0 = <&rmii_pe_pins>;
+	pinctrl-names = "default";
+	phy-handle = <&ext_rmii_phy>;
+	phy-mode = "rmii";
+	phy-supply = <&reg_vcc_3v3>;
+	status = "okay";
+};
+
+&mdio {
+	ext_rmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+		reset-gpios = <&pio 4 16 GPIO_ACTIVE_LOW>; /* PE16 */
+	};
+};
+
+&mmc1 {
+	bus-width = <4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	non-removable;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc1_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	xr829: wifi@1 {
+		reg = <1>;
+	};
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&pio {
+	clk_pg11_pin: clk-pg11-pin {
+		pins = "PG11";
+		function = "clk";
+	};
+};
+
+&uart1 {
+	uart-has-rtscts;
+	pinctrl-0 = <&uart1_pg6_pins>, <&uart1_pg8_rts_cts_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	/* XR829 bluetooth is connected here */
+};
+
+&usb_otg {
+	status = "disabled";
+};
+
+&usbphy {
+	/* PD20 and PD21 are repurposed for the LCD panel */
+	/delete-property/ usb0_id_det-gpios;
+	/delete-property/ usb0_vbus_det-gpios;
+	usb1_vbus-supply = <&reg_vcc>;
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-lichee-rv-dock.dts
@@ -0,0 +1,74 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Jisheng Zhang <jszhang@kernel.org>
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+#include <dt-bindings/input/input.h>
+
+#include "sun20i-d1-lichee-rv.dts"
+
+/ {
+	model = "Sipeed Lichee RV Dock";
+	compatible = "sipeed,lichee-rv-dock", "sipeed,lichee-rv",
+		     "allwinner,sun20i-d1";
+
+	aliases {
+		ethernet1 = &rtl8723ds;
+	};
+
+	wifi_pwrseq: wifi-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&pio 6 12 GPIO_ACTIVE_LOW>; /* PG12 */
+	};
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&lradc {
+	status = "okay";
+
+	button-220 {
+		label = "OK";
+		linux,code = <KEY_OK>;
+		channel = <0>;
+		voltage = <220000>;
+	};
+};
+
+&mmc1 {
+	bus-width = <4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	non-removable;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc1_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	rtl8723ds: wifi@1 {
+		reg = <1>;
+	};
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&uart1 {
+	uart-has-rtscts;
+	pinctrl-0 = <&uart1_pg6_pins>, <&uart1_pg8_rts_cts_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	bluetooth {
+		compatible = "realtek,rtl8723ds-bt";
+		device-wake-gpios = <&pio 6 15 GPIO_ACTIVE_HIGH>; /* PG16 */
+		enable-gpios = <&pio 6 18 GPIO_ACTIVE_HIGH>; /* PG18 */
+		host-wake-gpios = <&pio 6 17 GPIO_ACTIVE_HIGH>; /* PG17 */
+	};
+};
+
+&usbphy {
+	usb1_vbus-supply = <&reg_vcc>;
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-lichee-rv.dts
@@ -0,0 +1,84 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Jisheng Zhang <jszhang@kernel.org>
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+/dts-v1/;
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/leds/common.h>
+
+#include "sun20i-d1.dtsi"
+#include "sun20i-d1-common-regulators.dtsi"
+
+/ {
+	model = "Sipeed Lichee RV";
+	compatible = "sipeed,lichee-rv", "allwinner,sun20i-d1";
+
+	aliases {
+		mmc0 = &mmc0;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led-0 {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_STATUS;
+			gpios = <&pio 2 1 GPIO_ACTIVE_HIGH>; /* PC1 */
+		};
+	};
+
+	reg_vdd_cpu: vdd-cpu {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd-cpu";
+		regulator-min-microvolt = <900000>;
+		regulator-max-microvolt = <900000>;
+		vin-supply = <&reg_vcc>;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpu>;
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&mmc0 {
+	broken-cd;
+	bus-width = <4>;
+	disable-wp;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-0 = <&uart0_pb8_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "otg";
+	status = "okay";
+};
+
+&usbphy {
+	usb0_id_det-gpios = <&pio 3 21 GPIO_ACTIVE_HIGH>; /* PD21 */
+	usb0_vbus_det-gpios = <&pio 3 20 GPIO_ACTIVE_HIGH>; /* PD20 */
+	usb0_vbus-supply = <&reg_vcc>;
+	status = "okay";
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-mangopi-mq-pro.dts
@@ -0,0 +1,128 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2022 Samuel Holland <samuel@sholland.org>
+
+/dts-v1/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+#include "sun20i-d1.dtsi"
+#include "sun20i-d1-common-regulators.dtsi"
+
+/ {
+	model = "MangoPi MQ Pro";
+	compatible = "widora,mangopi-mq-pro", "allwinner,sun20i-d1";
+
+	aliases {
+		ethernet0 = &rtl8723ds;
+		mmc0 = &mmc0;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	reg_avdd2v8: avdd2v8 {
+		compatible = "regulator-fixed";
+		regulator-name = "avdd2v8";
+		regulator-min-microvolt = <2800000>;
+		regulator-max-microvolt = <2800000>;
+		vin-supply = <&reg_vcc_3v3>;
+	};
+
+	reg_dvdd: dvdd {
+		compatible = "regulator-fixed";
+		regulator-name = "dvdd";
+		regulator-min-microvolt = <1200000>;
+		regulator-max-microvolt = <1200000>;
+		vin-supply = <&reg_vcc_3v3>;
+	};
+
+	reg_vdd_cpu: vdd-cpu {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd-cpu";
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+		vin-supply = <&reg_vcc>;
+	};
+
+	wifi_pwrseq: wifi-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&pio 6 17 GPIO_ACTIVE_LOW>; /* PG17 */
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpu>;
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&mmc0 {
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>; /* PF6 */
+	disable-wp;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&mmc1 {
+	bus-width = <4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	non-removable;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc1_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	rtl8723ds: wifi@1 {
+		reg = <1>;
+		interrupt-parent = <&pio>;
+		interrupts = <6 10 IRQ_TYPE_LEVEL_LOW>; /* PG10 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&pio {
+	vcc-pe-supply = <&reg_avdd2v8>;
+};
+
+&uart0 {
+	pinctrl-0 = <&uart0_pb8_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&uart1 {
+	uart-has-rtscts;
+	pinctrl-0 = <&uart1_pg6_pins>, <&uart1_pg8_rts_cts_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	bluetooth {
+		compatible = "realtek,rtl8723ds-bt";
+		device-wake-gpios = <&pio 6 18 GPIO_ACTIVE_HIGH>; /* PG18 */
+		enable-gpios = <&pio 6 15 GPIO_ACTIVE_HIGH>; /* PG15 */
+		host-wake-gpios = <&pio 6 14 GPIO_ACTIVE_HIGH>; /* PG14 */
+	};
+};
+
+&usb_otg {
+	dr_mode = "peripheral";
+	status = "okay";
+};
+
+&usbphy {
+	usb0_vbus-supply = <&reg_vcc>;
+	status = "okay";
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1-nezha.dts
@@ -0,0 +1,171 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2021-2022 Samuel Holland <samuel@sholland.org>
+
+/dts-v1/;
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+
+#include "sun20i-d1.dtsi"
+#include "sun20i-d1-common-regulators.dtsi"
+
+/ {
+	model = "Allwinner D1 Nezha";
+	compatible = "allwinner,d1-nezha", "allwinner,sun20i-d1";
+
+	aliases {
+		ethernet0 = &emac;
+		ethernet1 = &xr829;
+		mmc0 = &mmc0;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	reg_usbvbus: usbvbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usbvbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		gpio = <&pio 3 19 GPIO_ACTIVE_HIGH>; /* PD19 */
+		enable-active-high;
+		vin-supply = <&reg_vcc>;
+	};
+
+	/*
+	 * This regulator is PWM-controlled, but the PWM controller is not
+	 * yet supported, so fix the regulator to its default voltage.
+	 */
+	reg_vdd_cpu: vdd-cpu {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd-cpu";
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+		vin-supply = <&reg_vcc>;
+	};
+
+	wifi_pwrseq: wifi-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&pio 6 12 GPIO_ACTIVE_LOW>; /* PG12 */
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpu>;
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&emac {
+	pinctrl-0 = <&rgmii_pe_pins>;
+	pinctrl-names = "default";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii-id";
+	phy-supply = <&reg_vcc_3v3>;
+	status = "okay";
+};
+
+&i2c2 {
+	pinctrl-0 = <&i2c2_pb0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	pcf8574a: gpio@38 {
+		compatible = "nxp,pcf8574a";
+		reg = <0x38>;
+		interrupt-parent = <&pio>;
+		interrupts = <1 2 IRQ_TYPE_LEVEL_LOW>; /* PB2 */
+		interrupt-controller;
+		gpio-controller;
+		#gpio-cells = <2>;
+		#interrupt-cells = <2>;
+	};
+};
+
+&lradc {
+	status = "okay";
+
+	button-160 {
+		label = "OK";
+		linux,code = <KEY_OK>;
+		channel = <0>;
+		voltage = <160000>;
+	};
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
+&mmc0 {
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>; /* PF6 */
+	disable-wp;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc0_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&mmc1 {
+	bus-width = <4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	non-removable;
+	vmmc-supply = <&reg_vcc_3v3>;
+	vqmmc-supply = <&reg_vcc_3v3>;
+	pinctrl-0 = <&mmc1_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	xr829: wifi@1 {
+		reg = <1>;
+	};
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-0 = <&uart0_pb8_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+};
+
+&uart1 {
+	uart-has-rtscts;
+	pinctrl-0 = <&uart1_pg6_pins>, <&uart1_pg8_rts_cts_pins>;
+	pinctrl-names = "default";
+	status = "okay";
+
+	/* XR829 bluetooth is connected here */
+};
+
+&usb_otg {
+	dr_mode = "otg";
+	status = "okay";
+};
+
+&usbphy {
+	usb0_id_det-gpios = <&pio 3 21 GPIO_ACTIVE_HIGH>; /* PD21 */
+	usb0_vbus_det-gpios = <&pio 3 20 GPIO_ACTIVE_HIGH>; /* PD20 */
+	usb0_vbus-supply = <&reg_usbvbus>;
+	usb1_vbus-supply = <&reg_vcc>;
+	status = "okay";
+};
--- /dev/null
+++ b/arch/riscv/dts/sun20i-d1.dtsi
@@ -0,0 +1,900 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+// Copyright (C) 2021-2022 Samuel Holland <samuel@sholland.org>
+
+#include <dt-bindings/clock/sun6i-rtc.h>
+#include <dt-bindings/clock/sun8i-de2.h>
+#include <dt-bindings/clock/sun8i-tcon-top.h>
+#include <dt-bindings/clock/sun20i-d1-ccu.h>
+#include <dt-bindings/clock/sun20i-d1-r-ccu.h>
+#include <dt-bindings/interrupt-controller/irq.h>
+#include <dt-bindings/reset/sun8i-de2.h>
+#include <dt-bindings/reset/sun20i-d1-ccu.h>
+#include <dt-bindings/reset/sun20i-d1-r-ccu.h>
+#include <dt-bindings/thermal/thermal.h>
+
+/ {
+	#address-cells = <1>;
+	#size-cells = <1>;
+
+	cpus {
+		timebase-frequency = <24000000>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		cpu0: cpu@0 {
+			compatible = "thead,c906", "riscv";
+			device_type = "cpu";
+			reg = <0>;
+			clocks = <&ccu CLK_RISCV>;
+			clock-frequency = <24000000>;
+			d-cache-block-size = <64>;
+			d-cache-sets = <256>;
+			d-cache-size = <32768>;
+			i-cache-block-size = <64>;
+			i-cache-sets = <128>;
+			i-cache-size = <32768>;
+			mmu-type = "riscv,sv39";
+			riscv,isa = "rv64imafdc";
+			#cooling-cells = <2>;
+
+			cpu0_intc: interrupt-controller {
+				compatible = "riscv,cpu-intc";
+				interrupt-controller;
+				#address-cells = <0>;
+				#interrupt-cells = <1>;
+			};
+		};
+	};
+
+	de: display-engine {
+		compatible = "allwinner,sun20i-d1-display-engine";
+		allwinner,pipelines = <&mixer0>, <&mixer1>;
+		status = "disabled";
+	};
+
+	osc24M: osc24M-clk {
+		compatible = "fixed-clock";
+		clock-frequency = <24000000>;
+		clock-output-names = "osc24M";
+		#clock-cells = <0>;
+	};
+
+	soc {
+		compatible = "simple-bus";
+		ranges;
+		interrupt-parent = <&plic>;
+		dma-noncoherent;
+		#address-cells = <1>;
+		#size-cells = <1>;
+
+		dsp_wdt: watchdog@1700400 {
+			compatible = "allwinner,sun20i-d1-wdt";
+			reg = <0x1700400 0x20>;
+			interrupts = <138 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&osc24M>, <&rtc CLK_OSC32K>;
+			clock-names = "hosc", "losc";
+			status = "reserved";
+		};
+
+		pio: pinctrl@2000000 {
+			compatible = "allwinner,sun20i-d1-pinctrl";
+			reg = <0x2000000 0x800>;
+			interrupts = <85 IRQ_TYPE_LEVEL_HIGH>,
+				     <87 IRQ_TYPE_LEVEL_HIGH>,
+				     <89 IRQ_TYPE_LEVEL_HIGH>,
+				     <91 IRQ_TYPE_LEVEL_HIGH>,
+				     <93 IRQ_TYPE_LEVEL_HIGH>,
+				     <95 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_APB0>,
+				 <&osc24M>,
+				 <&rtc CLK_OSC32K>;
+			clock-names = "apb", "hosc", "losc";
+			gpio-controller;
+			interrupt-controller;
+			#gpio-cells = <3>;
+			#interrupt-cells = <3>;
+
+			/omit-if-no-ref/
+			i2c0_pb10_pins: i2c0-pb10-pins {
+				pins = "PB10", "PB11";
+				function = "i2c0";
+			};
+
+			/omit-if-no-ref/
+			i2c2_pb0_pins: i2c2-pb0-pins {
+				pins = "PB0", "PB1";
+				function = "i2c2";
+			};
+
+			/omit-if-no-ref/
+			lcd_rgb666_pins: lcd-rgb666-pins {
+				pins = "PD0", "PD1", "PD2", "PD3", "PD4", "PD5",
+				       "PD6", "PD7", "PD8", "PD9", "PD10", "PD11",
+				       "PD12", "PD13", "PD14", "PD15", "PD16", "PD17",
+				       "PD18", "PD19", "PD20", "PD21";
+				function = "lcd0";
+			};
+
+			/omit-if-no-ref/
+			mmc0_pins: mmc0-pins {
+				pins = "PF0", "PF1", "PF2", "PF3", "PF4", "PF5";
+				function = "mmc0";
+			};
+
+			/omit-if-no-ref/
+			mmc1_pins: mmc1-pins {
+				pins = "PG0", "PG1", "PG2", "PG3", "PG4", "PG5";
+				function = "mmc1";
+			};
+
+			/omit-if-no-ref/
+			mmc2_pins: mmc2-pins {
+				pins = "PC2", "PC3", "PC4", "PC5", "PC6", "PC7";
+				function = "mmc2";
+			};
+
+			/omit-if-no-ref/
+			rgmii_pe_pins: rgmii-pe-pins {
+				pins = "PE0", "PE1", "PE2", "PE3", "PE4",
+				       "PE5", "PE6", "PE7", "PE8", "PE9",
+				       "PE11", "PE12", "PE13", "PE14", "PE15";
+				function = "emac";
+			};
+
+			/omit-if-no-ref/
+			rmii_pe_pins: rmii-pe-pins {
+				pins = "PE0", "PE1", "PE2", "PE3", "PE4",
+				       "PE5", "PE6", "PE7", "PE8", "PE9";
+				function = "emac";
+			};
+
+			/omit-if-no-ref/
+			uart0_pb8_pins: uart0-pb8-pins {
+				pins = "PB8", "PB9";
+				function = "uart0";
+			};
+
+			/omit-if-no-ref/
+			uart1_pg6_pins: uart1-pg6-pins {
+				pins = "PG6", "PG7";
+				function = "uart1";
+			};
+
+			/omit-if-no-ref/
+			uart1_pg8_rts_cts_pins: uart1-pg8-rts-cts-pins {
+				pins = "PG8", "PG9";
+				function = "uart1";
+			};
+		};
+
+		ccu: clock-controller@2001000 {
+			compatible = "allwinner,sun20i-d1-ccu";
+			reg = <0x2001000 0x1000>;
+			clocks = <&osc24M>,
+				 <&rtc CLK_OSC32K>,
+				 <&rtc CLK_IOSC>;
+			clock-names = "hosc", "losc", "iosc";
+			#clock-cells = <1>;
+			#reset-cells = <1>;
+		};
+
+		lradc: keys@2009800 {
+			compatible = "allwinner,sun20i-d1-lradc",
+				     "allwinner,sun50i-r329-lradc";
+			reg = <0x2009800 0x400>;
+			interrupts = <77 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_LRADC>;
+			resets = <&ccu RST_BUS_LRADC>;
+			status = "disabled";
+		};
+
+		codec: audio-codec@2030000 {
+			compatible = "simple-mfd", "syscon";
+			reg = <0x2030000 0x1000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			regulators@2030348 {
+				compatible = "allwinner,sun20i-d1-analog-ldos";
+				reg = <0x2030348 0x4>;
+				nvmem-cells = <&bg_trim>;
+				nvmem-cell-names = "bg_trim";
+
+				reg_aldo: aldo {
+				};
+
+				reg_hpldo: hpldo {
+				};
+			};
+		};
+
+		i2s0: i2s@2032000 {
+			compatible = "allwinner,sun20i-d1-i2s",
+				     "allwinner,sun50i-r329-i2s";
+			reg = <0x2032000 0x1000>;
+			interrupts = <42 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2S0>,
+				 <&ccu CLK_I2S0>;
+			clock-names = "apb", "mod";
+			resets = <&ccu RST_BUS_I2S0>;
+			dmas = <&dma 3>, <&dma 3>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+			#sound-dai-cells = <0>;
+		};
+
+		i2s1: i2s@2033000 {
+			compatible = "allwinner,sun20i-d1-i2s",
+				     "allwinner,sun50i-r329-i2s";
+			reg = <0x2033000 0x1000>;
+			interrupts = <43 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2S1>,
+				 <&ccu CLK_I2S1>;
+			clock-names = "apb", "mod";
+			resets = <&ccu RST_BUS_I2S1>;
+			dmas = <&dma 4>, <&dma 4>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+			#sound-dai-cells = <0>;
+		};
+
+		i2s2: i2s@2034000 {
+			compatible = "allwinner,sun20i-d1-i2s",
+				     "allwinner,sun50i-r329-i2s";
+			reg = <0x2034000 0x1000>;
+			interrupts = <44 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2S2>,
+				 <&ccu CLK_I2S2>;
+			clock-names = "apb", "mod";
+			resets = <&ccu RST_BUS_I2S2>;
+			dmas = <&dma 5>, <&dma 5>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+			#sound-dai-cells = <0>;
+		};
+
+		timer: timer@2050000 {
+			compatible = "allwinner,sun20i-d1-timer",
+				     "allwinner,sun8i-a23-timer";
+			reg = <0x2050000 0xa0>;
+			interrupts = <75 IRQ_TYPE_LEVEL_HIGH>,
+				     <76 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&osc24M>;
+		};
+
+		wdt: watchdog@20500a0 {
+			compatible = "allwinner,sun20i-d1-wdt-reset",
+				     "allwinner,sun20i-d1-wdt";
+			reg = <0x20500a0 0x20>;
+			interrupts = <79 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&osc24M>, <&rtc CLK_OSC32K>;
+			clock-names = "hosc", "losc";
+			status = "reserved";
+		};
+
+		uart0: serial@2500000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x2500000 0x400>;
+			reg-io-width = <4>;
+			reg-shift = <2>;
+			interrupts = <18 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_UART0>;
+			resets = <&ccu RST_BUS_UART0>;
+			dmas = <&dma 14>, <&dma 14>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
+		uart1: serial@2500400 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x2500400 0x400>;
+			reg-io-width = <4>;
+			reg-shift = <2>;
+			interrupts = <19 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_UART1>;
+			resets = <&ccu RST_BUS_UART1>;
+			dmas = <&dma 15>, <&dma 15>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
+		uart2: serial@2500800 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x2500800 0x400>;
+			reg-io-width = <4>;
+			reg-shift = <2>;
+			interrupts = <20 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_UART2>;
+			resets = <&ccu RST_BUS_UART2>;
+			dmas = <&dma 16>, <&dma 16>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
+		uart3: serial@2500c00 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x2500c00 0x400>;
+			reg-io-width = <4>;
+			reg-shift = <2>;
+			interrupts = <21 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_UART3>;
+			resets = <&ccu RST_BUS_UART3>;
+			dmas = <&dma 17>, <&dma 17>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
+		uart4: serial@2501000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x2501000 0x400>;
+			reg-io-width = <4>;
+			reg-shift = <2>;
+			interrupts = <22 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_UART4>;
+			resets = <&ccu RST_BUS_UART4>;
+			dmas = <&dma 18>, <&dma 18>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
+		uart5: serial@2501400 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x2501400 0x400>;
+			reg-io-width = <4>;
+			reg-shift = <2>;
+			interrupts = <23 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_UART5>;
+			resets = <&ccu RST_BUS_UART5>;
+			dmas = <&dma 19>, <&dma 19>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
+		i2c0: i2c@2502000 {
+			compatible = "allwinner,sun20i-d1-i2c",
+				     "allwinner,sun8i-v536-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x2502000 0x400>;
+			interrupts = <25 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C0>;
+			resets = <&ccu RST_BUS_I2C0>;
+			dmas = <&dma 43>, <&dma 43>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c1: i2c@2502400 {
+			compatible = "allwinner,sun20i-d1-i2c",
+				     "allwinner,sun8i-v536-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x2502400 0x400>;
+			interrupts = <26 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C1>;
+			resets = <&ccu RST_BUS_I2C1>;
+			dmas = <&dma 44>, <&dma 44>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c2: i2c@2502800 {
+			compatible = "allwinner,sun20i-d1-i2c",
+				     "allwinner,sun8i-v536-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x2502800 0x400>;
+			interrupts = <27 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C2>;
+			resets = <&ccu RST_BUS_I2C2>;
+			dmas = <&dma 45>, <&dma 45>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c3: i2c@2502c00 {
+			compatible = "allwinner,sun20i-d1-i2c",
+				     "allwinner,sun8i-v536-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x2502c00 0x400>;
+			interrupts = <28 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C3>;
+			resets = <&ccu RST_BUS_I2C3>;
+			dmas = <&dma 46>, <&dma 46>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		syscon: syscon@3000000 {
+			compatible = "allwinner,sun20i-d1-system-control";
+			reg = <0x3000000 0x1000>;
+			ranges;
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			regulators@3000150 {
+				compatible = "allwinner,sun20i-d1-system-ldos";
+				reg = <0x3000150 0x4>;
+
+				reg_ldoa: ldoa {
+				};
+
+				reg_ldob: ldob {
+				};
+			};
+		};
+
+		dma: dma-controller@3002000 {
+			compatible = "allwinner,sun20i-d1-dma";
+			reg = <0x3002000 0x1000>;
+			interrupts = <66 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_DMA>, <&ccu CLK_MBUS_DMA>;
+			clock-names = "bus", "mbus";
+			resets = <&ccu RST_BUS_DMA>;
+			dma-channels = <16>;
+			dma-requests = <48>;
+			#dma-cells = <1>;
+		};
+
+		sid: efuse@3006000 {
+			compatible = "allwinner,sun20i-d1-sid";
+			reg = <0x3006000 0x1000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			ths_calib: ths-calib@14 {
+				reg = <0x14 0x4>;
+			};
+
+			bg_trim: bg-trim@28 {
+				reg = <0x28 0x4>;
+				bits = <16 8>;
+			};
+		};
+
+		mbus: dram-controller@3102000 {
+			compatible = "allwinner,sun20i-d1-mbus";
+			reg = <0x3102000 0x1000>,
+			      <0x3103000 0x1000>;
+			reg-names = "mbus", "dram";
+			interrupts = <59 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_MBUS>,
+				 <&ccu CLK_DRAM>,
+				 <&ccu CLK_BUS_DRAM>;
+			clock-names = "mbus", "dram", "bus";
+			dma-ranges = <0 0x40000000 0x80000000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			#interconnect-cells = <1>;
+		};
+
+		mmc0: mmc@4020000 {
+			compatible = "allwinner,sun20i-d1-mmc";
+			reg = <0x4020000 0x1000>;
+			interrupts = <56 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_MMC0>, <&ccu CLK_MMC0>;
+			clock-names = "ahb", "mmc";
+			resets = <&ccu RST_BUS_MMC0>;
+			reset-names = "ahb";
+			cap-sd-highspeed;
+			max-frequency = <150000000>;
+			no-mmc;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		mmc1: mmc@4021000 {
+			compatible = "allwinner,sun20i-d1-mmc";
+			reg = <0x4021000 0x1000>;
+			interrupts = <57 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_MMC1>, <&ccu CLK_MMC1>;
+			clock-names = "ahb", "mmc";
+			resets = <&ccu RST_BUS_MMC1>;
+			reset-names = "ahb";
+			cap-sd-highspeed;
+			max-frequency = <150000000>;
+			no-mmc;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		mmc2: mmc@4022000 {
+			compatible = "allwinner,sun20i-d1-emmc",
+				     "allwinner,sun50i-a100-emmc";
+			reg = <0x4022000 0x1000>;
+			interrupts = <58 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_MMC2>, <&ccu CLK_MMC2>;
+			clock-names = "ahb", "mmc";
+			resets = <&ccu RST_BUS_MMC2>;
+			reset-names = "ahb";
+			cap-mmc-highspeed;
+			max-frequency = <150000000>;
+			mmc-ddr-1_8v;
+			mmc-ddr-3_3v;
+			no-sd;
+			no-sdio;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		usb_otg: usb@4100000 {
+			compatible = "allwinner,sun20i-d1-musb",
+				     "allwinner,sun8i-a33-musb";
+			reg = <0x4100000 0x400>;
+			interrupts = <45 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "mc";
+			clocks = <&ccu CLK_BUS_OTG>;
+			resets = <&ccu RST_BUS_OTG>;
+			extcon = <&usbphy 0>;
+			phys = <&usbphy 0>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		usbphy: phy@4100400 {
+			compatible = "allwinner,sun20i-d1-usb-phy";
+			reg = <0x4100400 0x100>,
+			      <0x4101800 0x100>,
+			      <0x4200800 0x100>;
+			reg-names = "phy_ctrl",
+				    "pmu0",
+				    "pmu1";
+			clocks = <&osc24M>,
+				 <&osc24M>;
+			clock-names = "usb0_phy",
+				      "usb1_phy";
+			resets = <&ccu RST_USB_PHY0>,
+				 <&ccu RST_USB_PHY1>;
+			reset-names = "usb0_reset",
+				      "usb1_reset";
+			status = "disabled";
+			#phy-cells = <1>;
+		};
+
+		ehci0: usb@4101000 {
+			compatible = "allwinner,sun20i-d1-ehci",
+				     "generic-ehci";
+			reg = <0x4101000 0x100>;
+			interrupts = <46 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI0>,
+				 <&ccu CLK_BUS_EHCI0>,
+				 <&ccu CLK_USB_OHCI0>;
+			resets = <&ccu RST_BUS_OHCI0>,
+				 <&ccu RST_BUS_EHCI0>;
+			phys = <&usbphy 0>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ohci0: usb@4101400 {
+			compatible = "allwinner,sun20i-d1-ohci",
+				     "generic-ohci";
+			reg = <0x4101400 0x100>;
+			interrupts = <47 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI0>,
+				 <&ccu CLK_USB_OHCI0>;
+			resets = <&ccu RST_BUS_OHCI0>;
+			phys = <&usbphy 0>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ehci1: usb@4200000 {
+			compatible = "allwinner,sun20i-d1-ehci",
+				     "generic-ehci";
+			reg = <0x4200000 0x100>;
+			interrupts = <49 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI1>,
+				 <&ccu CLK_BUS_EHCI1>,
+				 <&ccu CLK_USB_OHCI1>;
+			resets = <&ccu RST_BUS_OHCI1>,
+				 <&ccu RST_BUS_EHCI1>;
+			phys = <&usbphy 1>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ohci1: usb@4200400 {
+			compatible = "allwinner,sun20i-d1-ohci",
+				     "generic-ohci";
+			reg = <0x4200400 0x100>;
+			interrupts = <50 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI1>,
+				 <&ccu CLK_USB_OHCI1>;
+			resets = <&ccu RST_BUS_OHCI1>;
+			phys = <&usbphy 1>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		emac: ethernet@4500000 {
+			compatible = "allwinner,sun20i-d1-emac",
+				     "allwinner,sun50i-a64-emac";
+			reg = <0x4500000 0x10000>;
+			interrupts = <62 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			clocks = <&ccu CLK_BUS_EMAC>;
+			clock-names = "stmmaceth";
+			resets = <&ccu RST_BUS_EMAC>;
+			reset-names = "stmmaceth";
+			syscon = <&syscon>;
+			status = "disabled";
+
+			mdio: mdio {
+				compatible = "snps,dwmac-mdio";
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+
+		display_clocks: clock-controller@5000000 {
+			compatible = "allwinner,sun20i-d1-de2-clk",
+				     "allwinner,sun50i-h5-de2-clk";
+			reg = <0x5000000 0x10000>;
+			clocks = <&ccu CLK_BUS_DE>, <&ccu CLK_DE>;
+			clock-names = "bus", "mod";
+			resets = <&ccu RST_BUS_DE>;
+			#clock-cells = <1>;
+			#reset-cells = <1>;
+		};
+
+		mixer0: mixer@5100000 {
+			compatible = "allwinner,sun20i-d1-de2-mixer-0";
+			reg = <0x5100000 0x100000>;
+			clocks = <&display_clocks CLK_BUS_MIXER0>,
+				 <&display_clocks CLK_MIXER0>;
+			clock-names = "bus", "mod";
+			resets = <&display_clocks RST_MIXER0>;
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				mixer0_out: port@1 {
+					reg = <1>;
+
+					mixer0_out_tcon_top_mixer0: endpoint {
+						remote-endpoint = <&tcon_top_mixer0_in_mixer0>;
+					};
+				};
+			};
+		};
+
+		mixer1: mixer@5200000 {
+			compatible = "allwinner,sun20i-d1-de2-mixer-1";
+			reg = <0x5200000 0x100000>;
+			clocks = <&display_clocks CLK_BUS_MIXER1>,
+				 <&display_clocks CLK_MIXER1>;
+			clock-names = "bus", "mod";
+			resets = <&display_clocks RST_MIXER1>;
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				mixer1_out: port@1 {
+					reg = <1>;
+
+					mixer1_out_tcon_top_mixer1: endpoint {
+						remote-endpoint = <&tcon_top_mixer1_in_mixer1>;
+					};
+				};
+			};
+		};
+
+		tcon_top: tcon-top@5460000 {
+			compatible = "allwinner,sun20i-d1-tcon-top";
+			reg = <0x5460000 0x1000>;
+			clocks = <&ccu CLK_BUS_DPSS_TOP>,
+				 <&ccu CLK_TCON_TV>,
+				 <&ccu CLK_TVE>,
+				 <&ccu CLK_TCON_LCD0>;
+			clock-names = "bus", "tcon-tv0", "tve0", "dsi";
+			clock-output-names = "tcon-top-tv0", "tcon-top-dsi";
+			resets = <&ccu RST_BUS_DPSS_TOP>;
+			#clock-cells = <1>;
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon_top_mixer0_in: port@0 {
+					reg = <0>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					tcon_top_mixer0_in_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&mixer0_out_tcon_top_mixer0>;
+					};
+				};
+
+				tcon_top_mixer0_out: port@1 {
+					reg = <1>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					tcon_top_mixer0_out_tcon_lcd0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon_lcd0_in_tcon_top_mixer0>;
+					};
+
+					tcon_top_mixer0_out_tcon_tv0: endpoint@2 {
+						reg = <2>;
+						remote-endpoint = <&tcon_tv0_in_tcon_top_mixer0>;
+					};
+				};
+
+				tcon_top_mixer1_in: port@2 {
+					reg = <2>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					tcon_top_mixer1_in_mixer1: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&mixer1_out_tcon_top_mixer1>;
+					};
+				};
+
+				tcon_top_mixer1_out: port@3 {
+					reg = <3>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					tcon_top_mixer1_out_tcon_lcd0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon_lcd0_in_tcon_top_mixer1>;
+					};
+
+					tcon_top_mixer1_out_tcon_tv0: endpoint@2 {
+						reg = <2>;
+						remote-endpoint = <&tcon_tv0_in_tcon_top_mixer1>;
+					};
+				};
+
+				tcon_top_hdmi_in: port@4 {
+					reg = <4>;
+
+					tcon_top_hdmi_in_tcon_tv0: endpoint {
+						remote-endpoint = <&tcon_tv0_out_tcon_top_hdmi>;
+					};
+				};
+
+				tcon_top_hdmi_out: port@5 {
+					reg = <5>;
+				};
+			};
+		};
+
+		tcon_lcd0: lcd-controller@5461000 {
+			compatible = "allwinner,sun20i-d1-tcon-lcd";
+			reg = <0x5461000 0x1000>;
+			interrupts = <106 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON_LCD0>,
+				 <&ccu CLK_TCON_LCD0>;
+			clock-names = "ahb", "tcon-ch0";
+			clock-output-names = "tcon-pixel-clock";
+			resets = <&ccu RST_BUS_TCON_LCD0>,
+				 <&ccu RST_BUS_LVDS0>;
+			reset-names = "lcd", "lvds";
+			#clock-cells = <0>;
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon_lcd0_in: port@0 {
+					reg = <0>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					tcon_lcd0_in_tcon_top_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon_top_mixer0_out_tcon_lcd0>;
+					};
+
+					tcon_lcd0_in_tcon_top_mixer1: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&tcon_top_mixer1_out_tcon_lcd0>;
+					};
+				};
+
+				tcon_lcd0_out: port@1 {
+					reg = <1>;
+				};
+			};
+		};
+
+		tcon_tv0: lcd-controller@5470000 {
+			compatible = "allwinner,sun20i-d1-tcon-tv";
+			reg = <0x5470000 0x1000>;
+			interrupts = <107 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON_TV>,
+				 <&tcon_top CLK_TCON_TOP_TV0>;
+			clock-names = "ahb", "tcon-ch1";
+			resets = <&ccu RST_BUS_TCON_TV>;
+			reset-names = "lcd";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon_tv0_in: port@0 {
+					reg = <0>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					tcon_tv0_in_tcon_top_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon_top_mixer0_out_tcon_tv0>;
+					};
+
+					tcon_tv0_in_tcon_top_mixer1: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&tcon_top_mixer1_out_tcon_tv0>;
+					};
+				};
+
+				tcon_tv0_out: port@1 {
+					reg = <1>;
+
+					tcon_tv0_out_tcon_top_hdmi: endpoint {
+						remote-endpoint = <&tcon_top_hdmi_in_tcon_tv0>;
+					};
+				};
+			};
+		};
+
+		riscv_wdt: watchdog@6011000 {
+			compatible = "allwinner,sun20i-d1-wdt";
+			reg = <0x6011000 0x20>;
+			interrupts = <147 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&osc24M>, <&rtc CLK_OSC32K>;
+			clock-names = "hosc", "losc";
+		};
+
+		r_ccu: clock-controller@7010000 {
+			compatible = "allwinner,sun20i-d1-r-ccu";
+			reg = <0x7010000 0x400>;
+			clocks = <&osc24M>,
+				 <&rtc CLK_OSC32K>,
+				 <&rtc CLK_IOSC>,
+				 <&ccu CLK_PLL_PERIPH0_DIV3>;
+			clock-names = "hosc", "losc", "iosc", "pll-periph";
+			#clock-cells = <1>;
+			#reset-cells = <1>;
+		};
+
+		rtc: rtc@7090000 {
+			compatible = "allwinner,sun20i-d1-rtc",
+				     "allwinner,sun50i-r329-rtc";
+			reg = <0x7090000 0x400>;
+			interrupts = <160 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&r_ccu CLK_BUS_R_RTC>,
+				 <&osc24M>,
+				 <&r_ccu CLK_R_AHB>;
+			clock-names = "bus", "hosc", "ahb";
+			#clock-cells = <1>;
+		};
+
+		plic: interrupt-controller@10000000 {
+			compatible = "allwinner,sun20i-d1-plic",
+				     "thead,c900-plic";
+			reg = <0x10000000 0x4000000>;
+			interrupts-extended = <&cpu0_intc 11>,
+					      <&cpu0_intc 9>;
+			interrupt-controller;
+			riscv,ndev = <176>;
+			#address-cells = <0>;
+			#interrupt-cells = <2>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/riscv/dts/sunxi-u-boot.dtsi
@@ -0,0 +1,68 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+
+#include "binman.dtsi"
+
+/ {
+	cpus {
+		u-boot,dm-spl;
+	};
+
+	soc {
+		u-boot,dm-spl;
+	};
+};
+
+&binman {
+	u-boot-sunxi-with-spl {
+		filename = "u-boot-sunxi-with-spl.bin";
+		pad-byte = <0xff>;
+
+		blob@0 {
+			filename = "spl/sunxi-spl.bin";
+		};
+
+		blob@1 {
+			filename = "u-boot.itb";
+		};
+	};
+};
+
+&ccu {
+	u-boot,dm-spl;
+};
+
+&cpu0 {
+	u-boot,dm-spl;
+};
+
+&mbus {
+	u-boot,dm-spl;
+};
+
+&mmc0 {
+	u-boot,dm-spl;
+};
+
+&mmc0_pins {
+	u-boot,dm-spl;
+};
+
+&osc24M {
+	u-boot,dm-spl;
+};
+
+&pio {
+	u-boot,dm-spl;
+};
+
+&rtc {
+	u-boot,dm-spl;
+};
+
+&uart0 {
+	u-boot,dm-spl;
+};
+
+&uart0_pb8_pins {
+	u-boot,dm-spl;
+};
--- /dev/null
+++ b/include/dt-bindings/clock/sun20i-d1-r-ccu.h
@@ -0,0 +1,19 @@
+/* SPDX-License-Identifier: (GPL-2.0+ or MIT) */
+/*
+ * Copyright (C) 2021 Samuel Holland <samuel@sholland.org>
+ */
+
+#ifndef _DT_BINDINGS_CLK_SUN20I_D1_R_CCU_H_
+#define _DT_BINDINGS_CLK_SUN20I_D1_R_CCU_H_
+
+#define CLK_R_AHB		0
+
+#define CLK_BUS_R_TIMER		2
+#define CLK_BUS_R_TWD		3
+#define CLK_BUS_R_PPU		4
+#define CLK_R_IR_RX		5
+#define CLK_BUS_R_IR_RX		6
+#define CLK_BUS_R_RTC		7
+#define CLK_BUS_R_CPUCFG	8
+
+#endif /* _DT_BINDINGS_CLK_SUN20I_D1_R_CCU_H_ */
--- /dev/null
+++ b/include/dt-bindings/reset/sun20i-d1-r-ccu.h
@@ -0,0 +1,16 @@
+/* SPDX-License-Identifier: (GPL-2.0+ or MIT) */
+/*
+ * Copyright (C) 2021 Samuel Holland <samuel@sholland.org>
+ */
+
+#ifndef _DT_BINDINGS_RST_SUN20I_D1_R_CCU_H_
+#define _DT_BINDINGS_RST_SUN20I_D1_R_CCU_H_
+
+#define RST_BUS_R_TIMER		0
+#define RST_BUS_R_TWD		1
+#define RST_BUS_R_PPU		2
+#define RST_BUS_R_IR_RX		3
+#define RST_BUS_R_RTC		4
+#define RST_BUS_R_CPUCFG	5
+
+#endif /* _DT_BINDINGS_RST_SUN20I_D1_R_CCU_H_ */
