// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "Huawei AP5030DN";
	compatible = "huawei,ap5030dn", "qca,qca9550", "qca,qca9558";

	chosen {
		bootargs = "console=ttyS0,9600n8";
	};

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_function_red;
		led-failsafe = &led_function_red;
		led-running = &led_function_green;
		led-upgrade = &led_function_red;
	};

	leds {
		compatible = "gpio-leds";

		led_function_green: led-status-red {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 18 GPIO_ACTIVE_HIGH>;
		};

		led_function_red: led-status-green {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
		};

	};

	keys {
		compatible = "gpio-keys";

		restart {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	watchdog {
		pinctrl-names = "default";
		pinctrl-0 = <&wdt_gpio15>;

		compatible = "linux,wdt-gpio";
		gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		hw_algo = "toggle";
		hw_margin_ms = <100>;
		always-running;
	};

	virtual_flash {
		compatible = "mtd-concat";
		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "firmware";
				reg = <0x0 0x1e00000>;
				compatible = "openwrt,uimage", "denx,uimage";
			};
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot-a";
				reg = <0x0 0x80000>;
				read-only;
			};

			// The BootupA/B partitions store the addresses
			// of the main and backup kernel in flash (which is the same here).
			// During sysupgrade, these addresses are set to the start of the
			// "firmware" partition.
			partition@80000 {
				label = "BootupA";
				reg = <0x80000 0x20000>;
			};

			partition@a0000 {
				label = "BootupB";
				reg = <0xa0000 0x20000>;
			};

			partition@c0000 {
				label = "u-boot-env";
				reg = <0xc0000 0x20000>;
				read-only;
			};

			partition@e0000 {
				label = "BoardData";
				reg = <0xe0000 0x20000>;
				read-only;
			};

			// In the vendor layout, there are the "SysImageA" (12 MiB)
			// and the "ConfigA" (3 MiB) partitions here.
			fwconcat0: partition@100000 {
				label = "fwconcat0";
				reg = <0x100000 0xF00000>;
			};

			partition@1000000 {
				label = "u-boot-b";
				reg = <0x1000000 0x80000>;
				read-only;
			};

			partition@1080000 {
				label = "ResultA";
				reg = <0x1080000 0x20000>;
				read-only;
			};

			partition@10a0000 {
				label = "ResultB";
				reg = <0x10a0000 0x20000>;
				read-only;
			};

			// In the vendor layout, there are the "SysImageB" (12 MiB)
			// and the "ConfigB" (3 MiB) partitions here.
			fwconcat1: partition@10c0000 {
				label = "fwconcat1";
				reg = <0x10c0000 0xF00000>;
			};

			art: partition@1fc0000 {
				label = "art";
				reg = <0x1fc0000 0x40000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_art_2005b: macaddr@2005b {
						compatible = "mac-base";
						reg = <0x2005b 0x6>;
						#nvmem-cell-cells = <1>;
					};

					cal_art_1000: cal@1000 {
						reg = <0x1000 0x440>;
					};

					cal_art_5000: cal@5000 {
						reg = <0x5000 0x844>;
					};
				};
			};
		};
	};
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_art_2005b 3>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&macaddr_art_2005b 2>, <&cal_art_5000>;
		nvmem-cell-names = "mac-address", "calibration";
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_2005b 0>;
	nvmem-cell-names = "mac-address";

	pll-data = <0xa6000000 0xa0000101 0xa0001313>;
	phy-handle = <&phy0>;

	gmac-config {
		device = <&gmac>;
		rxdv-delay = <3>;
		rxd-delay = <3>;
		txen-delay = <0>;
		txd-delay = <0>;
	};
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_art_2005b 1>;
	nvmem-cell-names = "mac-address";

	pll-data = <0x03000101 0x00000101 0x00001313>;
	phy-handle = <&phy1>;
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@18 {
		reg = <0x18>;
	};
};

&mdio1 {
	status = "okay";

	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&pinmux {
	wdt_gpio15: pinmux_wdt_gpio15 {
		pinctrl-single,bits = <0xc 0x0 0xFF000000>;
	};
};

&wdt {
	status = "disabled";
};
