// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6368.dtsi"

/ {
	model = "Observa VH4032N";
	compatible = "observa,vh4032n", "brcm,bcm6368";

	aliases {
		led-boot = &led_power_blue;
		led-failsafe = &led_power_red;
		led-running = &led_power_blue;
		led-upgrade = &led_power_blue;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		rfkill {
			label = "rfkill";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led-2 {
			label = "blue:dsl";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		led-5 {
			label = "red:dsl";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		led-11 {
			label = "blue:hspa";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		led-12 {
			label = "red:hspa";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		led_power_blue: led-22 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 22 GPIO_ACTIVE_HIGH>;
		};

		led_power_red: led-24 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 24 GPIO_ACTIVE_HIGH>;
			panic-indicator;
		};

		led-25 {
			label = "blue:voice";
			gpios = <&gpio 25 GPIO_ACTIVE_LOW>;
		};

		led-26 {
			label = "red:voice";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};
	};

	bcm43222-sprom {
		compatible = "brcm,ssb-sprom";

		pci-bus = <0>;
		pci-dev = <1>;

		nvmem-cells = <&macaddr_cfe_6a0 1>;
		nvmem-cell-names = "mac-address";

		brcm,sprom = "brcm/bcm43222-sprom.bin";
		brcm,sprom-fixups = <2   0x04d2>, <4   0x4350>,
				    <65  0x1300>, <68  0x0402>,
				    <70  0x0090>, <71  0x4c19>,
				    <72  0x2345>, <87  0x0315>,
				    <88  0x0315>, <96  0x2048>,
				    <97  0xfed7>, <98  0x15a6>,
				    <99  0xfaee>, <100 0x3e3a>,
				    <101 0x3a36>, <102 0xff7f>,
				    <103 0x11b9>, <104 0xfc53>,
				    <105 0xffe6>, <106 0xfdd2>,
				    <107 0xfe49>, <108 0xff6a>,
				    <109 0x136e>, <110 0xfbed>,
				    <111 0x0000>, <112 0x2048>,
				    <113 0xfee2>, <114 0x15e5>,
				    <115 0xfaed>, <116 0x3e3a>,
				    <117 0x3a36>, <118 0xffc8>,
				    <119 0x12b8>, <120 0xfca1>,
				    <121 0xff9b>, <122 0x122a>,
				    <123 0xfcc8>, <124 0xff95>,
				    <125 0x146b>, <126 0xfbba>,
				    <127 0x0000>, <161 0x0000>,
				    <162 0x0000>, <169 0x0000>,
				    <170 0x0000>, <171 0x0000>,
				    <172 0x0000>, <173 0x0000>,
				    <174 0x0000>, <175 0x0000>,
				    <176 0x0000>, <219 0x1108>;
	};
};

&ehci {
	status = "okay";
};

&ethernet {
	status = "okay";

	nvmem-cells = <&macaddr_cfe_6a0 0>;
	nvmem-cell-names = "mac-address";
};

&gpio {
	usb_hub_reset {
		gpio-hog;
		gpios = <27 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "usb-hub-reset-gpio";
	};
};

&ohci {
	status = "okay";
};

&pci {
	status = "okay";
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "CFE";
			reg = <0x0000000 0x0020000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_cfe_6a0: macaddr@6a0 {
					compatible = "mac-base";
					reg = <0x6a0 0x6>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		partition@20000 {
			compatible = "brcm,bcm963xx-imagetag";
			label = "firmware";
			reg = <0x0020000 0x1fc0000>;
		};

		partition@1fe0000 {
			label = "nvram";
			reg = <0x1fe0000 0x020000>;
		};
	};
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ephy0_led &pinctrl_ephy1_led
		     &pinctrl_ephy2_led &pinctrl_ephy3_led>;
};

&switch0 {
	ports {
		port@0 {
			reg = <0>;
			label = "lan4";

			phy-handle = <&phy1>;
			phy-mode = "mii";
		};

		port@1 {
			reg = <1>;
			label = "lan3";

			phy-handle = <&phy2>;
			phy-mode = "mii";
		};

		port@2 {
			reg = <2>;
			label = "lan2";

			phy-handle = <&phy3>;
			phy-mode = "mii";
		};

		port@3 {
			reg = <3>;
			label = "lan1";

			phy-handle = <&phy4>;
			phy-mode = "mii";
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};
