From d94b5221af537cb8aab412e2641ec5baa0d20524 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <mripard@kernel.org>
Date: Fri, 25 Oct 2024 18:15:40 +0100
Subject: [PATCH] drm/vc4: drv: Support BCM2712

The BCM2712 has an improved display pipeline, most notably with a
different HVS and only HDMI and writeback outputs.

Let's introduce it as a new VideoCore generation and compatible.

Signed-off-by: Maxime Ripard <mripard@kernel.org>
Link: https://patchwork.freedesktop.org/patch/msgid/20241025-drm-vc4-2712-support-v2-9-35efa83c8fc0@raspberrypi.com
Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/vc4/vc4_drv.c | 1 +
 drivers/gpu/drm/vc4/vc4_drv.h | 1 +
 2 files changed, 2 insertions(+)

--- a/drivers/gpu/drm/vc4/vc4_drv.c
+++ b/drivers/gpu/drm/vc4/vc4_drv.c
@@ -456,6 +456,7 @@ static void vc4_platform_drm_shutdown(st
 
 static const struct of_device_id vc4_of_match[] = {
 	{ .compatible = "brcm,bcm2711-vc5", .data = (void *)VC4_GEN_5 },
+	{ .compatible = "brcm,bcm2712-vc6", .data = (void *)VC4_GEN_6_C },
 	{ .compatible = "brcm,bcm2835-vc4", .data = (void *)VC4_GEN_4 },
 	{ .compatible = "brcm,cygnus-vc4", .data = (void *)VC4_GEN_4 },
 	{},
--- a/drivers/gpu/drm/vc4/vc4_drv.h
+++ b/drivers/gpu/drm/vc4/vc4_drv.h
@@ -84,6 +84,7 @@ struct vc4_perfmon {
 enum vc4_gen {
 	VC4_GEN_4,
 	VC4_GEN_5,
+	VC4_GEN_6_C,
 };
 
 struct vc4_dev {
