From 42d20a6a61b8fccbb57d80df1ccde7dd82d5bbd6 Mon Sep 17 00:00:00 2001
From: Chris Packham <chris.packham@alliedtelesis.co.nz>
Date: Wed, 16 Oct 2024 11:54:34 +1300
Subject: [PATCH] spi: spi-mem: Add Realtek SPI-NAND controller

Add a driver for the SPI-NAND controller on the RTL9300 family of
devices.

The controller supports
* Serial/Dual/Quad data with
* PIO and DMA data read/write operation
* Configurable flash access timing

There is a separate ECC controller on the RTL9300 which isn't currently
supported (instead we rely on the on-die ECC supported by most SPI-NAND
chips).

Signed-off-by: Chris Packham <chris.packham@alliedtelesis.co.nz>
Link: https://patch.msgid.link/20241015225434.3970360-4-chris.packham@alliedtelesis.co.nz
Signed-off-by: Mark Brown <broonie@kernel.org>
---
 MAINTAINERS                         |   6 +
 drivers/spi/Kconfig                 |  11 +
 drivers/spi/Makefile                |   1 +
 drivers/spi/spi-realtek-rtl-snand.c | 405 ++++++++++++++++++++++++++++
 4 files changed, 423 insertions(+)
 create mode 100644 drivers/spi/spi-realtek-rtl-snand.c

--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -19500,6 +19500,12 @@ S:	Maintained
 F:	Documentation/devicetree/bindings/net/dsa/realtek.yaml
 F:	drivers/net/dsa/realtek/*
 
+REALTEK SPI-NAND
+M:	Chris Packham <chris.packham@alliedtelesis.co.nz>
+S:	Maintained
+F:	Documentation/devicetree/bindings/spi/realtek,rtl9301-snand.yaml
+F:	drivers/spi/spi-realtek-rtl-snand.c
+
 REALTEK WIRELESS DRIVER (rtlwifi family)
 M:	Ping-Ke Shih <pkshih@realtek.com>
 L:	linux-wireless@vger.kernel.org
--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -843,6 +843,17 @@ config SPI_PXA2XX
 config SPI_PXA2XX_PCI
 	def_tristate SPI_PXA2XX && PCI && COMMON_CLK
 
+config SPI_REALTEK_SNAND
+	tristate "Realtek SPI-NAND Flash Controller"
+	depends on MACH_REALTEK_RTL || COMPILE_TEST
+	select REGMAP
+	help
+	  This enables support for the SPI-NAND Flash controller on
+	  Realtek SoCs.
+
+	  This driver does not support generic SPI. The implementation
+	  only supports the spi-mem interface.
+
 config SPI_ROCKCHIP
 	tristate "Rockchip SPI controller driver"
 	depends on ARCH_ROCKCHIP || COMPILE_TEST
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -120,6 +120,7 @@ obj-$(CONFIG_SPI_ROCKCHIP)		+= spi-rockc
 obj-$(CONFIG_SPI_ROCKCHIP_SFC)		+= spi-rockchip-sfc.o
 obj-$(CONFIG_SPI_RB4XX)			+= spi-rb4xx.o
 obj-$(CONFIG_MACH_REALTEK_RTL)		+= spi-realtek-rtl.o
+obj-$(CONFIG_SPI_REALTEK_SNAND)		+= spi-realtek-rtl-snand.o
 obj-$(CONFIG_SPI_RPCIF)			+= spi-rpc-if.o
 obj-$(CONFIG_SPI_RSPI)			+= spi-rspi.o
 obj-$(CONFIG_SPI_RZV2M_CSI)		+= spi-rzv2m-csi.o
--- /dev/null
+++ b/drivers/spi/spi-realtek-rtl-snand.c
@@ -0,0 +1,405 @@
+// SPDX-License-Identifier: GPL-2.0-only
+
+#include <linux/completion.h>
+#include <linux/dma-mapping.h>
+#include <linux/interrupt.h>
+#include <linux/mod_devicetable.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+#include <linux/spi/spi.h>
+#include <linux/spi/spi-mem.h>
+
+#define SNAFCFR 0x00
+#define   SNAFCFR_DMA_IE BIT(20)
+#define SNAFCCR 0x04
+#define SNAFWCMR 0x08
+#define SNAFRCMR 0x0c
+#define SNAFRDR 0x10
+#define SNAFWDR 0x14
+#define SNAFDTR 0x18
+#define SNAFDRSAR 0x1c
+#define SNAFDIR 0x20
+#define   SNAFDIR_DMA_IP BIT(0)
+#define SNAFDLR 0x24
+#define SNAFSR 0x40
+#define  SNAFSR_NFCOS BIT(3)
+#define  SNAFSR_NFDRS BIT(2)
+#define  SNAFSR_NFDWS BIT(1)
+
+#define CMR_LEN(len) ((len) - 1)
+#define CMR_WID(width) (((width) >> 1) << 28)
+
+struct rtl_snand {
+	struct device *dev;
+	struct regmap *regmap;
+	struct completion comp;
+};
+
+static irqreturn_t rtl_snand_irq(int irq, void *data)
+{
+	struct rtl_snand *snand = data;
+	u32 val = 0;
+
+	regmap_read(snand->regmap, SNAFSR, &val);
+	if (val & (SNAFSR_NFCOS | SNAFSR_NFDRS | SNAFSR_NFDWS))
+		return IRQ_NONE;
+
+	regmap_write(snand->regmap, SNAFDIR, SNAFDIR_DMA_IP);
+	complete(&snand->comp);
+
+	return IRQ_HANDLED;
+}
+
+static bool rtl_snand_supports_op(struct spi_mem *mem,
+				  const struct spi_mem_op *op)
+{
+	if (!spi_mem_default_supports_op(mem, op))
+		return false;
+	if (op->cmd.nbytes != 1 || op->cmd.buswidth != 1)
+		return false;
+	return true;
+}
+
+static void rtl_snand_set_cs(struct rtl_snand *snand, int cs, bool active)
+{
+	u32 val;
+
+	if (active)
+		val = ~(1 << (4 * cs));
+	else
+		val = ~0;
+
+	regmap_write(snand->regmap, SNAFCCR, val);
+}
+
+static int rtl_snand_wait_ready(struct rtl_snand *snand)
+{
+	u32 val;
+
+	return regmap_read_poll_timeout(snand->regmap, SNAFSR, val, !(val & SNAFSR_NFCOS),
+					0, 2 * USEC_PER_MSEC);
+}
+
+static int rtl_snand_xfer_head(struct rtl_snand *snand, int cs, const struct spi_mem_op *op)
+{
+	int ret;
+	u32 val, len = 0;
+
+	rtl_snand_set_cs(snand, cs, true);
+
+	val = op->cmd.opcode << 24;
+	len = 1;
+	if (op->addr.nbytes && op->addr.buswidth == 1) {
+		val |= op->addr.val << ((3 - op->addr.nbytes) * 8);
+		len += op->addr.nbytes;
+	}
+
+	ret = rtl_snand_wait_ready(snand);
+	if (ret)
+		return ret;
+
+	ret = regmap_write(snand->regmap, SNAFWCMR, CMR_LEN(len));
+	if (ret)
+		return ret;
+
+	ret = regmap_write(snand->regmap, SNAFWDR, val);
+	if (ret)
+		return ret;
+
+	ret = rtl_snand_wait_ready(snand);
+	if (ret)
+		return ret;
+
+	if (op->addr.buswidth > 1) {
+		val = op->addr.val << ((3 - op->addr.nbytes) * 8);
+		len = op->addr.nbytes;
+
+		ret = regmap_write(snand->regmap, SNAFWCMR,
+				   CMR_WID(op->addr.buswidth) | CMR_LEN(len));
+		if (ret)
+			return ret;
+
+		ret = regmap_write(snand->regmap, SNAFWDR, val);
+		if (ret)
+			return ret;
+
+		ret = rtl_snand_wait_ready(snand);
+		if (ret)
+			return ret;
+	}
+
+	if (op->dummy.nbytes) {
+		val = 0;
+
+		ret = regmap_write(snand->regmap, SNAFWCMR,
+				   CMR_WID(op->dummy.buswidth) | CMR_LEN(op->dummy.nbytes));
+		if (ret)
+			return ret;
+
+		ret = regmap_write(snand->regmap, SNAFWDR, val);
+		if (ret)
+			return ret;
+
+		ret = rtl_snand_wait_ready(snand);
+		if (ret)
+			return ret;
+	}
+
+	return 0;
+}
+
+static void rtl_snand_xfer_tail(struct rtl_snand *snand, int cs)
+{
+	rtl_snand_set_cs(snand, cs, false);
+}
+
+static int rtl_snand_xfer(struct rtl_snand *snand, int cs, const struct spi_mem_op *op)
+{
+	unsigned int pos, nbytes;
+	int ret;
+	u32 val, len = 0;
+
+	ret = rtl_snand_xfer_head(snand, cs, op);
+	if (ret)
+		goto out_deselect;
+
+	if (op->data.dir == SPI_MEM_DATA_IN) {
+		pos = 0;
+		len = op->data.nbytes;
+
+		while (pos < len) {
+			nbytes = len - pos;
+			if (nbytes > 4)
+				nbytes = 4;
+
+			ret = rtl_snand_wait_ready(snand);
+			if (ret)
+				goto out_deselect;
+
+			ret = regmap_write(snand->regmap, SNAFRCMR,
+					   CMR_WID(op->data.buswidth) | CMR_LEN(nbytes));
+			if (ret)
+				goto out_deselect;
+
+			ret = rtl_snand_wait_ready(snand);
+			if (ret)
+				goto out_deselect;
+
+			ret = regmap_read(snand->regmap, SNAFRDR, &val);
+			if (ret)
+				goto out_deselect;
+
+			memcpy(op->data.buf.in + pos, &val, nbytes);
+
+			pos += nbytes;
+		}
+	} else if (op->data.dir == SPI_MEM_DATA_OUT) {
+		pos = 0;
+		len = op->data.nbytes;
+
+		while (pos < len) {
+			nbytes = len - pos;
+			if (nbytes > 4)
+				nbytes = 4;
+
+			memcpy(&val, op->data.buf.out + pos, nbytes);
+
+			pos += nbytes;
+
+			ret = regmap_write(snand->regmap, SNAFWCMR, CMR_LEN(nbytes));
+			if (ret)
+				goto out_deselect;
+
+			ret = regmap_write(snand->regmap, SNAFWDR, val);
+			if (ret)
+				goto out_deselect;
+
+			ret = rtl_snand_wait_ready(snand);
+			if (ret)
+				goto out_deselect;
+		}
+	}
+
+out_deselect:
+	rtl_snand_xfer_tail(snand, cs);
+
+	if (ret)
+		dev_err(snand->dev, "transfer failed %d\n", ret);
+
+	return ret;
+}
+
+static int rtl_snand_dma_xfer(struct rtl_snand *snand, int cs, const struct spi_mem_op *op)
+{
+	int ret;
+	dma_addr_t buf_dma;
+	enum dma_data_direction dir;
+	u32 trig;
+
+	ret = rtl_snand_xfer_head(snand, cs, op);
+	if (ret)
+		goto out_deselect;
+
+	if (op->data.dir == SPI_MEM_DATA_IN) {
+		dir = DMA_FROM_DEVICE;
+		trig = 0;
+	} else if (op->data.dir == SPI_MEM_DATA_OUT) {
+		dir = DMA_TO_DEVICE;
+		trig = 1;
+	} else {
+		ret = -EOPNOTSUPP;
+		goto out_deselect;
+	}
+
+	buf_dma = dma_map_single(snand->dev, op->data.buf.in, op->data.nbytes, dir);
+	ret = dma_mapping_error(snand->dev, buf_dma);
+	if (ret)
+		goto out_deselect;
+
+	ret = regmap_write(snand->regmap, SNAFDIR, SNAFDIR_DMA_IP);
+	if (ret)
+		goto out_unmap;
+
+	ret = regmap_update_bits(snand->regmap, SNAFCFR, SNAFCFR_DMA_IE, SNAFCFR_DMA_IE);
+	if (ret)
+		goto out_unmap;
+
+	reinit_completion(&snand->comp);
+
+	ret = regmap_write(snand->regmap, SNAFDRSAR, buf_dma);
+	if (ret)
+		goto out_disable_int;
+
+	ret = regmap_write(snand->regmap, SNAFDLR,
+			   CMR_WID(op->data.buswidth) | (op->data.nbytes & 0xffff));
+	if (ret)
+		goto out_disable_int;
+
+	ret = regmap_write(snand->regmap, SNAFDTR, trig);
+	if (ret)
+		goto out_disable_int;
+
+	if (!wait_for_completion_timeout(&snand->comp, usecs_to_jiffies(20000)))
+		ret = -ETIMEDOUT;
+
+	if (ret)
+		goto out_disable_int;
+
+out_disable_int:
+	regmap_update_bits(snand->regmap, SNAFCFR, SNAFCFR_DMA_IE, 0);
+out_unmap:
+	dma_unmap_single(snand->dev, buf_dma, op->data.nbytes, dir);
+out_deselect:
+	rtl_snand_xfer_tail(snand, cs);
+
+	if (ret)
+		dev_err(snand->dev, "transfer failed %d\n", ret);
+
+	return ret;
+}
+
+static bool rtl_snand_dma_op(const struct spi_mem_op *op)
+{
+	switch (op->data.dir) {
+	case SPI_MEM_DATA_IN:
+	case SPI_MEM_DATA_OUT:
+		return op->data.nbytes > 32;
+	default:
+		return false;
+	}
+}
+
+static int rtl_snand_exec_op(struct spi_mem *mem, const struct spi_mem_op *op)
+{
+	struct rtl_snand *snand = spi_controller_get_devdata(mem->spi->controller);
+	int cs = spi_get_chipselect(mem->spi, 0);
+
+	dev_dbg(snand->dev, "cs %d op cmd %02x %d:%d, dummy %d:%d, addr %08llx@%d:%d, data %d:%d\n",
+		cs, op->cmd.opcode,
+		op->cmd.buswidth, op->cmd.nbytes, op->dummy.buswidth,
+		op->dummy.nbytes, op->addr.val, op->addr.buswidth,
+		op->addr.nbytes, op->data.buswidth, op->data.nbytes);
+
+	if (rtl_snand_dma_op(op))
+		return rtl_snand_dma_xfer(snand, cs, op);
+	else
+		return rtl_snand_xfer(snand, cs, op);
+}
+
+static const struct spi_controller_mem_ops rtl_snand_mem_ops = {
+	.supports_op = rtl_snand_supports_op,
+	.exec_op = rtl_snand_exec_op,
+};
+
+static const struct of_device_id rtl_snand_match[] = {
+	{ .compatible = "realtek,rtl9301-snand" },
+	{ .compatible = "realtek,rtl9302b-snand" },
+	{ .compatible = "realtek,rtl9302c-snand" },
+	{ .compatible = "realtek,rtl9303-snand" },
+	{},
+};
+MODULE_DEVICE_TABLE(of, rtl_snand_match);
+
+static int rtl_snand_probe(struct platform_device *pdev)
+{
+	struct rtl_snand *snand;
+	struct device *dev = &pdev->dev;
+	struct spi_controller *ctrl;
+	void __iomem *base;
+	const struct regmap_config rc = {
+		.reg_bits	= 32,
+		.val_bits	= 32,
+		.reg_stride	= 4,
+		.cache_type	= REGCACHE_NONE,
+	};
+	int irq, ret;
+
+	ctrl = devm_spi_alloc_host(dev, sizeof(*snand));
+	if (!ctrl)
+		return -ENOMEM;
+
+	snand = spi_controller_get_devdata(ctrl);
+	snand->dev = dev;
+
+	base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(base))
+		return PTR_ERR(base);
+
+	snand->regmap = devm_regmap_init_mmio(dev, base, &rc);
+	if (IS_ERR(snand->regmap))
+		return PTR_ERR(snand->regmap);
+
+	init_completion(&snand->comp);
+
+	irq = platform_get_irq(pdev, 0);
+	if (irq < 0)
+		return irq;
+
+	ret = dma_set_mask(snand->dev, DMA_BIT_MASK(32));
+	if (ret)
+		return dev_err_probe(dev, ret, "failed to set DMA mask\n");
+
+	ret = devm_request_irq(dev, irq, rtl_snand_irq, 0, "rtl-snand", snand);
+	if (ret)
+		return dev_err_probe(dev, ret, "failed to request irq\n");
+
+	ctrl->num_chipselect = 2;
+	ctrl->mem_ops = &rtl_snand_mem_ops;
+	ctrl->bits_per_word_mask = SPI_BPW_MASK(8);
+	ctrl->mode_bits = SPI_RX_DUAL | SPI_RX_QUAD | SPI_TX_DUAL | SPI_TX_QUAD;
+	device_set_node(&ctrl->dev, dev_fwnode(dev));
+
+	return devm_spi_register_controller(dev, ctrl);
+}
+
+static struct platform_driver rtl_snand_driver = {
+	.driver = {
+		.name = "realtek-rtl-snand",
+		.of_match_table = rtl_snand_match,
+	},
+	.probe = rtl_snand_probe,
+};
+module_platform_driver(rtl_snand_driver);
+
+MODULE_DESCRIPTION("Realtek SPI-NAND Flash Controller Driver");
+MODULE_LICENSE("GPL");
