From b899c45208d6f204a6da9a1132577993eeecf0fb Mon Sep 17 00:00:00 2001
From: Boris Brezillon <boris.brezillon@free-electrons.com>
Date: Fri, 2 Dec 2016 14:48:12 +0100
Subject: [PATCH] ARM: dts: bcm283x: Add VEC node in bcm283x.dtsi

Add the VEC (Video EnCoder) node definition in bcm283x.dtsi.

Signed-off-by: Boris Brezillon <boris.brezillon@free-electrons.com>
Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm283x.dtsi | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/arch/arm/boot/dts/bcm283x.dtsi
+++ b/arch/arm/boot/dts/bcm283x.dtsi
@@ -481,6 +481,14 @@
 			status = "disabled";
 		};
 
+		vec: vec@7e806000 {
+			compatible = "brcm,bcm2835-vec";
+			reg = <0x7e806000 0x1000>;
+			clocks = <&clocks BCM2835_CLOCK_VEC>;
+			interrupts = <2 27>;
+			status = "disabled";
+		};
+
 		pixelvalve@7e807000 {
 			compatible = "brcm,bcm2835-pixelvalve2";
 			reg = <0x7e807000 0x100>;
