#!/bin/sh

. /lib/functions/uci-defaults.sh

board=$(board_name)
board_config_update

case $board in
	"akitio,myloud")
		ucidef_set_led_default "status" "status" "akitio:red:status" "0"
		;;
	"mitrastar,stg-212")
		ucidef_set_led_default "power" "power" "zyxel:blue:status" "1"
		ucidef_set_led_usbdev "usb" "USB" "zyxel:orange:copy" "1-1"
		;;
	"shuttle,kd20")
		ucidef_set_led_default "power" "power" "kd20:blue:status" "1"
		;;
	"cloudengines,pogoplug"*)
		ucidef_set_led_default "power" "power" "pogoplug:blue:internal" "1"
		;;

esac

board_config_flush

exit 0
