From 22d319f2665dd3458d59c934fa0c8cf1b1d7227f Mon Sep 17 00:00:00 2001
From: Stijn Tintel <stijn@linux-ipv6.be>
Date: Sat, 10 Nov 2018 13:25:20 +0200
Subject: [PATCH wireless-drivers] brcmfmac: fix roamoff=1 modparam

When the update_connect_param callback is set, nl80211 expects the flag
WIPHY_FLAG_SUPPORTS_FW_ROAM to be set as well. However, this flag is
only set when modparam roamoff=0, while the callback is set
unconditionally. Since commit 7f9a3e150ec7 this causes a warning in
wiphy_register, which breaks brcmfmac.

Disable the update_connect_param callback when roamoff=0 to fix this.

Fixes: 7f9a3e150ec7 ("nl80211: Update ERP info using NL80211_CMD_UPDATE_CONNECT_PARAMS")
Cc: Stable <stable@vger.kernel.org> # 4.19+
Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
Signed-off-by: Stijn Tintel <stijn@linux-ipv6.be>
---
 .../wireless/broadcom/brcm80211/brcmfmac/cfg80211.c   | 11 +++++++++--
 .../wireless/broadcom/brcm80211/brcmfmac/cfg80211.h   |  2 +-
 .../net/wireless/broadcom/brcm80211/brcmfmac/core.c   |  2 +-
 3 files changed, 11 insertions(+), 4 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
@@ -5188,10 +5188,17 @@ static struct cfg80211_ops brcmf_cfg8021
 	.del_pmk = brcmf_cfg80211_del_pmk,
 };
 
-struct cfg80211_ops *brcmf_cfg80211_get_ops(void)
+struct cfg80211_ops *brcmf_cfg80211_get_ops(struct brcmf_mp_device *settings)
 {
-	return kmemdup(&brcmf_cfg80211_ops, sizeof(brcmf_cfg80211_ops),
+	struct cfg80211_ops *ops;
+
+	ops = kmemdup(&brcmf_cfg80211_ops, sizeof(brcmf_cfg80211_ops),
 		       GFP_KERNEL);
+
+	if (ops && settings->roamoff)
+		ops->update_connect_params = NULL;
+
+	return ops;
 }
 
 struct brcmf_cfg80211_vif *brcmf_alloc_vif(struct brcmf_cfg80211_info *cfg,
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h
@@ -404,7 +404,7 @@ struct brcmf_cfg80211_info *brcmf_cfg802
 void brcmf_cfg80211_detach(struct brcmf_cfg80211_info *cfg);
 s32 brcmf_cfg80211_up(struct net_device *ndev);
 s32 brcmf_cfg80211_down(struct net_device *ndev);
-struct cfg80211_ops *brcmf_cfg80211_get_ops(void);
+struct cfg80211_ops *brcmf_cfg80211_get_ops(struct brcmf_mp_device *settings);
 enum nl80211_iftype brcmf_cfg80211_get_iftype(struct brcmf_if *ifp);
 
 struct brcmf_cfg80211_vif *brcmf_alloc_vif(struct brcmf_cfg80211_info *cfg,
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.c
@@ -1151,7 +1151,7 @@ int brcmf_attach(struct device *dev, str
 
 	brcmf_dbg(TRACE, "Enter\n");
 
-	ops = brcmf_cfg80211_get_ops();
+	ops = brcmf_cfg80211_get_ops(settings);
 	if (!ops)
 		return -ENOMEM;
 
