/*
 * Device Tree file for the Linksys E1700
 *
 * Copyright (C) 2014 Imre Kaloz <kaloz@openwrt.org>
 *
 * This file is licensed under the terms of the GNU General Public
 * License version 2.  This program is licensed "as is" without any
 * warranty of any kind, whether express or implied.
 */

/dts-v1/;

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "linksys,e1700", "ralink,mt7620a-soc";
	model = "Linksys E1700";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "e1700:green:power";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};

		wan {
			label = "e1700:green:wps";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x28>;
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii1_pins &rgmii2_pins &mdio_pins>;

	port@5 {
		status = "okay";
		mediatek,fixed-link = <1000 1 1 1>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			reg = <0>;
			phy-mode = "rgmii";
		};

		phy1: ethernet-phy@1 {
			reg = <1>;
			phy-mode = "rgmii";
		};

		phy2: ethernet-phy@2 {
			reg = <2>;
			phy-mode = "rgmii";
		};

		phy3: ethernet-phy@3 {
			reg = <3>;
			phy-mode = "rgmii";
		};

		phy4: ethernet-phy@4 {
			reg = <4>;
			phy-mode = "rgmii";
		};

		phy1f: ethernet-phy@1f {
			reg = <0x1f>;
			phy-mode = "rgmii";
		};
	};
};

&gsw {
	mediatek,port4 = "gmac";
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};
