#!/bin/sh

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
mikrotik,rb750gr3)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "17"
	;;
ubnt-erx)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "0"
	;;
ubnt-erx-sfp)
	ucidef_add_gpio_switch "poe_power_port0" "PoE Power Port0" "496"
	ucidef_add_gpio_switch "poe_power_port1" "PoE Power Port1" "497"
	ucidef_add_gpio_switch "poe_power_port2" "PoE Power Port2" "498"
	ucidef_add_gpio_switch "poe_power_port3" "PoE Power Port3" "499"
	ucidef_add_gpio_switch "poe_power_port4" "PoE Power Port4" "500"
	;;
esac

board_config_flush

exit 0
