From 21ff843931b2e5a9b628ac56fd0f2e4355890096 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Mon, 19 Sep 2016 10:43:18 +0200
Subject: [PATCH] ARM: dts: bcm283x: Define standard pinctrl groups in the gpio
 node.

The BCM2835-ARM-Peripherals.pdf documentation specifies what the
function selects do for the pins, and there are a bunch of obvious
groupings to be made.  With these created, we'll be able to replace
bcm2835-rpi.dtsi's main "set all of these pins to alt0" with
references to specific groups we want enabled.

Also add pinctrl groups for emmc and sdhost.

Based on patches by Eric Anholt, with fixups by Gerd Hoffmann.

Signed-off-by: Gerd Hoffmann <kraxel@redhat.com>
Signed-off-by: Eric Anholt <eric@anholt.net>
Acked-by: Stefan Wahren <stefan.wahren@i2se.com>
---
 arch/arm/boot/dts/bcm283x.dtsi | 203 +++++++++++++++++++++++++++++++++++++++++
 1 file changed, 203 insertions(+)

--- a/arch/arm/boot/dts/bcm283x.dtsi
+++ b/arch/arm/boot/dts/bcm283x.dtsi
@@ -137,6 +137,209 @@
 
 			interrupt-controller;
 			#interrupt-cells = <2>;
+
+			/* Defines pin muxing groups according to
+			 * BCM2835-ARM-Peripherals.pdf page 102.
+			 *
+			 * While each pin can have its mux selected
+			 * for various functions individually, some
+			 * groups only make sense to switch to a
+			 * particular function together.
+			 */
+			dpi_gpio0: dpi_gpio0 {
+				brcm,pins = <0 1 2 3 4 5 6 7 8 9 10 11
+					     12 13 14 15 16 17 18 19
+					     20 21 22 23 24 25 26 27>;
+				brcm,function = <BCM2835_FSEL_ALT2>;
+			};
+			emmc_gpio22: emmc_gpio22 {
+				brcm,pins = <22 23 24 25 26 27>;
+				brcm,function = <BCM2835_FSEL_ALT3>;
+			};
+			emmc_gpio34: emmc_gpio34 {
+				brcm,pins = <34 35 36 37 38 39>;
+				brcm,function = <BCM2835_FSEL_ALT3>;
+				brcm,pull = <BCM2835_PUD_OFF
+					     BCM2835_PUD_UP
+					     BCM2835_PUD_UP
+					     BCM2835_PUD_UP
+					     BCM2835_PUD_UP
+					     BCM2835_PUD_UP>;
+			};
+			emmc_gpio48: emmc_gpio48 {
+				brcm,pins = <48 49 50 51 52 53>;
+				brcm,function = <BCM2835_FSEL_ALT3>;
+			};
+
+			gpclk0_gpio4: gpclk0_gpio4 {
+				brcm,pins = <4>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			gpclk1_gpio5: gpclk1_gpio5 {
+				brcm,pins = <5>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			gpclk1_gpio42: gpclk1_gpio42 {
+				brcm,pins = <42>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			gpclk1_gpio44: gpclk1_gpio44 {
+				brcm,pins = <44>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			gpclk2_gpio6: gpclk2_gpio6 {
+				brcm,pins = <6>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			gpclk2_gpio43: gpclk2_gpio43 {
+				brcm,pins = <43>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+
+			i2c0_gpio0: i2c0_gpio0 {
+				brcm,pins = <0 1>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			i2c0_gpio32: i2c0_gpio32 {
+				brcm,pins = <32 34>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			i2c0_gpio44: i2c0_gpio44 {
+				brcm,pins = <44 45>;
+				brcm,function = <BCM2835_FSEL_ALT1>;
+			};
+			i2c1_gpio2: i2c1_gpio2 {
+				brcm,pins = <2 3>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			i2c1_gpio44: i2c1_gpio44 {
+				brcm,pins = <44 45>;
+				brcm,function = <BCM2835_FSEL_ALT2>;
+			};
+			i2c_slave_gpio18: i2c_slave_gpio18 {
+				brcm,pins = <18 19 20 21>;
+				brcm,function = <BCM2835_FSEL_ALT3>;
+			};
+
+			jtag_gpio4: jtag_gpio4 {
+				brcm,pins = <4 5 6 12 13>;
+				brcm,function = <BCM2835_FSEL_ALT4>;
+			};
+			jtag_gpio22: jtag_gpio22 {
+				brcm,pins = <22 23 24 25 26 27>;
+				brcm,function = <BCM2835_FSEL_ALT4>;
+			};
+
+			pcm_gpio18: pcm_gpio18 {
+				brcm,pins = <18 19 20 21>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			pcm_gpio28: pcm_gpio28 {
+				brcm,pins = <28 29 30 31>;
+				brcm,function = <BCM2835_FSEL_ALT2>;
+			};
+
+			pwm0_gpio12: pwm0_gpio12 {
+				brcm,pins = <12>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			pwm0_gpio18: pwm0_gpio18 {
+				brcm,pins = <18>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
+			pwm0_gpio40: pwm0_gpio40 {
+				brcm,pins = <40>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			pwm1_gpio13: pwm1_gpio13 {
+				brcm,pins = <13>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			pwm1_gpio19: pwm1_gpio19 {
+				brcm,pins = <19>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
+			pwm1_gpio41: pwm1_gpio41 {
+				brcm,pins = <41>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			pwm1_gpio45: pwm1_gpio45 {
+				brcm,pins = <45>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+
+			sdhost_gpio48: sdhost_gpio48 {
+				brcm,pins = <48 49 50 51 52 53>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+
+			spi0_gpio7: spi0_gpio7 {
+				brcm,pins = <7 8 9 10 11>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			spi0_gpio35: spi0_gpio35 {
+				brcm,pins = <35 36 37 38 39>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			spi1_gpio16: spi1_gpio16 {
+				brcm,pins = <16 17 18 19 20 21>;
+				brcm,function = <BCM2835_FSEL_ALT4>;
+			};
+			spi2_gpio40: spi2_gpio40 {
+				brcm,pins = <40 41 42 43 44 45>;
+				brcm,function = <BCM2835_FSEL_ALT4>;
+			};
+
+			uart0_gpio14: uart0_gpio14 {
+				brcm,pins = <14 15>;
+				brcm,function = <BCM2835_FSEL_ALT0>;
+			};
+			/* Separate from the uart0_gpio14 group
+			 * because it conflicts with spi1_gpio16, and
+			 * people often run uart0 on the two pins
+			 * without flow contrl.
+			 */
+			uart0_ctsrts_gpio16: uart0_ctsrts_gpio16 {
+				brcm,pins = <16 17>;
+				brcm,function = <BCM2835_FSEL_ALT3>;
+			};
+			uart0_gpio30: uart0_gpio30 {
+				brcm,pins = <30 31>;
+				brcm,function = <BCM2835_FSEL_ALT3>;
+			};
+			uart0_ctsrts_gpio32: uart0_ctsrts_gpio32 {
+				brcm,pins = <32 33>;
+				brcm,function = <BCM2835_FSEL_ALT3>;
+			};
+
+			uart1_gpio14: uart1_gpio14 {
+				brcm,pins = <14 15>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
+			uart1_ctsrts_gpio16: uart1_ctsrts_gpio16 {
+				brcm,pins = <16 17>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
+			uart1_gpio32: uart1_gpio32 {
+				brcm,pins = <32 33>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
+			uart1_ctsrts_gpio30: uart1_ctsrts_gpio30 {
+				brcm,pins = <30 31>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
+			uart1_gpio36: uart1_gpio36 {
+				brcm,pins = <36 37 38 39>;
+				brcm,function = <BCM2835_FSEL_ALT2>;
+			};
+			uart1_gpio40: uart1_gpio40 {
+				brcm,pins = <40 41>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
+			uart1_ctsrts_gpio42: uart1_ctsrts_gpio42 {
+				brcm,pins = <42 43>;
+				brcm,function = <BCM2835_FSEL_ALT5>;
+			};
 		};
 
 		uart0: serial@7e201000 {
