/dts-v1/;

#include "skeleton.dtsi"
#include <dt-bindings/clock/qcom,gcc-ipq806x.h>
#include <dt-bindings/mfd/qcom-rpm.h>
#include <dt-bindings/clock/qcom,rpmcc.h>
#include <dt-bindings/clock/qcom,lcc-ipq806x.h>
#include <dt-bindings/soc/qcom,gsbi.h>
#include <dt-bindings/reset/qcom,gcc-ipq806x.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	model = "Qualcomm IPQ8064";
	compatible = "qcom,ipq8064";
	interrupt-parent = <&intc>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc0>;
			qcom,saw = <&saw0>;
			clocks = <&kraitcc 0>, <&kraitcc 4>;
			clock-names = "cpu", "l2";
			clock-latency = <100000>;
			cpu-supply = <&smb208_s2a>;
			voltage-tolerance = <5>;
			cooling-min-state = <0>;
			cooling-max-state = <10>;
			#cooling-cells = <2>;
			cpu-idle-states = <&CPU_SPC>;
		};

		cpu1: cpu@1 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc1>;
			qcom,saw = <&saw1>;
			clocks = <&kraitcc 1>, <&kraitcc 4>;
			clock-names = "cpu", "l2";
			clock-latency = <100000>;
			cpu-supply = <&smb208_s2b>;
			cooling-min-state = <0>;
			cooling-max-state = <10>;
			#cooling-cells = <2>;
			cpu-idle-states = <&CPU_SPC>;
		};

		L2: l2-cache {
			compatible = "cache";
			cache-level = <2>;
			qcom,saw = <&saw_l2>;
		};

		qcom,l2 {
			qcom,l2-rates = <384000000 1000000000 1200000000>;
		};

		idle-states {
			CPU_SPC: spc {
				compatible = "qcom,idle-state-spc",
						"arm,idle-state";
				entry-latency-us = <400>;
				exit-latency-us = <900>;
				min-residency-us = <3000>;
			};
		};
	};

	thermal-zones {
		tsens_tz_sensor0 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 0>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor1 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 1>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor2 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 2>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor3 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 3>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor4 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 4>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor5 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 5>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor6 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 6>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor7 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 7>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor8 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 8>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor9 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 9>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};

		tsens_tz_sensor10 {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 10>;

			trips {
				cpu-critical-hi {
					temperature = <125000>;
					hysteresis = <2000>;
					type = "critical_high";
				};

				cpu-config-hi {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "configurable_hi";
				};

				cpu-config-lo {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "configurable_lo";
				};

				cpu-critical-low {
					temperature = <0>;
					hysteresis = <2000>;
					type = "critical_low";
				};
			};
		};
	};

	cpu-pmu {
		compatible = "qcom,krait-pmu";
		interrupts = <1 10 0x304>;
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		nss@40000000 {
			reg = <0x40000000 0x1000000>;
			no-map;
		};

		smem: smem@41000000 {
			reg = <0x41000000 0x200000>;
			no-map;
		};
	};

	clocks {
		cxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <25000000>;
		};

		pxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <25000000>;
		};

		sleep_clk: sleep_clk {
			compatible = "fixed-clock";
			clock-frequency = <32768>;
			#clock-cells = <0>;
		};
	};

	firmware {
		scm {
			compatible = "qcom,scm-ipq806x";
		};
	};

	kraitcc: clock-controller {
		compatible = "qcom,krait-cc-v1";
		#clock-cells = <1>;
	};

	qcom,pvs {
		qcom,pvs-format-a;
		qcom,speed0-pvs0-bin-v0 =
			< 1400000000 1250000 >,
			< 1200000000 1200000 >,
			< 1000000000 1150000 >,
			 < 800000000 1100000 >,
			 < 600000000 1050000 >,
			 < 384000000 1000000 >;

		qcom,speed0-pvs1-bin-v0 =
			< 1400000000 1175000 >,
			< 1200000000 1125000 >,
			< 1000000000 1075000 >,
			 < 800000000 1025000 >,
			 < 600000000  975000 >,
			 < 384000000  925000 >;

		qcom,speed0-pvs2-bin-v0 =
			< 1400000000 1125000 >,
			< 1200000000 1075000 >,
			< 1000000000 1025000 >,
			 < 800000000  995000 >,
			 < 600000000  925000 >,
			 < 384000000  875000 >;

		qcom,speed0-pvs3-bin-v0 =
			< 1400000000 1050000 >,
			< 1200000000 1000000 >,
			< 1000000000  950000 >,
			 < 800000000  900000 >,
			 < 600000000  850000 >,
			 < 384000000  800000 >;
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		lpass@28100000 {
			compatible = "qcom,lpass-cpu";
			status = "disabled";
			clocks = <&lcc AHBIX_CLK>,
					<&lcc MI2S_OSR_CLK>,
					<&lcc MI2S_BIT_CLK>;
			clock-names = "ahbix-clk",
					"mi2s-osr-clk",
					"mi2s-bit-clk";
			interrupts = <0 85 1>;
			interrupt-names = "lpass-irq-lpaif";
			reg = <0x28100000 0x10000>;
			reg-names = "lpass-lpaif";
		};

		qfprom: qfprom@700000 {
			compatible = "qcom,qfprom", "syscon";
			reg = <0x700000 0x1000>;
			#address-cells = <1>;
			#size-cells = <1>;
			status = "okay";
			tsens_calib: calib@400 {
				reg = <0x400 0x10>;
			};
			tsens_backup: backup@410 {
				reg = <0x410 0x10>;
			};
		};

		rpm@108000 {
			compatible = "qcom,rpm-ipq8064";
			reg = <0x108000 0x1000>;
			qcom,ipc = <&l2cc 0x8 2>;

			interrupts = <0 19 0>,
				     <0 21 0>,
				     <0 22 0>;
			interrupt-names = "ack",
					  "err",
					  "wakeup";

			clocks = <&gcc RPM_MSG_RAM_H_CLK>;
			clock-names = "ram";

			#address-cells = <1>;
			#size-cells = <0>;

			rpmcc: clock-controller {
				compatible	= "qcom,rpmcc-ipq806x", "qcom,rpmcc";
				#clock-cells = <1>;
			};

			regulators {
				compatible = "qcom,rpm-smb208-regulators";

				smb208_s1a: s1a {
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1150000>;

					qcom,switch-mode-frequency = <1200000>;

				};

				smb208_s1b: s1b {
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1150000>;

					qcom,switch-mode-frequency = <1200000>;
				};

				smb208_s2a: s2a {
					regulator-min-microvolt = < 800000>;
					regulator-max-microvolt = <1250000>;

					qcom,switch-mode-frequency = <1200000>;
				};

				smb208_s2b: s2b {
					regulator-min-microvolt = < 800000>;
					regulator-max-microvolt = <1250000>;

					qcom,switch-mode-frequency = <1200000>;
				};
			};
		};

		rng@1a500000 {
			compatible = "qcom,prng";
			reg = <0x1a500000 0x200>;
			clocks = <&gcc PRNG_CLK>;
			clock-names = "core";
		};

		qcom_pinmux: pinmux@800000 {
			compatible = "qcom,ipq8064-pinctrl";
			reg = <0x800000 0x4000>;

			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			interrupts = <0 16 0x4>;

			pcie0_pins: pcie0_pinmux {
				mux {
					pins = "gpio3";
					function = "pcie1_rst";
					drive-strength = <2>;
					bias-disable;
				};
			};

			pcie1_pins: pcie1_pinmux {
				mux {
					pins = "gpio48";
					function = "pcie2_rst";
					drive-strength = <2>;
					bias-disable;
				};
			};

			pcie2_pins: pcie2_pinmux {
				mux {
					pins = "gpio63";
					function = "pcie3_rst";
					drive-strength = <2>;
					bias-disable;
					output-low;
				};
			};
		};

		intc: interrupt-controller@2000000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0x02000000 0x1000>,
			      <0x02002000 0x1000>;
		};

		timer@200a000 {
			compatible = "qcom,kpss-timer", "qcom,msm-timer";
			interrupts = <1 1 0x301>,
				     <1 2 0x301>,
				     <1 3 0x301>,
				     <1 4 0x301>,
				     <1 5 0x301>;
			reg = <0x0200a000 0x100>;
			clock-frequency = <25000000>,
					  <32768>;
			clocks = <&sleep_clk>;
			clock-names = "sleep";
			cpu-offset = <0x80000>;
		};

		acc0: clock-controller@2088000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02088000 0x1000>, <0x02008000 0x1000>;
			clock-output-names = "acpu0_aux";
		};

		acc1: clock-controller@2098000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02098000 0x1000>, <0x02008000 0x1000>;
			clock-output-names = "acpu1_aux";
		};

		l2cc: clock-controller@2011000 {
			compatible = "qcom,kpss-gcc", "syscon";
			reg = <0x2011000 0x1000>;
			clock-output-names = "acpu_l2_aux";
		};

		saw0: regulator@2089000 {
			compatible = "qcom,saw2", "syscon";
			reg = <0x02089000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		saw1: regulator@2099000 {
			compatible = "qcom,saw2", "syscon";
			reg = <0x02099000 0x1000>, <0x02009000 0x1000>;
			regulator;
		};

		saw_l2: regulator@02012000 {
			compatible = "qcom,saw2", "syscon";
			reg = <0x02012000 0x1000>;
			regulator;
		};

		sic_non_secure: sic-non-secure@12100000 {
			compatible = "syscon";
			reg = <0x12100000 0x10000>;
		};

		gsbi2: gsbi@12480000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <2>;
			reg = <0x12480000 0x100>;
			clocks = <&gcc GSBI2_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			uart2: serial@12490000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x12490000 0x1000>,
				      <0x12480000 0x1000>;
				interrupts = <0 195 0x0>;
				clocks = <&gcc GSBI2_UART_CLK>, <&gcc GSBI2_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@124a0000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x124a0000 0x1000>;
				interrupts = <0 196 0>;

				clocks = <&gcc GSBI2_QUP_CLK>, <&gcc GSBI2_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};

		};

		gsbi4: gsbi@16300000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <4>;
			reg = <0x16300000 0x100>;
			clocks = <&gcc GSBI4_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			gsbi4_serial: serial@16340000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16340000 0x1000>,
				      <0x16300000 0x1000>;
				interrupts = <0 152 0x0>;
				clocks = <&gcc GSBI4_UART_CLK>, <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@16380000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16380000 0x1000>;
				interrupts = <0 153 0>;

				clocks = <&gcc GSBI4_QUP_CLK>, <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		gsbi5: gsbi@1a200000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <5>;
			reg = <0x1a200000 0x100>;
			clocks = <&gcc GSBI5_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			uart5: serial@1a240000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x1a240000 0x1000>,
				      <0x1a200000 0x1000>;
				interrupts = <0 154 0x0>;
				clocks = <&gcc GSBI5_UART_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@1a280000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x1a280000 0x1000>;
				interrupts = <0 155 0>;

				clocks = <&gcc GSBI5_QUP_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};

			spi@1a280000 {
				compatible = "qcom,spi-qup-v1.1.1";
				reg = <0x1a280000 0x1000>;
				interrupts = <0 155 0>;

				clocks = <&gcc GSBI5_QUP_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		sata_phy: sata-phy@1b400000 {
			compatible = "qcom,ipq806x-sata-phy";
			reg = <0x1b400000 0x200>;

			clocks = <&gcc SATA_PHY_CFG_CLK>;
			clock-names = "cfg";

			#phy-cells = <0>;
			status = "disabled";
		};

		sata@29000000 {
			compatible = "qcom,ipq806x-ahci", "generic-ahci";
			reg = <0x29000000 0x180>;

			interrupts = <0 209 0x0>;

			clocks = <&gcc SFAB_SATA_S_H_CLK>,
				 <&gcc SATA_H_CLK>,
				 <&gcc SATA_A_CLK>,
				 <&gcc SATA_RXOOB_CLK>,
				 <&gcc SATA_PMALIVE_CLK>;
			clock-names = "slave_face", "iface", "core",
					"rxoob", "pmalive";

			assigned-clocks = <&gcc SATA_RXOOB_CLK>, <&gcc SATA_PMALIVE_CLK>;
			assigned-clock-rates = <100000000>, <100000000>;

			phys = <&sata_phy>;
			phy-names = "sata-phy";
			status = "disabled";
		};

		qcom,ssbi@500000 {
			compatible = "qcom,ssbi";
			reg = <0x00500000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		gcc: clock-controller@900000 {
			compatible = "qcom,gcc-ipq8064";
			reg = <0x00900000 0x4000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
			#power-domain-cells = <1>;
		};

		tsens: thermal-sensor@900000 {
			compatible = "qcom,ipq8064-tsens";
			reg = <0x900000 0x3680>;
			nvmem-cells = <&tsens_calib>, <&tsens_backup>;
			nvmem-cell-names = "calib", "calib_backup";
			interrupts = <0 178 0>;
			#thermal-sensor-cells = <1>;
		};

		tcsr: syscon@1a400000 {
			compatible = "qcom,tcsr-ipq8064", "syscon";
			reg = <0x1a400000 0x100>;
		};

		lcc: clock-controller@28000000 {
			compatible = "qcom,lcc-ipq8064";
			reg = <0x28000000 0x1000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
		};

		sfpb_mutex_block: syscon@1200600 {
			compatible = "syscon";
			reg = <0x01200600 0x100>;
		};

		hs_phy_1: phy@100f8800 {
			compatible = "qcom,dwc3-hs-usb-phy";
			reg = <0x100f8800 0x30>;
			clocks = <&gcc USB30_1_UTMI_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		ss_phy_1: phy@100f8830 {
			compatible = "qcom,dwc3-ss-usb-phy";
			reg = <0x100f8830 0x30>;
			clocks = <&gcc USB30_1_MASTER_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		hs_phy_0: phy@110f8800 {
			compatible = "qcom,dwc3-hs-usb-phy";
			reg = <0x110f8800 0x30>;
			clocks = <&gcc USB30_0_UTMI_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		ss_phy_0: phy@110f8830 {
			compatible = "qcom,dwc3-ss-usb-phy";
			reg = <0x110f8830 0x30>;
			clocks = <&gcc USB30_0_MASTER_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		usb3_0: usb30@0 {
			compatible = "qcom,dwc3";
			#address-cells = <1>;
			#size-cells = <1>;
			clocks = <&gcc USB30_0_MASTER_CLK>;
			clock-names = "core";

			ranges;

			resets = <&gcc USB30_0_MASTER_RESET>;
			reset-names = "usb30_0_mstr_rst";

			status = "disabled";

			dwc3_0: dwc3@11000000 {
				compatible = "snps,dwc3";
				reg = <0x11000000 0xcd00>;
				interrupts = <0 110 0x4>;
				phys = <&hs_phy_0>, <&ss_phy_0>;
				phy-names = "usb2-phy", "usb3-phy";
				dr_mode = "host";
				snps,dis_u3_susphy_quirk;
			};
		};

		usb3_1: usb30@1 {
			compatible = "qcom,dwc3";
			#address-cells = <1>;
			#size-cells = <1>;
			clocks = <&gcc USB30_1_MASTER_CLK>;
			clock-names = "core";

			ranges;

			resets = <&gcc USB30_1_MASTER_RESET>;
			reset-names = "usb30_1_mstr_rst";

			status = "disabled";

			dwc3_1: dwc3@10000000 {
				compatible = "snps,dwc3";
				reg = <0x10000000 0xcd00>;
				interrupts = <0 205 0x4>;
				phys = <&hs_phy_1>, <&ss_phy_1>;
				phy-names = "usb2-phy", "usb3-phy";
				dr_mode = "host";
				snps,dis_u3_susphy_quirk;
			};
		};

		pcie0: pci@1b500000 {
			compatible = "qcom,pcie-ipq8064";
			reg = <0x1b500000 0x1000
			       0x1b502000 0x80
			       0x1b600000 0x100
			       0x0ff00000 0x100000>;
			reg-names = "dbi", "elbi", "parf", "config";
			device_type = "pci";
			linux,pci-domain = <0>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;
			#address-cells = <3>;
			#size-cells = <2>;

			ranges = <0x81000000 0 0x0fe00000 0x0fe00000 0 0x00100000   /* downstream I/O */
				  0x82000000 0 0x08000000 0x08000000 0 0x07e00000>; /* non-prefetchable memory */

			interrupts = <GIC_SPI 35 IRQ_TYPE_NONE>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 36 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 37 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 38 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 39 IRQ_TYPE_LEVEL_HIGH>; /* int_d */

			clocks = <&gcc PCIE_A_CLK>,
				 <&gcc PCIE_H_CLK>,
				 <&gcc PCIE_PHY_CLK>,
				 <&gcc PCIE_AUX_CLK>,
				 <&gcc PCIE_ALT_REF_CLK>;
			clock-names = "core", "iface", "phy", "aux", "ref";

			assigned-clocks = <&gcc PCIE_ALT_REF_CLK>;
			assigned-clock-rates = <100000000>;

			resets = <&gcc PCIE_ACLK_RESET>,
				 <&gcc PCIE_HCLK_RESET>,
				 <&gcc PCIE_POR_RESET>,
				 <&gcc PCIE_PCI_RESET>,
				 <&gcc PCIE_PHY_RESET>,
				 <&gcc PCIE_EXT_RESET>;
			reset-names = "axi", "ahb", "por", "pci", "phy", "ext";

			pinctrl-0 = <&pcie0_pins>;
			pinctrl-names = "default";

			perst-gpios = <&qcom_pinmux 3 GPIO_ACTIVE_LOW>;

			phy-tx0-term-offset = <7>;

			status = "disabled";
		};

		pcie1: pci@1b700000 {
			compatible = "qcom,pcie-ipq8064";
			reg = <0x1b700000 0x1000
			       0x1b702000 0x80
			       0x1b800000 0x100
			       0x31f00000 0x100000>;
			reg-names = "dbi", "elbi", "parf", "config";
			device_type = "pci";
			linux,pci-domain = <1>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;
			#address-cells = <3>;
			#size-cells = <2>;

			ranges = <0x81000000 0 0x31e00000 0x31e00000 0 0x00100000   /* downstream I/O */
				  0x82000000 0 0x2e000000 0x2e000000 0 0x03e00000>; /* non-prefetchable memory */

			interrupts = <GIC_SPI 57 IRQ_TYPE_NONE>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 58 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 59 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 60 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 61 IRQ_TYPE_LEVEL_HIGH>; /* int_d */

			clocks = <&gcc PCIE_1_A_CLK>,
				 <&gcc PCIE_1_H_CLK>,
				 <&gcc PCIE_1_PHY_CLK>,
				 <&gcc PCIE_1_AUX_CLK>,
				 <&gcc PCIE_1_ALT_REF_CLK>;
			clock-names = "core", "iface", "phy", "aux", "ref";

			assigned-clocks = <&gcc PCIE_1_ALT_REF_CLK>;
			assigned-clock-rates = <100000000>;

			resets = <&gcc PCIE_1_ACLK_RESET>,
				 <&gcc PCIE_1_HCLK_RESET>,
				 <&gcc PCIE_1_POR_RESET>,
				 <&gcc PCIE_1_PCI_RESET>,
				 <&gcc PCIE_1_PHY_RESET>,
				 <&gcc PCIE_1_EXT_RESET>;
			reset-names = "axi", "ahb", "por", "pci", "phy", "ext";

			pinctrl-0 = <&pcie1_pins>;
			pinctrl-names = "default";

			perst-gpios = <&qcom_pinmux 48 GPIO_ACTIVE_LOW>;

			phy-tx0-term-offset = <7>;

			status = "disabled";
		};

		pcie2: pci@1b900000 {
			compatible = "qcom,pcie-ipq8064";
			reg = <0x1b900000 0x1000
			       0x1b902000 0x80
			       0x1ba00000 0x100
			       0x35f00000 0x100000>;
			reg-names = "dbi", "elbi", "parf", "config";
			device_type = "pci";
			linux,pci-domain = <2>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;
			#address-cells = <3>;
			#size-cells = <2>;

			ranges = <0x81000000 0 0x35e00000 0x35e00000 0 0x00100000   /* downstream I/O */
				  0x82000000 0 0x32000000 0x32000000 0 0x03e00000>; /* non-prefetchable memory */

			interrupts = <GIC_SPI 71 IRQ_TYPE_NONE>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 72 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 73 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 74 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 75 IRQ_TYPE_LEVEL_HIGH>; /* int_d */

			clocks = <&gcc PCIE_2_A_CLK>,
				 <&gcc PCIE_2_H_CLK>,
				 <&gcc PCIE_2_PHY_CLK>,
				 <&gcc PCIE_2_AUX_CLK>,
				 <&gcc PCIE_2_ALT_REF_CLK>;
			clock-names = "core", "iface", "phy", "aux", "ref";

			assigned-clocks = <&gcc PCIE_2_ALT_REF_CLK>;
			assigned-clock-rates = <100000000>;

			resets = <&gcc PCIE_2_ACLK_RESET>,
				 <&gcc PCIE_2_HCLK_RESET>,
				 <&gcc PCIE_2_POR_RESET>,
				 <&gcc PCIE_2_PCI_RESET>,
				 <&gcc PCIE_2_PHY_RESET>,
				 <&gcc PCIE_2_EXT_RESET>;
			reset-names = "axi", "ahb", "por", "pci", "phy", "ext";

			pinctrl-0 = <&pcie2_pins>;
			pinctrl-names = "default";

			perst-gpios = <&qcom_pinmux 63 GPIO_ACTIVE_LOW>;

			phy-tx0-term-offset = <7>;

			status = "disabled";
		};

		adm_dma: dma@18300000 {
			compatible = "qcom,adm";
			reg = <0x18300000 0x100000>;
			interrupts = <0 170 0>;
			#dma-cells = <1>;

			clocks = <&gcc ADM0_CLK>, <&gcc ADM0_PBUS_CLK>;
			clock-names = "core", "iface";

			resets = <&gcc ADM0_RESET>,
				 <&gcc ADM0_PBUS_RESET>,
				 <&gcc ADM0_C0_RESET>,
				 <&gcc ADM0_C1_RESET>,
				 <&gcc ADM0_C2_RESET>;
			reset-names = "clk", "pbus", "c0", "c1", "c2";
			qcom,ee = <0>;

			status = "disabled";
		};

		nand@1ac00000 {
			compatible = "qcom,ipq806x-nand";
			reg = <0x1ac00000 0x800>;

			clocks = <&gcc EBI2_CLK>,
				 <&gcc EBI2_AON_CLK>;
			clock-names = "core", "aon";

			dmas = <&adm_dma 3>;
			dma-names = "rxtx";
			qcom,cmd-crci = <15>;
			qcom,data-crci = <3>;

			status = "disabled";

			#address-cells = <1>;
			#size-cells = <0>;
		};

		nss_common: syscon@03000000 {
			compatible = "syscon";
			reg = <0x03000000 0x0000FFFF>;
		};

		qsgmii_csr: syscon@1bb00000 {
			compatible = "syscon";
			reg = <0x1bb00000 0x000001FF>;
		};

		stmmac_axi_setup: stmmac-axi-config {
			snps,wr_osr_lmt = <7>;
			snps,rd_osr_lmt = <7>;
			snps,blen = <16 0 0 0 0 0 0>;
		};

		gmac0: ethernet@37000000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac";
			reg = <0x37000000 0x200000>;
			interrupts = <GIC_SPI 220 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal = <1>;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE1_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE1_RESET>;
			reset-names = "stmmaceth";

			status = "disabled";
		};

		gmac1: ethernet@37200000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac";
			reg = <0x37200000 0x200000>;
			interrupts = <GIC_SPI 223 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal = <1>;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE2_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE2_RESET>;
			reset-names = "stmmaceth";

			status = "disabled";
		};

		gmac2: ethernet@37400000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac";
			reg = <0x37400000 0x200000>;
			interrupts = <GIC_SPI 226 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal = <1>;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE3_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE3_RESET>;
			reset-names = "stmmaceth";

			status = "disabled";
		};

		gmac3: ethernet@37600000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac";
			reg = <0x37600000 0x200000>;
			interrupts = <GIC_SPI 229 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal = <1>;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE4_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE4_RESET>;
			reset-names = "stmmaceth";

			status = "disabled";
		};

		/* Temporary fixed regulator */
		vsdcc_fixed: vsdcc-regulator {
			compatible = "regulator-fixed";
			regulator-name = "SDCC Power";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};

		sdcc1bam:dma@12402000 {
			compatible = "qcom,bam-v1.3.0";
			reg = <0x12402000 0x8000>;
			interrupts = <0 98 0>;
			clocks = <&gcc SDC1_H_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
                };

		sdcc3bam:dma@12182000 {
			compatible = "qcom,bam-v1.3.0";
			reg = <0x12182000 0x8000>;
			interrupts = <0 96 0>;
			clocks = <&gcc SDC3_H_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
		};

		amba {
			compatible = "arm,amba-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			sdcc1: sdcc@12400000 {
				status          = "disabled";
				compatible      = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				reg             = <0x12400000 0x2000>;
				interrupts      = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "cmd_irq";
				clocks          = <&gcc SDC1_CLK>, <&gcc SDC1_H_CLK>;
				clock-names     = "mclk", "apb_pclk";
				bus-width       = <8>;
				max-frequency   = <96000000>;
				non-removable;
				cap-sd-highspeed;
				cap-mmc-highspeed;
				vmmc-supply = <&vsdcc_fixed>;
				dmas = <&sdcc1bam 2>, <&sdcc1bam 1>;
				dma-names = "tx", "rx";
			};

			sdcc3: sdcc@12180000 {
				compatible      = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				status          = "disabled";
				reg             = <0x12180000 0x2000>;
				interrupts      = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "cmd_irq";
				clocks          = <&gcc SDC3_CLK>, <&gcc SDC3_H_CLK>;
				clock-names     = "mclk", "apb_pclk";
				bus-width       = <8>;
				cap-sd-highspeed;
				cap-mmc-highspeed;
				max-frequency   = <192000000>;
				#mmc-ddr-1_8v;
				sd-uhs-sdr104;
				sd-uhs-ddr50;
				vqmmc-supply = <&vsdcc_fixed>;
				dmas = <&sdcc3bam 2>, <&sdcc3bam 1>;
				dma-names = "tx", "rx";
			};
		};
	};

	sfpb_mutex: sfpb-mutex {
		compatible = "qcom,sfpb-mutex";
		syscon = <&sfpb_mutex_block 4 4>;

		#hwlock-cells = <1>;
	};

	smem {
		compatible = "qcom,smem";
		memory-region = <&smem>;
		hwlocks = <&sfpb_mutex 3>;
	};
};
