/dts-v1/;

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "buffalo,wcr-1166ds", "mediatek,mt7628an-soc";
	model = "Buffalo WCR-1166DS";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		aoss {
			label = "aoss";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		ap {
			label = "ap";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		reset {
			label = "reset";
			gpios = <&gpio1 14 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		router_o {
			label = "wcr-1166ds:orange:router";
			gpios = <&gpio1 5 GPIO_ACTIVE_LOW>;
		};

		router_g {
			label = "wcr-1166ds:green:router";
			gpios = <&gpio1 6 GPIO_ACTIVE_LOW>;
		};

		internet_o {
			label = "wcr-1166ds:orange:internet";
			gpios = <&gpio1 7 GPIO_ACTIVE_LOW>;
		};

		internet_g {
			label = "wcr-1166ds:green:internet";
			gpios = <&gpio1 8 GPIO_ACTIVE_LOW>;
		};

		wireless_o {
			label = "wcr-1166ds:orange:wireless";
			gpios = <&gpio1 9 GPIO_ACTIVE_LOW>;
		};

		wireless_g {
			label = "wcr-1166ds:green:wireless";
			gpios = <&gpio1 10 GPIO_ACTIVE_LOW>;
		};

		diag {
			label = "wcr-1166ds:orange:diag";
			gpios = <&gpio1 11 GPIO_ACTIVE_LOW>;
		};

		led_power: power {
			label = "wcr-1166ds:green:power";
			gpios = <&gpio1 12 GPIO_ACTIVE_LOW>;
		};
	};
};

&ehci {
	status = "disabled";
};

&esw {
	mediatek,portmap = <0x2f>;
	mediatek,portdisable = <0x27>;
};

&ohci {
	status = "disabled";
};

&pcie {
	status = "okay";
};

&pcie0 {
	mt76@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "uart1", "wled_an", "p0led_an", "p1led_an", "p2led_an", "p3led_an", "p4led_an", "wdt", "refclk", "gpio", "i2s";
			ralink,function = "gpio";
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;
		m25p,chunked-io = <32>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "firmware";
				reg = <0x50000 0x7c0000>;
			};

			partition@810000 {
				label = "firmware2";
				reg = <0x810000 0x7c0000>;
			};

			partition@fd0000 {
				label = "glbcfg";
				reg = <0xfd0000 0x10000>;
				read-only;
			};

			partition@fe0000 {
				label = "board_data";
				reg = <0xfe0000 0x10000>;
				read-only;
			};
		};
	};
};

&wmac {
	status = "okay";
};
