From 9807eb80a1b3bad7a4a89aa6566497bb1cadd6ef Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Fri, 3 Jun 2016 13:12:20 +0200
Subject: [PATCH] arch: mips: increase io_space_limit

this value comes from x86 and breaks some pci devices

Signed-off-by: John Crispin <john@phrozen.org>
---
 arch/mips/include/asm/mach-lantiq/spaces.h | 8 ++++++++
 1 file changed, 8 insertions(+)
 create mode 100644 arch/mips/include/asm/mach-lantiq/spaces.h

--- /dev/null
+++ b/arch/mips/include/asm/mach-lantiq/spaces.h
@@ -0,0 +1,8 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+#ifndef __ASM_MACH_LANTIQ_SPACES_H_
+#define __ASM_MACH_LANTIQ_SPACES_H_
+
+#define IO_SPACE_LIMIT  0xffffffff
+
+#include <asm/mach-generic/spaces.h>
+#endif
