From ba751e28d44255744a30190faad0ca09b455c44d Mon Sep 17 00:00:00 2001
From: DENG Qingfang <dqfext@gmail.com>
Date: Wed, 19 May 2021 11:32:00 +0800
Subject: [PATCH] net: dsa: mt7530: add interrupt support

Add support for MT7530 interrupt controller to handle internal PHYs.
In order to assign an IRQ number to each PHY, the registration of MDIO bus
is also done in this driver.

Signed-off-by: DENG Qingfang <dqfext@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Reviewed-by: Vladimir Oltean <olteanv@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/dsa/mt7530.c | 264 +++++++++++++++++++++++++++++++++++----
 drivers/net/dsa/mt7530.h |  20 ++-
 2 files changed, 256 insertions(+), 28 deletions(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -10,6 +10,7 @@
 #include <linux/mfd/syscon.h>
 #include <linux/module.h>
 #include <linux/netdevice.h>
+#include <linux/of_irq.h>
 #include <linux/of_mdio.h>
 #include <linux/of_net.h>
 #include <linux/of_platform.h>
@@ -603,18 +604,14 @@ mt7530_mib_reset(struct dsa_switch *ds)
 	mt7530_write(priv, MT7530_MIB_CCR, CCR_MIB_ACTIVATE);
 }
 
-static int mt7530_phy_read(struct dsa_switch *ds, int port, int regnum)
+static int mt7530_phy_read(struct mt7530_priv *priv, int port, int regnum)
 {
-	struct mt7530_priv *priv = ds->priv;
-
 	return mdiobus_read_nested(priv->bus, port, regnum);
 }
 
-static int mt7530_phy_write(struct dsa_switch *ds, int port, int regnum,
+static int mt7530_phy_write(struct mt7530_priv *priv, int port, int regnum,
 			    u16 val)
 {
-	struct mt7530_priv *priv = ds->priv;
-
 	return mdiobus_write_nested(priv->bus, port, regnum, val);
 }
 
@@ -792,9 +789,8 @@ out:
 }
 
 static int
-mt7531_ind_phy_read(struct dsa_switch *ds, int port, int regnum)
+mt7531_ind_phy_read(struct mt7530_priv *priv, int port, int regnum)
 {
-	struct mt7530_priv *priv = ds->priv;
 	int devad;
 	int ret;
 
@@ -810,10 +806,9 @@ mt7531_ind_phy_read(struct dsa_switch *d
 }
 
 static int
-mt7531_ind_phy_write(struct dsa_switch *ds, int port, int regnum,
+mt7531_ind_phy_write(struct mt7530_priv *priv, int port, int regnum,
 		     u16 data)
 {
-	struct mt7530_priv *priv = ds->priv;
 	int devad;
 	int ret;
 
@@ -829,6 +824,22 @@ mt7531_ind_phy_write(struct dsa_switch *
 	return ret;
 }
 
+static int
+mt753x_phy_read(struct mii_bus *bus, int port, int regnum)
+{
+	struct mt7530_priv *priv = bus->priv;
+
+	return priv->info->phy_read(priv, port, regnum);
+}
+
+static int
+mt753x_phy_write(struct mii_bus *bus, int port, int regnum, u16 val)
+{
+	struct mt7530_priv *priv = bus->priv;
+
+	return priv->info->phy_write(priv, port, regnum, val);
+}
+
 static void
 mt7530_get_strings(struct dsa_switch *ds, int port, u32 stringset,
 		   uint8_t *data)
@@ -1796,6 +1807,210 @@ mt7530_setup_gpio(struct mt7530_priv *pr
 	return devm_gpiochip_add_data(dev, gc, priv);
 }
 
+static irqreturn_t
+mt7530_irq_thread_fn(int irq, void *dev_id)
+{
+	struct mt7530_priv *priv = dev_id;
+	bool handled = false;
+	u32 val;
+	int p;
+
+	mutex_lock_nested(&priv->bus->mdio_lock, MDIO_MUTEX_NESTED);
+	val = mt7530_mii_read(priv, MT7530_SYS_INT_STS);
+	mt7530_mii_write(priv, MT7530_SYS_INT_STS, val);
+	mutex_unlock(&priv->bus->mdio_lock);
+
+	for (p = 0; p < MT7530_NUM_PHYS; p++) {
+		if (BIT(p) & val) {
+			unsigned int irq;
+
+			irq = irq_find_mapping(priv->irq_domain, p);
+			handle_nested_irq(irq);
+			handled = true;
+		}
+	}
+
+	return IRQ_RETVAL(handled);
+}
+
+static void
+mt7530_irq_mask(struct irq_data *d)
+{
+	struct mt7530_priv *priv = irq_data_get_irq_chip_data(d);
+
+	priv->irq_enable &= ~BIT(d->hwirq);
+}
+
+static void
+mt7530_irq_unmask(struct irq_data *d)
+{
+	struct mt7530_priv *priv = irq_data_get_irq_chip_data(d);
+
+	priv->irq_enable |= BIT(d->hwirq);
+}
+
+static void
+mt7530_irq_bus_lock(struct irq_data *d)
+{
+	struct mt7530_priv *priv = irq_data_get_irq_chip_data(d);
+
+	mutex_lock_nested(&priv->bus->mdio_lock, MDIO_MUTEX_NESTED);
+}
+
+static void
+mt7530_irq_bus_sync_unlock(struct irq_data *d)
+{
+	struct mt7530_priv *priv = irq_data_get_irq_chip_data(d);
+
+	mt7530_mii_write(priv, MT7530_SYS_INT_EN, priv->irq_enable);
+	mutex_unlock(&priv->bus->mdio_lock);
+}
+
+static struct irq_chip mt7530_irq_chip = {
+	.name = KBUILD_MODNAME,
+	.irq_mask = mt7530_irq_mask,
+	.irq_unmask = mt7530_irq_unmask,
+	.irq_bus_lock = mt7530_irq_bus_lock,
+	.irq_bus_sync_unlock = mt7530_irq_bus_sync_unlock,
+};
+
+static int
+mt7530_irq_map(struct irq_domain *domain, unsigned int irq,
+	       irq_hw_number_t hwirq)
+{
+	irq_set_chip_data(irq, domain->host_data);
+	irq_set_chip_and_handler(irq, &mt7530_irq_chip, handle_simple_irq);
+	irq_set_nested_thread(irq, true);
+	irq_set_noprobe(irq);
+
+	return 0;
+}
+
+static const struct irq_domain_ops mt7530_irq_domain_ops = {
+	.map = mt7530_irq_map,
+	.xlate = irq_domain_xlate_onecell,
+};
+
+static void
+mt7530_setup_mdio_irq(struct mt7530_priv *priv)
+{
+	struct dsa_switch *ds = priv->ds;
+	int p;
+
+	for (p = 0; p < MT7530_NUM_PHYS; p++) {
+		if (BIT(p) & ds->phys_mii_mask) {
+			unsigned int irq;
+
+			irq = irq_create_mapping(priv->irq_domain, p);
+			ds->slave_mii_bus->irq[p] = irq;
+		}
+	}
+}
+
+static int
+mt7530_setup_irq(struct mt7530_priv *priv)
+{
+	struct device *dev = priv->dev;
+	struct device_node *np = dev->of_node;
+	int ret;
+
+	if (!of_property_read_bool(np, "interrupt-controller")) {
+		dev_info(dev, "no interrupt support\n");
+		return 0;
+	}
+
+	priv->irq = of_irq_get(np, 0);
+	if (priv->irq <= 0) {
+		dev_err(dev, "failed to get parent IRQ: %d\n", priv->irq);
+		return priv->irq ? : -EINVAL;
+	}
+
+	priv->irq_domain = irq_domain_add_linear(np, MT7530_NUM_PHYS,
+						 &mt7530_irq_domain_ops, priv);
+	if (!priv->irq_domain) {
+		dev_err(dev, "failed to create IRQ domain\n");
+		return -ENOMEM;
+	}
+
+	/* This register must be set for MT7530 to properly fire interrupts */
+	if (priv->id != ID_MT7531)
+		mt7530_set(priv, MT7530_TOP_SIG_CTRL, TOP_SIG_CTRL_NORMAL);
+
+	ret = request_threaded_irq(priv->irq, NULL, mt7530_irq_thread_fn,
+				   IRQF_ONESHOT, KBUILD_MODNAME, priv);
+	if (ret) {
+		irq_domain_remove(priv->irq_domain);
+		dev_err(dev, "failed to request IRQ: %d\n", ret);
+		return ret;
+	}
+
+	return 0;
+}
+
+static void
+mt7530_free_mdio_irq(struct mt7530_priv *priv)
+{
+	int p;
+
+	for (p = 0; p < MT7530_NUM_PHYS; p++) {
+		if (BIT(p) & priv->ds->phys_mii_mask) {
+			unsigned int irq;
+
+			irq = irq_find_mapping(priv->irq_domain, p);
+			irq_dispose_mapping(irq);
+		}
+	}
+}
+
+static void
+mt7530_free_irq_common(struct mt7530_priv *priv)
+{
+	free_irq(priv->irq, priv);
+	irq_domain_remove(priv->irq_domain);
+}
+
+static void
+mt7530_free_irq(struct mt7530_priv *priv)
+{
+	mt7530_free_mdio_irq(priv);
+	mt7530_free_irq_common(priv);
+}
+
+static int
+mt7530_setup_mdio(struct mt7530_priv *priv)
+{
+	struct dsa_switch *ds = priv->ds;
+	struct device *dev = priv->dev;
+	struct mii_bus *bus;
+	static int idx;
+	int ret;
+
+	bus = devm_mdiobus_alloc(dev);
+	if (!bus)
+		return -ENOMEM;
+
+	ds->slave_mii_bus = bus;
+	bus->priv = priv;
+	bus->name = KBUILD_MODNAME "-mii";
+	snprintf(bus->id, MII_BUS_ID_SIZE, KBUILD_MODNAME "-%d", idx++);
+	bus->read = mt753x_phy_read;
+	bus->write = mt753x_phy_write;
+	bus->parent = dev;
+	bus->phy_mask = ~ds->phys_mii_mask;
+
+	if (priv->irq)
+		mt7530_setup_mdio_irq(priv);
+
+	ret = devm_mdiobus_register(dev, bus);
+	if (ret) {
+		dev_err(dev, "failed to register MDIO bus: %d\n", ret);
+		if (priv->irq)
+			mt7530_free_mdio_irq(priv);
+	}
+
+	return ret;
+}
+
 static int
 mt7530_setup(struct dsa_switch *ds)
 {
@@ -2747,24 +2962,20 @@ static int
 mt753x_setup(struct dsa_switch *ds)
 {
 	struct mt7530_priv *priv = ds->priv;
+	int ret = priv->info->sw_setup(ds);
 
-	return priv->info->sw_setup(ds);
-}
-
-static int
-mt753x_phy_read(struct dsa_switch *ds, int port, int regnum)
-{
-	struct mt7530_priv *priv = ds->priv;
+	if (ret)
+		return ret;
 
-	return priv->info->phy_read(ds, port, regnum);
-}
+	ret = mt7530_setup_irq(priv);
+	if (ret)
+		return ret;
 
-static int
-mt753x_phy_write(struct dsa_switch *ds, int port, int regnum, u16 val)
-{
-	struct mt7530_priv *priv = ds->priv;
+	ret = mt7530_setup_mdio(priv);
+	if (ret && priv->irq)
+		mt7530_free_irq_common(priv);
 
-	return priv->info->phy_write(ds, port, regnum, val);
+	return ret;
 }
 
 static int mt753x_get_mac_eee(struct dsa_switch *ds, int port,
@@ -2801,8 +3012,6 @@ static const struct dsa_switch_ops mt753
 	.get_tag_protocol	= mtk_get_tag_protocol,
 	.setup			= mt753x_setup,
 	.get_strings		= mt7530_get_strings,
-	.phy_read		= mt753x_phy_read,
-	.phy_write		= mt753x_phy_write,
 	.get_ethtool_stats	= mt7530_get_ethtool_stats,
 	.get_sset_count		= mt7530_get_sset_count,
 	.set_ageing_time	= mt7530_set_ageing_time,
@@ -2985,6 +3194,9 @@ mt7530_remove(struct mdio_device *mdiode
 		dev_err(priv->dev, "Failed to disable io pwr: %d\n",
 			ret);
 
+	if (priv->irq)
+		mt7530_free_irq(priv);
+
 	dsa_unregister_switch(priv->ds);
 	mutex_destroy(&priv->reg_mutex);
 }
--- a/drivers/net/dsa/mt7530.h
+++ b/drivers/net/dsa/mt7530.h
@@ -7,6 +7,7 @@
 #define __MT7530_H
 
 #define MT7530_NUM_PORTS		7
+#define MT7530_NUM_PHYS			5
 #define MT7530_CPU_PORT			6
 #define MT7530_NUM_FDB_RECORDS		2048
 #define MT7530_ALL_MEMBERS		0xff
@@ -392,6 +393,12 @@ enum mt7531_sgmii_force_duplex {
 #define  SYS_CTRL_SW_RST		BIT(1)
 #define  SYS_CTRL_REG_RST		BIT(0)
 
+/* Register for system interrupt */
+#define MT7530_SYS_INT_EN		0x7008
+
+/* Register for system interrupt status */
+#define MT7530_SYS_INT_STS		0x700c
+
 /* Register for PHY Indirect Access Control */
 #define MT7531_PHY_IAC			0x701C
 #define  MT7531_PHY_ACS_ST		BIT(31)
@@ -713,6 +720,8 @@ static const char *p5_intf_modes(unsigne
 	}
 }
 
+struct mt7530_priv;
+
 /* struct mt753x_info -	This is the main data structure for holding the specific
  *			part for each supported device
  * @sw_setup:		Holding the handler to a device initialization
@@ -737,8 +746,8 @@ struct mt753x_info {
 	enum mt753x_id id;
 
 	int (*sw_setup)(struct dsa_switch *ds);
-	int (*phy_read)(struct dsa_switch *ds, int port, int regnum);
-	int (*phy_write)(struct dsa_switch *ds, int port, int regnum, u16 val);
+	int (*phy_read)(struct mt7530_priv *priv, int port, int regnum);
+	int (*phy_write)(struct mt7530_priv *priv, int port, int regnum, u16 val);
 	int (*pad_setup)(struct dsa_switch *ds, phy_interface_t interface);
 	int (*cpu_port_config)(struct dsa_switch *ds, int port);
 	bool (*phy_mode_supported)(struct dsa_switch *ds, int port,
@@ -772,6 +781,10 @@ struct mt753x_info {
  *			registers
  * @p6_interface	Holding the current port 6 interface
  * @p5_intf_sel:	Holding the current port 5 interface select
+ *
+ * @irq:		IRQ number of the switch
+ * @irq_domain:		IRQ domain of the switch irq_chip
+ * @irq_enable:		IRQ enable bits, synced to SYS_INT_EN
  */
 struct mt7530_priv {
 	struct device		*dev;
@@ -793,6 +806,9 @@ struct mt7530_priv {
 	struct mt7530_port	ports[MT7530_NUM_PORTS];
 	/* protect among processes for registers access*/
 	struct mutex reg_mutex;
+	int irq;
+	struct irq_domain *irq_domain;
+	u32 irq_enable;
 };
 
 struct mt7530_hw_vlan_entry {
