From ded8f22945899f4e87dd6d952bbc4abce6e64b7e Mon Sep 17 00:00:00 2001
From: William Zhang <william.zhang@broadcom.com>
Date: Wed, 3 Aug 2022 10:54:50 -0700
Subject: [PATCH] arm64: dts: Move BCM4908 dts to bcmbca folder

As part of ARCH_BCM4908 to ARCH_BCMBCA migration, move the BCM4908 dts
files to bcmbca folder and use CONFIG_ARCH_BCMBCA to build all the
BCM4908 board dts. Delete bcm4908 folder and its makefile as well.

Signed-off-by: William Zhang <william.zhang@broadcom.com>
Link: https://lore.kernel.org/r/20220803175455.47638-5-william.zhang@broadcom.com
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm64/boot/dts/broadcom/Makefile                        | 1 -
 arch/arm64/boot/dts/broadcom/bcm4908/Makefile                | 5 -----
 arch/arm64/boot/dts/broadcom/bcmbca/Makefile                 | 4 ++++
 .../broadcom/{bcm4908 => bcmbca}/bcm4906-netgear-r8000p.dts  | 0
 .../{bcm4908 => bcmbca}/bcm4906-tplink-archer-c2300-v1.dts   | 0
 .../arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4906.dtsi | 0
 .../broadcom/{bcm4908 => bcmbca}/bcm4908-asus-gt-ac5300.dts  | 0
 .../broadcom/{bcm4908 => bcmbca}/bcm4908-netgear-raxe500.dts | 0
 .../arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4908.dtsi | 0
 9 files changed, 4 insertions(+), 6 deletions(-)
 delete mode 100644 arch/arm64/boot/dts/broadcom/bcm4908/Makefile
 rename arch/arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4906-netgear-r8000p.dts (100%)
 rename arch/arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4906-tplink-archer-c2300-v1.dts (100%)
 rename arch/arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4906.dtsi (100%)
 rename arch/arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4908-asus-gt-ac5300.dts (100%)
 rename arch/arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4908-netgear-raxe500.dts (100%)
 rename arch/arm64/boot/dts/broadcom/{bcm4908 => bcmbca}/bcm4908.dtsi (100%)

--- a/arch/arm64/boot/dts/broadcom/Makefile
+++ b/arch/arm64/boot/dts/broadcom/Makefile
@@ -6,7 +6,6 @@ dtb-$(CONFIG_ARCH_BCM2835) += bcm2711-rp
 			      bcm2837-rpi-3-b-plus.dtb \
 			      bcm2837-rpi-cm3-io3.dtb
 
-subdir-y	+= bcm4908
 subdir-y	+= bcmbca
 subdir-y	+= northstar2
 subdir-y	+= stingray
--- a/arch/arm64/boot/dts/broadcom/bcm4908/Makefile
+++ /dev/null
@@ -1,5 +0,0 @@
-# SPDX-License-Identifier: GPL-2.0
-dtb-$(CONFIG_ARCH_BCM4908) += bcm4906-netgear-r8000p.dtb
-dtb-$(CONFIG_ARCH_BCM4908) += bcm4906-tplink-archer-c2300-v1.dtb
-dtb-$(CONFIG_ARCH_BCM4908) += bcm4908-asus-gt-ac5300.dtb
-dtb-$(CONFIG_ARCH_BCM4908) += bcm4908-netgear-raxe500.dtb
--- a/arch/arm64/boot/dts/broadcom/bcmbca/Makefile
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/Makefile
@@ -1,5 +1,9 @@
 # SPDX-License-Identifier: GPL-2.0
 dtb-$(CONFIG_ARCH_BCMBCA) += \
+				bcm4906-netgear-r8000p.dtb \
+				bcm4906-tplink-archer-c2300-v1.dtb \
+				bcm4908-asus-gt-ac5300.dtb \
+				bcm4908-netgear-raxe500.dtb \
 				bcm4912-asus-gt-ax6000.dtb \
 				bcm94912.dtb \
 				bcm963158.dtb \
--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4906-netgear-r8000p.dts
+++ /dev/null
@@ -1,157 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
-
-#include <dt-bindings/gpio/gpio.h>
-#include <dt-bindings/input/input.h>
-#include <dt-bindings/leds/common.h>
-
-#include "bcm4906.dtsi"
-
-/ {
-	compatible = "netgear,r8000p", "brcm,bcm4906", "brcm,bcm4908", "brcm,bcmbca";
-	model = "Netgear R8000P";
-
-	memory@0 {
-		device_type = "memory";
-		reg = <0x00 0x00 0x00 0x20000000>;
-	};
-
-	leds {
-		compatible = "gpio-leds";
-
-		led-power-white {
-			function = LED_FUNCTION_POWER;
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
-		};
-
-		led-power-amber {
-			function = LED_FUNCTION_POWER;
-			color = <LED_COLOR_ID_AMBER>;
-			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
-		};
-
-		led-wps {
-			function = LED_FUNCTION_WPS;
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
-		};
-
-		led-2ghz {
-			function = "2ghz";
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
-		};
-
-		led-5ghz-1 {
-			function = "5ghz-1";
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 15 GPIO_ACTIVE_LOW>;
-		};
-
-		led-5ghz-2 {
-			function = "5ghz-2";
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 16 GPIO_ACTIVE_LOW>;
-		};
-
-		led-usb2 {
-			function = "usb2";
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 17 GPIO_ACTIVE_LOW>;
-		};
-
-		led-usb3 {
-			function = "usb3";
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
-		};
-
-		led-wifi {
-			function = "wifi";
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 56 GPIO_ACTIVE_LOW>;
-		};
-	};
-};
-
-&enet {
-	nvmem-cells = <&base_mac_addr>;
-	nvmem-cell-names = "mac-address";
-};
-
-&usb_phy {
-	brcm,ioc = <1>;
-	status = "okay";
-};
-
-&ehci {
-	status = "okay";
-};
-
-&ohci {
-	status = "okay";
-};
-
-&xhci {
-	status = "okay";
-};
-
-&ports {
-	port@0 {
-		label = "lan4";
-	};
-
-	port@1 {
-		label = "lan3";
-	};
-
-	port@2 {
-		label = "lan2";
-	};
-
-	port@3 {
-		label = "lan1";
-	};
-
-	port@7 {
-		reg = <7>;
-		phy-mode = "internal";
-		phy-handle = <&phy12>;
-		label = "wan";
-	};
-};
-
-&nandcs {
-	nand-ecc-strength = <4>;
-	nand-ecc-step-size = <512>;
-	nand-on-flash-bbt;
-
-	#address-cells = <1>;
-	#size-cells = <0>;
-
-	partitions {
-		compatible = "fixed-partitions";
-		#address-cells = <1>;
-		#size-cells = <1>;
-
-		partition@0 {
-			compatible = "nvmem-cells";
-			label = "cferom";
-			reg = <0x0 0x100000>;
-
-			#address-cells = <1>;
-			#size-cells = <1>;
-			ranges = <0 0x0 0x100000>;
-
-			base_mac_addr: mac@106a0 {
-				reg = <0x106a0 0x6>;
-			};
-		};
-
-		partition@100000 {
-			compatible = "brcm,bcm4908-firmware";
-			label = "firmware";
-			reg = <0x100000 0x4400000>;
-		};
-	};
-};
--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4906-tplink-archer-c2300-v1.dts
+++ /dev/null
@@ -1,182 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
-
-#include <dt-bindings/gpio/gpio.h>
-#include <dt-bindings/input/input.h>
-#include <dt-bindings/leds/common.h>
-
-#include "bcm4906.dtsi"
-
-/ {
-	compatible = "tplink,archer-c2300-v1", "brcm,bcm4906", "brcm,bcm4908", "brcm,bcmbca";
-	model = "TP-Link Archer C2300 V1";
-
-	memory@0 {
-		device_type = "memory";
-		reg = <0x00 0x00 0x00 0x20000000>;
-	};
-
-	leds {
-		compatible = "gpio-leds";
-
-		led-power {
-			function = LED_FUNCTION_POWER;
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
-		};
-
-		led-2ghz {
-			function = "2ghz";
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
-		};
-
-		led-5ghz {
-			function = "5ghz";
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 3 GPIO_ACTIVE_LOW>;
-		};
-
-		led-wan-amber {
-			function = LED_FUNCTION_WAN;
-			color = <LED_COLOR_ID_AMBER>;
-			gpios = <&gpio0 4 GPIO_ACTIVE_HIGH>;
-		};
-
-		led-wan-blue {
-			function = LED_FUNCTION_WAN;
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
-		};
-
-		led-lan {
-			function = LED_FUNCTION_LAN;
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
-		};
-
-		led-wps {
-			function = LED_FUNCTION_WPS;
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
-		};
-
-		led-usb2 {
-			function = "usb2";
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 15 GPIO_ACTIVE_LOW>;
-		};
-
-		led-usb3 {
-			function = "usbd3";
-			color = <LED_COLOR_ID_BLUE>;
-			gpios = <&gpio0 17 GPIO_ACTIVE_LOW>;
-		};
-
-		led-brightness {
-			function = LED_FUNCTION_BACKLIGHT;
-			color = <LED_COLOR_ID_WHITE>;
-			gpios = <&gpio0 19 GPIO_ACTIVE_LOW>;
-		};
-	};
-
-	gpio-keys-polled {
-		compatible = "gpio-keys-polled";
-		poll-interval = <100>;
-
-		key-brightness {
-			label = "LEDs";
-			linux,code = <KEY_BRIGHTNESS_ZERO>;
-			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
-		};
-
-		key-wps {
-			label = "WPS";
-			linux,code = <KEY_WPS_BUTTON>;
-			gpios = <&gpio0 21 GPIO_ACTIVE_LOW>;
-		};
-
-		key-wifi {
-			label = "WiFi";
-			linux,code = <KEY_RFKILL>;
-			gpios = <&gpio0 22 GPIO_ACTIVE_LOW>;
-		};
-
-		key-restart {
-			label = "Reset";
-			linux,code = <KEY_RESTART>;
-			gpios = <&gpio0 23 GPIO_ACTIVE_LOW>;
-		};
-	};
-};
-
-&usb_phy {
-	brcm,ioc = <1>;
-	status = "okay";
-};
-
-&ehci {
-	status = "okay";
-};
-
-&ohci {
-	status = "okay";
-};
-
-&xhci {
-	status = "okay";
-};
-
-&ports {
-	port@0 {
-		label = "lan4";
-	};
-
-	port@1 {
-		label = "lan3";
-	};
-
-	port@2 {
-		label = "lan2";
-	};
-
-	port@3 {
-		label = "lan1";
-	};
-
-	port@7 {
-		reg = <7>;
-		phy-mode = "internal";
-		phy-handle = <&phy12>;
-		label = "wan";
-	};
-};
-
-&nandcs {
-	nand-ecc-strength = <4>;
-	nand-ecc-step-size = <512>;
-	nand-on-flash-bbt;
-
-	#address-cells = <1>;
-	#size-cells = <0>;
-
-	partitions {
-		compatible = "brcm,bcm4908-partitions";
-		#address-cells = <1>;
-		#size-cells = <1>;
-
-		partition@0 {
-			label = "cferom";
-			reg = <0x0 0x100000>;
-		};
-
-		partition@100000 {
-			compatible = "brcm,bcm4908-firmware";
-			reg = <0x100000 0x3900000>;
-		};
-
-		partition@5800000 {
-			compatible = "brcm,bcm4908-firmware";
-			reg = <0x3a00000 0x3900000>;
-		};
-	};
-};
--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4906.dtsi
+++ /dev/null
@@ -1,34 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
-
-#include "bcm4908.dtsi"
-
-/ {
-	cpus {
-		/delete-node/ cpu@2;
-
-		/delete-node/ cpu@3;
-	};
-
-	timer {
-		compatible = "arm,armv8-timer";
-		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>;
-	};
-
-	timer {
-		compatible = "arm,armv8-timer";
-		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>;
-	};
-
-	pmu {
-		compatible = "arm,cortex-a53-pmu";
-		interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>,
-			     <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
-		interrupt-affinity = <&cpu0>, <&cpu1>;
-	};
-};
--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908-asus-gt-ac5300.dts
+++ /dev/null
@@ -1,207 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
-
-#include <dt-bindings/gpio/gpio.h>
-#include <dt-bindings/input/input.h>
-#include <dt-bindings/leds/common.h>
-
-#include "bcm4908.dtsi"
-
-/ {
-	compatible = "asus,gt-ac5300", "brcm,bcm4908", "brcm,bcmbca";
-	model = "Asus GT-AC5300";
-
-	memory@0 {
-		device_type = "memory";
-		reg = <0x00 0x00 0x00 0x40000000>;
-	};
-
-	gpio-keys-polled {
-		compatible = "gpio-keys-polled";
-		poll-interval = <100>;
-
-		key-wifi {
-			label = "WiFi";
-			linux,code = <KEY_RFKILL>;
-			gpios = <&gpio0 28 GPIO_ACTIVE_LOW>;
-		};
-
-		key-wps {
-			label = "WPS";
-			linux,code = <KEY_WPS_BUTTON>;
-			gpios = <&gpio0 29 GPIO_ACTIVE_LOW>;
-		};
-
-		key-restart {
-			label = "Reset";
-			linux,code = <KEY_RESTART>;
-			gpios = <&gpio0 30 GPIO_ACTIVE_LOW>;
-		};
-
-		key-brightness {
-			label = "LEDs";
-			linux,code = <KEY_BRIGHTNESS_ZERO>;
-			gpios = <&gpio0 31 GPIO_ACTIVE_LOW>;
-		};
-	};
-};
-
-&enet {
-	nvmem-cells = <&base_mac_addr>;
-	nvmem-cell-names = "mac-address";
-};
-
-&usb_phy {
-	brcm,ioc = <1>;
-	status = "okay";
-};
-
-&ehci {
-	status = "okay";
-};
-
-&ohci {
-	status = "okay";
-};
-
-&xhci {
-	status = "okay";
-};
-
-&ports {
-	port@0 {
-		label = "lan2";
-	};
-
-	port@1 {
-		label = "lan1";
-	};
-
-	port@2 {
-		label = "lan6";
-	};
-
-	port@3 {
-		label = "lan5";
-	};
-
-	/* External BCM53134S switch */
-	port@7 {
-		label = "sw";
-		reg = <7>;
-		phy-mode = "rgmii";
-
-		fixed-link {
-			speed = <1000>;
-			full-duplex;
-		};
-	};
-};
-
-&mdio {
-	/* lan8 */
-	ethernet-phy@0 {
-		reg = <0>;
-	};
-
-	/* lan7 */
-	ethernet-phy@1 {
-		reg = <1>;
-	};
-
-	/* lan4 */
-	ethernet-phy@2 {
-		reg = <2>;
-	};
-
-	/* lan3 */
-	ethernet-phy@3 {
-		reg = <3>;
-	};
-};
-
-&leds {
-	led-power@11 {
-		reg = <0x11>;
-		function = LED_FUNCTION_POWER;
-		color = <LED_COLOR_ID_WHITE>;
-		default-state = "on";
-		active-low;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pins_led_17_a>;
-	};
-
-	led-wan-red@12 {
-		reg = <0x12>;
-		function = LED_FUNCTION_WAN;
-		color = <LED_COLOR_ID_RED>;
-		active-low;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pins_led_18_a>;
-	};
-
-	led-wps@14 {
-		reg = <0x14>;
-		function = LED_FUNCTION_WPS;
-		color = <LED_COLOR_ID_WHITE>;
-		active-low;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pins_led_20_a>;
-	};
-
-	led-wan-white@15 {
-		reg = <0x15>;
-		function = LED_FUNCTION_WAN;
-		color = <LED_COLOR_ID_WHITE>;
-		active-low;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pins_led_21_a>;
-	};
-
-	led-lan@19 {
-		reg = <0x19>;
-		function = LED_FUNCTION_LAN;
-		color = <LED_COLOR_ID_WHITE>;
-		pinctrl-names = "default";
-		pinctrl-0 = <&pins_led_25_a>;
-	};
-};
-
-&nandcs {
-	nand-ecc-strength = <4>;
-	nand-ecc-step-size = <512>;
-	nand-on-flash-bbt;
-	brcm,nand-has-wp;
-
-	#address-cells = <1>;
-	#size-cells = <0>;
-
-	partitions {
-		compatible = "brcm,bcm4908-partitions";
-		#address-cells = <1>;
-		#size-cells = <1>;
-
-		partition@0 {
-			compatible = "nvmem-cells";
-			label = "cferom";
-			reg = <0x0 0x100000>;
-
-			#address-cells = <1>;
-			#size-cells = <1>;
-			ranges = <0 0x0 0x100000>;
-
-			base_mac_addr: mac@106a0 {
-				reg = <0x106a0 0x6>;
-			};
-		};
-
-		partition@100000 {
-			compatible = "brcm,bcm4908-firmware";
-			reg = <0x100000 0x5700000>;
-		};
-
-		partition@5800000 {
-			compatible = "brcm,bcm4908-firmware";
-			reg = <0x5800000 0x5700000>;
-		};
-	};
-};
--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908-netgear-raxe500.dts
+++ /dev/null
@@ -1,50 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
-
-#include "bcm4908.dtsi"
-
-/ {
-	compatible = "netgear,raxe500", "brcm,bcm4908", "brcm,bcmbca";
-	model = "Netgear RAXE500";
-
-	memory@0 {
-		device_type = "memory";
-		reg = <0x00 0x00 0x00 0x40000000>;
-	};
-};
-
-&ehci {
-	status = "okay";
-};
-
-&ohci {
-	status = "okay";
-};
-
-&xhci {
-	status = "okay";
-};
-
-&ports {
-	port@0 {
-		label = "lan4";
-	};
-
-	port@1 {
-		label = "lan3";
-	};
-
-	port@2 {
-		label = "lan2";
-	};
-
-	port@3 {
-		label = "lan1";
-	};
-
-	port@7 {
-		reg = <7>;
-		phy-mode = "internal";
-		phy-handle = <&phy12>;
-		label = "wan";
-	};
-};
--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi
+++ /dev/null
@@ -1,575 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
-
-#include <dt-bindings/interrupt-controller/irq.h>
-#include <dt-bindings/interrupt-controller/arm-gic.h>
-#include <dt-bindings/phy/phy.h>
-#include <dt-bindings/soc/bcm-pmb.h>
-
-/dts-v1/;
-
-/ {
-	interrupt-parent = <&gic>;
-
-	#address-cells = <2>;
-	#size-cells = <2>;
-
-	aliases {
-		serial0 = &uart0;
-	};
-
-	chosen {
-		stdout-path = "serial0:115200n8";
-	};
-
-	cpus {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
-		cpu0: cpu@0 {
-			device_type = "cpu";
-			compatible = "brcm,brahma-b53";
-			reg = <0x0>;
-			enable-method = "spin-table";
-			cpu-release-addr = <0x0 0xfff8>;
-			next-level-cache = <&l2>;
-		};
-
-		cpu1: cpu@1 {
-			device_type = "cpu";
-			compatible = "brcm,brahma-b53";
-			reg = <0x1>;
-			enable-method = "spin-table";
-			cpu-release-addr = <0x0 0xfff8>;
-			next-level-cache = <&l2>;
-		};
-
-		cpu2: cpu@2 {
-			device_type = "cpu";
-			compatible = "brcm,brahma-b53";
-			reg = <0x2>;
-			enable-method = "spin-table";
-			cpu-release-addr = <0x0 0xfff8>;
-			next-level-cache = <&l2>;
-		};
-
-		cpu3: cpu@3 {
-			device_type = "cpu";
-			compatible = "brcm,brahma-b53";
-			reg = <0x3>;
-			enable-method = "spin-table";
-			cpu-release-addr = <0x0 0xfff8>;
-			next-level-cache = <&l2>;
-		};
-
-		l2: l2-cache0 {
-			compatible = "cache";
-		};
-	};
-
-	axi@81000000 {
-		compatible = "simple-bus";
-		#address-cells = <1>;
-		#size-cells = <1>;
-		ranges = <0x00 0x00 0x81000000 0x4000>;
-
-		gic: interrupt-controller@1000 {
-			compatible = "arm,gic-400";
-			#interrupt-cells = <3>;
-			#address-cells = <0>;
-			interrupt-controller;
-			reg = <0x1000 0x1000>,
-			      <0x2000 0x2000>;
-		};
-	};
-
-	timer {
-		compatible = "arm,armv8-timer";
-		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
-			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
-	};
-
-	pmu {
-		compatible = "arm,cortex-a53-pmu";
-		interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>,
-			     <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>,
-			     <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>,
-			     <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
-		interrupt-affinity = <&cpu0>, <&cpu1>, <&cpu2>, <&cpu3>;
-	};
-
-	clocks {
-		periph_clk: periph_clk {
-			compatible = "fixed-clock";
-			#clock-cells = <0>;
-			clock-frequency = <50000000>;
-			clock-output-names = "periph";
-		};
-	};
-
-	soc {
-		compatible = "simple-bus";
-		#address-cells = <1>;
-		#size-cells = <1>;
-		ranges = <0x00 0x00 0x80000000 0x281000>;
-
-		enet: ethernet@2000 {
-			compatible = "brcm,bcm4908-enet";
-			reg = <0x2000 0x1000>;
-
-			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>,
-				     <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "rx", "tx";
-		};
-
-		usb_phy: usb-phy@c200 {
-			compatible = "brcm,bcm4908-usb-phy";
-			reg = <0xc200 0x100>;
-			reg-names = "ctrl";
-			power-domains = <&pmb BCM_PMB_HOST_USB>;
-			dr_mode = "host";
-			brcm,has-xhci;
-			brcm,has-eohci;
-			#phy-cells = <1>;
-			status = "disabled";
-		};
-
-		ehci: usb@c300 {
-			compatible = "generic-ehci";
-			reg = <0xc300 0x100>;
-			interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
-			phys = <&usb_phy PHY_TYPE_USB2>;
-			status = "disabled";
-		};
-
-		ohci: usb@c400 {
-			compatible = "generic-ohci";
-			reg = <0xc400 0x100>;
-			interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
-			phys = <&usb_phy PHY_TYPE_USB2>;
-			status = "disabled";
-		};
-
-		xhci: usb@d000 {
-			compatible = "generic-xhci";
-			reg = <0xd000 0x8c8>;
-			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
-			phys = <&usb_phy PHY_TYPE_USB3>;
-			status = "disabled";
-		};
-
-		bus@80000 {
-			compatible = "simple-bus";
-			#size-cells = <1>;
-			#address-cells = <1>;
-			ranges = <0 0x80000 0x50000>;
-
-			ethernet-switch@0 {
-				compatible = "brcm,bcm4908-switch";
-				reg = <0x0 0x40000>,
-				      <0x40000 0x110>,
-				      <0x40340 0x30>,
-				      <0x40380 0x30>,
-				      <0x40600 0x34>,
-				      <0x40800 0x208>;
-				reg-names = "core", "reg", "intrl2_0",
-					    "intrl2_1", "fcb", "acb";
-				interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>,
-					     <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>;
-				brcm,num-gphy = <5>;
-				brcm,num-rgmii-ports = <2>;
-
-				#address-cells = <1>;
-				#size-cells = <0>;
-
-				ports: ports {
-					#address-cells = <1>;
-					#size-cells = <0>;
-
-					port@0 {
-						reg = <0>;
-						phy-mode = "internal";
-						phy-handle = <&phy8>;
-					};
-
-					port@1 {
-						reg = <1>;
-						phy-mode = "internal";
-						phy-handle = <&phy9>;
-					};
-
-					port@2 {
-						reg = <2>;
-						phy-mode = "internal";
-						phy-handle = <&phy10>;
-					};
-
-					port@3 {
-						reg = <3>;
-						phy-mode = "internal";
-						phy-handle = <&phy11>;
-					};
-
-					port@8 {
-						reg = <8>;
-						phy-mode = "internal";
-						ethernet = <&enet>;
-
-						fixed-link {
-							speed = <1000>;
-							full-duplex;
-						};
-					};
-				};
-			};
-
-			mdio: mdio@405c0 {
-				compatible = "brcm,unimac-mdio";
-				reg = <0x405c0 0x8>;
-				reg-names = "mdio";
-				#size-cells = <0>;
-				#address-cells = <1>;
-
-				phy8: ethernet-phy@8 {
-					reg = <8>;
-				};
-
-				phy9: ethernet-phy@9 {
-					reg = <9>;
-				};
-
-				phy10: ethernet-phy@a {
-					reg = <10>;
-				};
-
-				phy11: ethernet-phy@b {
-					reg = <11>;
-				};
-
-				phy12: ethernet-phy@c {
-					reg = <12>;
-				};
-			};
-		};
-
-		procmon: syscon@280000 {
-			compatible = "simple-bus";
-			reg = <0x280000 0x1000>;
-			ranges;
-
-			#address-cells = <1>;
-			#size-cells = <1>;
-
-			pmb: power-controller@2800c0 {
-				compatible = "brcm,bcm4908-pmb";
-				reg = <0x2800c0 0x40>;
-				#power-domain-cells = <1>;
-			};
-		};
-	};
-
-	bus@ff800000 {
-		compatible = "simple-bus";
-		#address-cells = <1>;
-		#size-cells = <1>;
-		ranges = <0x00 0x00 0xff800000 0x3000>;
-
-		twd: timer-mfd@400 {
-			compatible = "brcm,bcm4908-twd", "simple-mfd", "syscon";
-			reg = <0x400 0x4c>;
-			ranges = <0x0 0x400 0x4c>;
-
-			#address-cells = <1>;
-			#size-cells = <1>;
-
-			watchdog@28 {
-				compatible = "brcm,bcm6345-wdt";
-				reg = <0x28 0x8>;
-			};
-		};
-
-		gpio0: gpio-controller@500 {
-			compatible = "brcm,bcm6345-gpio";
-			reg-names = "dirout", "dat";
-			reg = <0x500 0x28>, <0x528 0x28>;
-
-			#gpio-cells = <2>;
-			gpio-controller;
-		};
-
-		pinctrl@560 {
-			compatible = "brcm,bcm4908-pinctrl";
-			reg = <0x560 0x10>;
-
-			pins_led_0_a: led_0-a-pins {
-				function = "led_0";
-				groups = "led_0_grp_a";
-			};
-
-			pins_led_1_a: led_1-a-pins {
-				function = "led_1";
-				groups = "led_1_grp_a";
-			};
-
-			pins_led_2_a: led_2-a-pins {
-				function = "led_2";
-				groups = "led_2_grp_a";
-			};
-
-			pins_led_3_a: led_3-a-pins {
-				function = "led_3";
-				groups = "led_3_grp_a";
-			};
-
-			pins_led_4_a: led_4-a-pins {
-				function = "led_4";
-				groups = "led_4_grp_a";
-			};
-
-			pins_led_5_a: led_5-a-pins {
-				function = "led_5";
-				groups = "led_5_grp_a";
-			};
-
-			pins_led_6_a: led_6-a-pins {
-				function = "led_6";
-				groups = "led_6_grp_a";
-			};
-
-			pins_led_7_a: led_7-a-pins {
-				function = "led_7";
-				groups = "led_7_grp_a";
-			};
-
-			pins_led_8_a: led_8-a-pins {
-				function = "led_8";
-				groups = "led_8_grp_a";
-			};
-
-			pins_led_9_a: led_9-a-pins {
-				function = "led_9";
-				groups = "led_9_grp_a";
-			};
-
-			pins_led_10_a: led_10-a-pins {
-				function = "led_10";
-				groups = "led_10_grp_a";
-			};
-
-			pins_led_11_a: led_11-a-pins {
-				function = "led_11";
-				groups = "led_11_grp_a";
-			};
-
-			pins_led_12_a: led_12-a-pins {
-				function = "led_12";
-				groups = "led_12_grp_a";
-			};
-
-			pins_led_13_a: led_13-a-pins {
-				function = "led_13";
-				groups = "led_13_grp_a";
-			};
-
-			pins_led_14_a: led_14-a-pins {
-				function = "led_14";
-				groups = "led_14_grp_a";
-			};
-
-			pins_led_15_a: led_15-a-pins {
-				function = "led_15";
-				groups = "led_15_grp_a";
-			};
-
-			pins_led_16_a: led_16-a-pins {
-				function = "led_16";
-				groups = "led_16_grp_a";
-			};
-
-			pins_led_17_a: led_17-a-pins {
-				function = "led_17";
-				groups = "led_17_grp_a";
-			};
-
-			pins_led_18_a: led_18-a-pins {
-				function = "led_18";
-				groups = "led_18_grp_a";
-			};
-
-			pins_led_19_a: led_19-a-pins {
-				function = "led_19";
-				groups = "led_19_grp_a";
-			};
-
-			pins_led_20_a: led_20-a-pins {
-				function = "led_20";
-				groups = "led_20_grp_a";
-			};
-
-			pins_led_21_a: led_21-a-pins {
-				function = "led_21";
-				groups = "led_21_grp_a";
-			};
-
-			pins_led_22_a: led_22-a-pins {
-				function = "led_22";
-				groups = "led_22_grp_a";
-			};
-
-			pins_led_23_a: led_23-a-pins {
-				function = "led_23";
-				groups = "led_23_grp_a";
-			};
-
-			pins_led_24_a: led_24-a-pins {
-				function = "led_24";
-				groups = "led_24_grp_a";
-			};
-
-			pins_led_25_a: led_25-a-pins {
-				function = "led_25";
-				groups = "led_25_grp_a";
-			};
-
-			pins_led_26_a: led_26-a-pins {
-				function = "led_26";
-				groups = "led_26_grp_a";
-			};
-
-			pins_led_27_a: led_27-a-pins {
-				function = "led_27";
-				groups = "led_27_grp_a";
-			};
-
-			pins_led_28_a: led_28-a-pins {
-				function = "led_28";
-				groups = "led_28_grp_a";
-			};
-
-			pins_led_29_a: led_29-a-pins {
-				function = "led_29";
-				groups = "led_29_grp_a";
-			};
-
-			pins_led_30_a: led_30-a-pins {
-				function = "led_30";
-				groups = "led_30_grp_a";
-			};
-
-			pins_led_31_a: led_31-a-pins {
-				function = "led_31";
-				groups = "led_31_grp_a";
-			};
-
-			pins_hs_uart: hs_uart-pins {
-				function = "hs_uart";
-				groups = "hs_uart_grp";
-			};
-
-			pins_i2c_a: i2c-a-pins {
-				function = "i2c";
-				groups = "i2c_grp_a";
-			};
-
-			pins_i2c_b: i2c-b-pins {
-				function = "i2c";
-				groups = "i2c_grp_b";
-			};
-
-			pins_i2s: i2s-pins {
-				function = "i2s";
-				groups = "i2s_grp";
-			};
-
-			pins_nand_ctrl: nand_ctrl-pins {
-				function = "nand_ctrl";
-				groups = "nand_ctrl_grp";
-			};
-
-			pins_nand_data: nand_data-pins {
-				function = "nand_data";
-				groups = "nand_data_grp";
-			};
-
-			pins_emmc_ctrl: emmc_ctrl-pins {
-				function = "emmc_ctrl";
-				groups = "emmc_ctrl_grp";
-			};
-
-			pins_usb0_pwr: usb0_pwr-pins {
-				function = "usb0_pwr";
-				groups = "usb0_pwr_grp";
-			};
-
-			pins_usb1_pwr: usb1_pwr-pins {
-				function = "usb1_pwr";
-				groups = "usb1_pwr_grp";
-			};
-		};
-
-		uart0: serial@640 {
-			compatible = "brcm,bcm6345-uart";
-			reg = <0x640 0x18>;
-			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&periph_clk>;
-			clock-names = "refclk";
-			status = "okay";
-		};
-
-		leds: leds@800 {
-			compatible = "brcm,bcm4908-leds", "brcm,bcm63138-leds";
-			reg = <0x800 0xdc>;
-
-			#address-cells = <1>;
-			#size-cells = <0>;
-		};
-
-		nand-controller@1800 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "brcm,nand-bcm63138", "brcm,brcmnand-v7.1", "brcm,brcmnand";
-			reg = <0x1800 0x600>, <0x2000 0x10>;
-			reg-names = "nand", "nand-int-base";
-			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "nand";
-			status = "okay";
-
-			nandcs: nand@0 {
-				compatible = "brcm,nandcs";
-				reg = <0>;
-			};
-		};
-
-		i2c@2100 {
-			compatible = "brcm,brcmper-i2c";
-			reg = <0x2100 0x58>;
-			clock-frequency = <97500>;
-			pinctrl-names = "default";
-			pinctrl-0 = <&pins_i2c_a>;
-			status = "disabled";
-		};
-
-		misc@2600 {
-			compatible = "brcm,misc", "simple-mfd";
-			reg = <0x2600 0xe4>;
-
-			#address-cells = <1>;
-			#size-cells = <1>;
-			ranges = <0x00 0x2600 0xe4>;
-
-			reset-controller@2644 {
-				compatible = "brcm,bcm4908-misc-pcie-reset";
-				reg = <0x44 0x04>;
-				#reset-cells = <1>;
-			};
-		};
-	};
-
-	reboot {
-		compatible = "syscon-reboot";
-		regmap = <&twd>;
-		offset = <0x34>;
-		mask = <1>;
-	};
-};
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4906-netgear-r8000p.dts
@@ -0,0 +1,157 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/leds/common.h>
+
+#include "bcm4906.dtsi"
+
+/ {
+	compatible = "netgear,r8000p", "brcm,bcm4906", "brcm,bcm4908", "brcm,bcmbca";
+	model = "Netgear R8000P";
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x00 0x00 0x00 0x20000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led-power-white {
+			function = LED_FUNCTION_POWER;
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
+		};
+
+		led-power-amber {
+			function = LED_FUNCTION_POWER;
+			color = <LED_COLOR_ID_AMBER>;
+			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
+		};
+
+		led-wps {
+			function = LED_FUNCTION_WPS;
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
+		};
+
+		led-2ghz {
+			function = "2ghz";
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
+		};
+
+		led-5ghz-1 {
+			function = "5ghz-1";
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 15 GPIO_ACTIVE_LOW>;
+		};
+
+		led-5ghz-2 {
+			function = "5ghz-2";
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 16 GPIO_ACTIVE_LOW>;
+		};
+
+		led-usb2 {
+			function = "usb2";
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 17 GPIO_ACTIVE_LOW>;
+		};
+
+		led-usb3 {
+			function = "usb3";
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
+		};
+
+		led-wifi {
+			function = "wifi";
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 56 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&enet {
+	nvmem-cells = <&base_mac_addr>;
+	nvmem-cell-names = "mac-address";
+};
+
+&usb_phy {
+	brcm,ioc = <1>;
+	status = "okay";
+};
+
+&ehci {
+	status = "okay";
+};
+
+&ohci {
+	status = "okay";
+};
+
+&xhci {
+	status = "okay";
+};
+
+&ports {
+	port@0 {
+		label = "lan4";
+	};
+
+	port@1 {
+		label = "lan3";
+	};
+
+	port@2 {
+		label = "lan2";
+	};
+
+	port@3 {
+		label = "lan1";
+	};
+
+	port@7 {
+		reg = <7>;
+		phy-mode = "internal";
+		phy-handle = <&phy12>;
+		label = "wan";
+	};
+};
+
+&nandcs {
+	nand-ecc-strength = <4>;
+	nand-ecc-step-size = <512>;
+	nand-on-flash-bbt;
+
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	partitions {
+		compatible = "fixed-partitions";
+		#address-cells = <1>;
+		#size-cells = <1>;
+
+		partition@0 {
+			compatible = "nvmem-cells";
+			label = "cferom";
+			reg = <0x0 0x100000>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0 0x0 0x100000>;
+
+			base_mac_addr: mac@106a0 {
+				reg = <0x106a0 0x6>;
+			};
+		};
+
+		partition@100000 {
+			compatible = "brcm,bcm4908-firmware";
+			label = "firmware";
+			reg = <0x100000 0x4400000>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4906-tplink-archer-c2300-v1.dts
@@ -0,0 +1,182 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/leds/common.h>
+
+#include "bcm4906.dtsi"
+
+/ {
+	compatible = "tplink,archer-c2300-v1", "brcm,bcm4906", "brcm,bcm4908", "brcm,bcmbca";
+	model = "TP-Link Archer C2300 V1";
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x00 0x00 0x00 0x20000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led-power {
+			function = LED_FUNCTION_POWER;
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
+		};
+
+		led-2ghz {
+			function = "2ghz";
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
+		};
+
+		led-5ghz {
+			function = "5ghz";
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 3 GPIO_ACTIVE_LOW>;
+		};
+
+		led-wan-amber {
+			function = LED_FUNCTION_WAN;
+			color = <LED_COLOR_ID_AMBER>;
+			gpios = <&gpio0 4 GPIO_ACTIVE_HIGH>;
+		};
+
+		led-wan-blue {
+			function = LED_FUNCTION_WAN;
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
+		};
+
+		led-lan {
+			function = LED_FUNCTION_LAN;
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
+		};
+
+		led-wps {
+			function = LED_FUNCTION_WPS;
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
+		};
+
+		led-usb2 {
+			function = "usb2";
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 15 GPIO_ACTIVE_LOW>;
+		};
+
+		led-usb3 {
+			function = "usbd3";
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&gpio0 17 GPIO_ACTIVE_LOW>;
+		};
+
+		led-brightness {
+			function = LED_FUNCTION_BACKLIGHT;
+			color = <LED_COLOR_ID_WHITE>;
+			gpios = <&gpio0 19 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	gpio-keys-polled {
+		compatible = "gpio-keys-polled";
+		poll-interval = <100>;
+
+		key-brightness {
+			label = "LEDs";
+			linux,code = <KEY_BRIGHTNESS_ZERO>;
+			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
+		};
+
+		key-wps {
+			label = "WPS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&gpio0 21 GPIO_ACTIVE_LOW>;
+		};
+
+		key-wifi {
+			label = "WiFi";
+			linux,code = <KEY_RFKILL>;
+			gpios = <&gpio0 22 GPIO_ACTIVE_LOW>;
+		};
+
+		key-restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&gpio0 23 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&usb_phy {
+	brcm,ioc = <1>;
+	status = "okay";
+};
+
+&ehci {
+	status = "okay";
+};
+
+&ohci {
+	status = "okay";
+};
+
+&xhci {
+	status = "okay";
+};
+
+&ports {
+	port@0 {
+		label = "lan4";
+	};
+
+	port@1 {
+		label = "lan3";
+	};
+
+	port@2 {
+		label = "lan2";
+	};
+
+	port@3 {
+		label = "lan1";
+	};
+
+	port@7 {
+		reg = <7>;
+		phy-mode = "internal";
+		phy-handle = <&phy12>;
+		label = "wan";
+	};
+};
+
+&nandcs {
+	nand-ecc-strength = <4>;
+	nand-ecc-step-size = <512>;
+	nand-on-flash-bbt;
+
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	partitions {
+		compatible = "brcm,bcm4908-partitions";
+		#address-cells = <1>;
+		#size-cells = <1>;
+
+		partition@0 {
+			label = "cferom";
+			reg = <0x0 0x100000>;
+		};
+
+		partition@100000 {
+			compatible = "brcm,bcm4908-firmware";
+			reg = <0x100000 0x3900000>;
+		};
+
+		partition@5800000 {
+			compatible = "brcm,bcm4908-firmware";
+			reg = <0x3a00000 0x3900000>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4906.dtsi
@@ -0,0 +1,34 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include "bcm4908.dtsi"
+
+/ {
+	cpus {
+		/delete-node/ cpu@2;
+
+		/delete-node/ cpu@3;
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>;
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>;
+	};
+
+	pmu {
+		compatible = "arm,cortex-a53-pmu";
+		interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>,
+			     <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-affinity = <&cpu0>, <&cpu1>;
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4908-asus-gt-ac5300.dts
@@ -0,0 +1,207 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/leds/common.h>
+
+#include "bcm4908.dtsi"
+
+/ {
+	compatible = "asus,gt-ac5300", "brcm,bcm4908", "brcm,bcmbca";
+	model = "Asus GT-AC5300";
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x00 0x00 0x00 0x40000000>;
+	};
+
+	gpio-keys-polled {
+		compatible = "gpio-keys-polled";
+		poll-interval = <100>;
+
+		key-wifi {
+			label = "WiFi";
+			linux,code = <KEY_RFKILL>;
+			gpios = <&gpio0 28 GPIO_ACTIVE_LOW>;
+		};
+
+		key-wps {
+			label = "WPS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&gpio0 29 GPIO_ACTIVE_LOW>;
+		};
+
+		key-restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&gpio0 30 GPIO_ACTIVE_LOW>;
+		};
+
+		key-brightness {
+			label = "LEDs";
+			linux,code = <KEY_BRIGHTNESS_ZERO>;
+			gpios = <&gpio0 31 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&enet {
+	nvmem-cells = <&base_mac_addr>;
+	nvmem-cell-names = "mac-address";
+};
+
+&usb_phy {
+	brcm,ioc = <1>;
+	status = "okay";
+};
+
+&ehci {
+	status = "okay";
+};
+
+&ohci {
+	status = "okay";
+};
+
+&xhci {
+	status = "okay";
+};
+
+&ports {
+	port@0 {
+		label = "lan2";
+	};
+
+	port@1 {
+		label = "lan1";
+	};
+
+	port@2 {
+		label = "lan6";
+	};
+
+	port@3 {
+		label = "lan5";
+	};
+
+	/* External BCM53134S switch */
+	port@7 {
+		label = "sw";
+		reg = <7>;
+		phy-mode = "rgmii";
+
+		fixed-link {
+			speed = <1000>;
+			full-duplex;
+		};
+	};
+};
+
+&mdio {
+	/* lan8 */
+	ethernet-phy@0 {
+		reg = <0>;
+	};
+
+	/* lan7 */
+	ethernet-phy@1 {
+		reg = <1>;
+	};
+
+	/* lan4 */
+	ethernet-phy@2 {
+		reg = <2>;
+	};
+
+	/* lan3 */
+	ethernet-phy@3 {
+		reg = <3>;
+	};
+};
+
+&leds {
+	led-power@11 {
+		reg = <0x11>;
+		function = LED_FUNCTION_POWER;
+		color = <LED_COLOR_ID_WHITE>;
+		default-state = "on";
+		active-low;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pins_led_17_a>;
+	};
+
+	led-wan-red@12 {
+		reg = <0x12>;
+		function = LED_FUNCTION_WAN;
+		color = <LED_COLOR_ID_RED>;
+		active-low;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pins_led_18_a>;
+	};
+
+	led-wps@14 {
+		reg = <0x14>;
+		function = LED_FUNCTION_WPS;
+		color = <LED_COLOR_ID_WHITE>;
+		active-low;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pins_led_20_a>;
+	};
+
+	led-wan-white@15 {
+		reg = <0x15>;
+		function = LED_FUNCTION_WAN;
+		color = <LED_COLOR_ID_WHITE>;
+		active-low;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pins_led_21_a>;
+	};
+
+	led-lan@19 {
+		reg = <0x19>;
+		function = LED_FUNCTION_LAN;
+		color = <LED_COLOR_ID_WHITE>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pins_led_25_a>;
+	};
+};
+
+&nandcs {
+	nand-ecc-strength = <4>;
+	nand-ecc-step-size = <512>;
+	nand-on-flash-bbt;
+	brcm,nand-has-wp;
+
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	partitions {
+		compatible = "brcm,bcm4908-partitions";
+		#address-cells = <1>;
+		#size-cells = <1>;
+
+		partition@0 {
+			compatible = "nvmem-cells";
+			label = "cferom";
+			reg = <0x0 0x100000>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0 0x0 0x100000>;
+
+			base_mac_addr: mac@106a0 {
+				reg = <0x106a0 0x6>;
+			};
+		};
+
+		partition@100000 {
+			compatible = "brcm,bcm4908-firmware";
+			reg = <0x100000 0x5700000>;
+		};
+
+		partition@5800000 {
+			compatible = "brcm,bcm4908-firmware";
+			reg = <0x5800000 0x5700000>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4908-netgear-raxe500.dts
@@ -0,0 +1,50 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include "bcm4908.dtsi"
+
+/ {
+	compatible = "netgear,raxe500", "brcm,bcm4908", "brcm,bcmbca";
+	model = "Netgear RAXE500";
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x00 0x00 0x00 0x40000000>;
+	};
+};
+
+&ehci {
+	status = "okay";
+};
+
+&ohci {
+	status = "okay";
+};
+
+&xhci {
+	status = "okay";
+};
+
+&ports {
+	port@0 {
+		label = "lan4";
+	};
+
+	port@1 {
+		label = "lan3";
+	};
+
+	port@2 {
+		label = "lan2";
+	};
+
+	port@3 {
+		label = "lan1";
+	};
+
+	port@7 {
+		reg = <7>;
+		phy-mode = "internal";
+		phy-handle = <&phy12>;
+		label = "wan";
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4908.dtsi
@@ -0,0 +1,575 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include <dt-bindings/interrupt-controller/irq.h>
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/phy/phy.h>
+#include <dt-bindings/soc/bcm-pmb.h>
+
+/dts-v1/;
+
+/ {
+	interrupt-parent = <&gic>;
+
+	#address-cells = <2>;
+	#size-cells = <2>;
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "brcm,brahma-b53";
+			reg = <0x0>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0xfff8>;
+			next-level-cache = <&l2>;
+		};
+
+		cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "brcm,brahma-b53";
+			reg = <0x1>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0xfff8>;
+			next-level-cache = <&l2>;
+		};
+
+		cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "brcm,brahma-b53";
+			reg = <0x2>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0xfff8>;
+			next-level-cache = <&l2>;
+		};
+
+		cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "brcm,brahma-b53";
+			reg = <0x3>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0xfff8>;
+			next-level-cache = <&l2>;
+		};
+
+		l2: l2-cache0 {
+			compatible = "cache";
+		};
+	};
+
+	axi@81000000 {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges = <0x00 0x00 0x81000000 0x4000>;
+
+		gic: interrupt-controller@1000 {
+			compatible = "arm,gic-400";
+			#interrupt-cells = <3>;
+			#address-cells = <0>;
+			interrupt-controller;
+			reg = <0x1000 0x1000>,
+			      <0x2000 0x2000>;
+		};
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
+	};
+
+	pmu {
+		compatible = "arm,cortex-a53-pmu";
+		interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>,
+			     <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>,
+			     <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>,
+			     <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-affinity = <&cpu0>, <&cpu1>, <&cpu2>, <&cpu3>;
+	};
+
+	clocks {
+		periph_clk: periph_clk {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <50000000>;
+			clock-output-names = "periph";
+		};
+	};
+
+	soc {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges = <0x00 0x00 0x80000000 0x281000>;
+
+		enet: ethernet@2000 {
+			compatible = "brcm,bcm4908-enet";
+			reg = <0x2000 0x1000>;
+
+			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "rx", "tx";
+		};
+
+		usb_phy: usb-phy@c200 {
+			compatible = "brcm,bcm4908-usb-phy";
+			reg = <0xc200 0x100>;
+			reg-names = "ctrl";
+			power-domains = <&pmb BCM_PMB_HOST_USB>;
+			dr_mode = "host";
+			brcm,has-xhci;
+			brcm,has-eohci;
+			#phy-cells = <1>;
+			status = "disabled";
+		};
+
+		ehci: usb@c300 {
+			compatible = "generic-ehci";
+			reg = <0xc300 0x100>;
+			interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
+			phys = <&usb_phy PHY_TYPE_USB2>;
+			status = "disabled";
+		};
+
+		ohci: usb@c400 {
+			compatible = "generic-ohci";
+			reg = <0xc400 0x100>;
+			interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
+			phys = <&usb_phy PHY_TYPE_USB2>;
+			status = "disabled";
+		};
+
+		xhci: usb@d000 {
+			compatible = "generic-xhci";
+			reg = <0xd000 0x8c8>;
+			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
+			phys = <&usb_phy PHY_TYPE_USB3>;
+			status = "disabled";
+		};
+
+		bus@80000 {
+			compatible = "simple-bus";
+			#size-cells = <1>;
+			#address-cells = <1>;
+			ranges = <0 0x80000 0x50000>;
+
+			ethernet-switch@0 {
+				compatible = "brcm,bcm4908-switch";
+				reg = <0x0 0x40000>,
+				      <0x40000 0x110>,
+				      <0x40340 0x30>,
+				      <0x40380 0x30>,
+				      <0x40600 0x34>,
+				      <0x40800 0x208>;
+				reg-names = "core", "reg", "intrl2_0",
+					    "intrl2_1", "fcb", "acb";
+				interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>,
+					     <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>;
+				brcm,num-gphy = <5>;
+				brcm,num-rgmii-ports = <2>;
+
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				ports: ports {
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					port@0 {
+						reg = <0>;
+						phy-mode = "internal";
+						phy-handle = <&phy8>;
+					};
+
+					port@1 {
+						reg = <1>;
+						phy-mode = "internal";
+						phy-handle = <&phy9>;
+					};
+
+					port@2 {
+						reg = <2>;
+						phy-mode = "internal";
+						phy-handle = <&phy10>;
+					};
+
+					port@3 {
+						reg = <3>;
+						phy-mode = "internal";
+						phy-handle = <&phy11>;
+					};
+
+					port@8 {
+						reg = <8>;
+						phy-mode = "internal";
+						ethernet = <&enet>;
+
+						fixed-link {
+							speed = <1000>;
+							full-duplex;
+						};
+					};
+				};
+			};
+
+			mdio: mdio@405c0 {
+				compatible = "brcm,unimac-mdio";
+				reg = <0x405c0 0x8>;
+				reg-names = "mdio";
+				#size-cells = <0>;
+				#address-cells = <1>;
+
+				phy8: ethernet-phy@8 {
+					reg = <8>;
+				};
+
+				phy9: ethernet-phy@9 {
+					reg = <9>;
+				};
+
+				phy10: ethernet-phy@a {
+					reg = <10>;
+				};
+
+				phy11: ethernet-phy@b {
+					reg = <11>;
+				};
+
+				phy12: ethernet-phy@c {
+					reg = <12>;
+				};
+			};
+		};
+
+		procmon: syscon@280000 {
+			compatible = "simple-bus";
+			reg = <0x280000 0x1000>;
+			ranges;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			pmb: power-controller@2800c0 {
+				compatible = "brcm,bcm4908-pmb";
+				reg = <0x2800c0 0x40>;
+				#power-domain-cells = <1>;
+			};
+		};
+	};
+
+	bus@ff800000 {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges = <0x00 0x00 0xff800000 0x3000>;
+
+		twd: timer-mfd@400 {
+			compatible = "brcm,bcm4908-twd", "simple-mfd", "syscon";
+			reg = <0x400 0x4c>;
+			ranges = <0x0 0x400 0x4c>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			watchdog@28 {
+				compatible = "brcm,bcm6345-wdt";
+				reg = <0x28 0x8>;
+			};
+		};
+
+		gpio0: gpio-controller@500 {
+			compatible = "brcm,bcm6345-gpio";
+			reg-names = "dirout", "dat";
+			reg = <0x500 0x28>, <0x528 0x28>;
+
+			#gpio-cells = <2>;
+			gpio-controller;
+		};
+
+		pinctrl@560 {
+			compatible = "brcm,bcm4908-pinctrl";
+			reg = <0x560 0x10>;
+
+			pins_led_0_a: led_0-a-pins {
+				function = "led_0";
+				groups = "led_0_grp_a";
+			};
+
+			pins_led_1_a: led_1-a-pins {
+				function = "led_1";
+				groups = "led_1_grp_a";
+			};
+
+			pins_led_2_a: led_2-a-pins {
+				function = "led_2";
+				groups = "led_2_grp_a";
+			};
+
+			pins_led_3_a: led_3-a-pins {
+				function = "led_3";
+				groups = "led_3_grp_a";
+			};
+
+			pins_led_4_a: led_4-a-pins {
+				function = "led_4";
+				groups = "led_4_grp_a";
+			};
+
+			pins_led_5_a: led_5-a-pins {
+				function = "led_5";
+				groups = "led_5_grp_a";
+			};
+
+			pins_led_6_a: led_6-a-pins {
+				function = "led_6";
+				groups = "led_6_grp_a";
+			};
+
+			pins_led_7_a: led_7-a-pins {
+				function = "led_7";
+				groups = "led_7_grp_a";
+			};
+
+			pins_led_8_a: led_8-a-pins {
+				function = "led_8";
+				groups = "led_8_grp_a";
+			};
+
+			pins_led_9_a: led_9-a-pins {
+				function = "led_9";
+				groups = "led_9_grp_a";
+			};
+
+			pins_led_10_a: led_10-a-pins {
+				function = "led_10";
+				groups = "led_10_grp_a";
+			};
+
+			pins_led_11_a: led_11-a-pins {
+				function = "led_11";
+				groups = "led_11_grp_a";
+			};
+
+			pins_led_12_a: led_12-a-pins {
+				function = "led_12";
+				groups = "led_12_grp_a";
+			};
+
+			pins_led_13_a: led_13-a-pins {
+				function = "led_13";
+				groups = "led_13_grp_a";
+			};
+
+			pins_led_14_a: led_14-a-pins {
+				function = "led_14";
+				groups = "led_14_grp_a";
+			};
+
+			pins_led_15_a: led_15-a-pins {
+				function = "led_15";
+				groups = "led_15_grp_a";
+			};
+
+			pins_led_16_a: led_16-a-pins {
+				function = "led_16";
+				groups = "led_16_grp_a";
+			};
+
+			pins_led_17_a: led_17-a-pins {
+				function = "led_17";
+				groups = "led_17_grp_a";
+			};
+
+			pins_led_18_a: led_18-a-pins {
+				function = "led_18";
+				groups = "led_18_grp_a";
+			};
+
+			pins_led_19_a: led_19-a-pins {
+				function = "led_19";
+				groups = "led_19_grp_a";
+			};
+
+			pins_led_20_a: led_20-a-pins {
+				function = "led_20";
+				groups = "led_20_grp_a";
+			};
+
+			pins_led_21_a: led_21-a-pins {
+				function = "led_21";
+				groups = "led_21_grp_a";
+			};
+
+			pins_led_22_a: led_22-a-pins {
+				function = "led_22";
+				groups = "led_22_grp_a";
+			};
+
+			pins_led_23_a: led_23-a-pins {
+				function = "led_23";
+				groups = "led_23_grp_a";
+			};
+
+			pins_led_24_a: led_24-a-pins {
+				function = "led_24";
+				groups = "led_24_grp_a";
+			};
+
+			pins_led_25_a: led_25-a-pins {
+				function = "led_25";
+				groups = "led_25_grp_a";
+			};
+
+			pins_led_26_a: led_26-a-pins {
+				function = "led_26";
+				groups = "led_26_grp_a";
+			};
+
+			pins_led_27_a: led_27-a-pins {
+				function = "led_27";
+				groups = "led_27_grp_a";
+			};
+
+			pins_led_28_a: led_28-a-pins {
+				function = "led_28";
+				groups = "led_28_grp_a";
+			};
+
+			pins_led_29_a: led_29-a-pins {
+				function = "led_29";
+				groups = "led_29_grp_a";
+			};
+
+			pins_led_30_a: led_30-a-pins {
+				function = "led_30";
+				groups = "led_30_grp_a";
+			};
+
+			pins_led_31_a: led_31-a-pins {
+				function = "led_31";
+				groups = "led_31_grp_a";
+			};
+
+			pins_hs_uart: hs_uart-pins {
+				function = "hs_uart";
+				groups = "hs_uart_grp";
+			};
+
+			pins_i2c_a: i2c-a-pins {
+				function = "i2c";
+				groups = "i2c_grp_a";
+			};
+
+			pins_i2c_b: i2c-b-pins {
+				function = "i2c";
+				groups = "i2c_grp_b";
+			};
+
+			pins_i2s: i2s-pins {
+				function = "i2s";
+				groups = "i2s_grp";
+			};
+
+			pins_nand_ctrl: nand_ctrl-pins {
+				function = "nand_ctrl";
+				groups = "nand_ctrl_grp";
+			};
+
+			pins_nand_data: nand_data-pins {
+				function = "nand_data";
+				groups = "nand_data_grp";
+			};
+
+			pins_emmc_ctrl: emmc_ctrl-pins {
+				function = "emmc_ctrl";
+				groups = "emmc_ctrl_grp";
+			};
+
+			pins_usb0_pwr: usb0_pwr-pins {
+				function = "usb0_pwr";
+				groups = "usb0_pwr_grp";
+			};
+
+			pins_usb1_pwr: usb1_pwr-pins {
+				function = "usb1_pwr";
+				groups = "usb1_pwr_grp";
+			};
+		};
+
+		uart0: serial@640 {
+			compatible = "brcm,bcm6345-uart";
+			reg = <0x640 0x18>;
+			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&periph_clk>;
+			clock-names = "refclk";
+			status = "okay";
+		};
+
+		leds: leds@800 {
+			compatible = "brcm,bcm4908-leds", "brcm,bcm63138-leds";
+			reg = <0x800 0xdc>;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		nand-controller@1800 {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			compatible = "brcm,nand-bcm63138", "brcm,brcmnand-v7.1", "brcm,brcmnand";
+			reg = <0x1800 0x600>, <0x2000 0x10>;
+			reg-names = "nand", "nand-int-base";
+			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "nand";
+			status = "okay";
+
+			nandcs: nand@0 {
+				compatible = "brcm,nandcs";
+				reg = <0>;
+			};
+		};
+
+		i2c@2100 {
+			compatible = "brcm,brcmper-i2c";
+			reg = <0x2100 0x58>;
+			clock-frequency = <97500>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&pins_i2c_a>;
+			status = "disabled";
+		};
+
+		misc@2600 {
+			compatible = "brcm,misc", "simple-mfd";
+			reg = <0x2600 0xe4>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0x00 0x2600 0xe4>;
+
+			reset-controller@2644 {
+				compatible = "brcm,bcm4908-misc-pcie-reset";
+				reg = <0x44 0x04>;
+				#reset-cells = <1>;
+			};
+		};
+	};
+
+	reboot {
+		compatible = "syscon-reboot";
+		regmap = <&twd>;
+		offset = <0x34>;
+		mask = <1>;
+	};
+};
