#include "bcm6328.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Broadcom bcm963281TAN reference board";
	compatible = "brcm,bcm963281tan", "brcm,bcm6328";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";

		inet {
			label = "internet";
			gpios = <&pinctrl 1 1>;
		};
		led_power: power {
			label = "power";
			gpios = <&pinctrl 4 1>;
			default-state = "on";
		};
		inet_fail {
			label = "internet-fail";
			gpios = <&pinctrl 7 1>;
		};
		power_fail {
			label = "power-fail";
			gpios = <&pinctrl 8 1>;
		};
		wps {
			label = "wps";
			gpios = <&pinctrl 9 1>;
		};
		dsl {
			label = "dsl";
			gpios = <&pinctrl 11 1>;
		};
	};
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <16666667>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "brcm,bcm963xx-cfe-nor-partitions";
		};
	};
};

&uart0 {
	status = "okay";
};
