From f4a7e56f4956f0450b9f671ed93d45ffcc15aa62 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Tue, 18 Jan 2022 01:22:05 +0100
Subject: [PATCH v6 13/15] dt-bindings: reset: add ipq8064 ce5 resets

Add ipq8064 ce5 resets needed for CryptoEngine gcc driver.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Reviewed-by: Bjorn Andersson <bjorn.andersson@linaro.org>
Acked-by: Philipp Zabel <p.zabel@pengutronix.de>
Acked-by: Rob Herring <robh@kernel.org>
Reviewed-by: Stephen Boyd <sboyd@kernel.org>
---
 include/dt-bindings/reset/qcom,gcc-ipq806x.h | 5 +++++
 1 file changed, 5 insertions(+)

--- a/include/dt-bindings/reset/qcom,gcc-ipq806x.h
+++ b/include/dt-bindings/reset/qcom,gcc-ipq806x.h
@@ -163,5 +163,10 @@
 #define NSS_CAL_PRBS_RST_N_RESET			154
 #define NSS_LCKDT_RST_N_RESET				155
 #define NSS_SRDS_N_RESET				156
+#define CRYPTO_ENG1_RESET				157
+#define CRYPTO_ENG2_RESET				158
+#define CRYPTO_ENG3_RESET				159
+#define CRYPTO_ENG4_RESET				160
+#define CRYPTO_AHB_RESET				161
 
 #endif
