From 7e4ae2d6285095794d73d2f2ce61404f61d4e633 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Tue, 17 May 2022 15:55:36 +0200
Subject: [PATCH 11/11] treewide: fix confusing printing of registered netdev

Net core implementation changed and now printing the netdev name cause
confusing printing if done before register_netdev. Move the old printing
to dbg and add an additional info log right after register_netdev to
give the user some info on correct nss-dp probe.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
---
 hal/dp_ops/edma_dp/edma_v1/edma_data_plane.c | 4 ++--
 nss_dp_main.c                                | 3 +++
 2 files changed, 5 insertions(+), 2 deletions(-)

--- a/hal/dp_ops/edma_dp/edma_v1/edma_data_plane.c
+++ b/hal/dp_ops/edma_dp/edma_v1/edma_data_plane.c
@@ -822,8 +822,8 @@ static int edma_register_netdevice(struc
 		return -EINVAL;
 	}
 
-	netdev_info(netdev, "nss_dp_edma: Registering netdev %s(qcom-id:%d) with EDMA\n",
-		netdev->name, macid);
+	netdev_dbg(netdev, "nss_dp_edma: Registering netdev %s(qcom-id:%d) with EDMA\n",
+		   netdev->name, macid);
 
 	/*
 	 * We expect 'macid' to correspond to ports numbers on
--- a/nss_dp_main.c
+++ b/nss_dp_main.c
@@ -875,6 +875,9 @@ static int32_t nss_dp_probe(struct platf
 		goto phy_setup_fail;
 	}
 
+	netdev_info(netdev, "Registered netdev %s(qcom-id:%d)\n",
+		    netdev->name, port_id);
+
 	dp_global_ctx.nss_dp[dp_priv->macid - 1] = dp_priv;
 	dp_global_ctx.slowproto_acl_bm = 0;
 
