#include "qcom-ipq8064-v2.0.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "TP-Link Archer VR2600v";
	compatible = "tplink,vr2600v", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		mdio-gpio0 = &mdio0;

		led-boot = &power;
		led-failsafe = &general;
		led-running = &power;
		led-upgrade = &general;
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wifi {
			label = "wifi";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};

		dect {
			label = "dect";
			gpios = <&qcom_pinmux 67 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_PHONE>;
			debounce-interval = <60>;
			wakeup-source;
		};

		ledswitch {
			label = "ledswitch";
			gpios = <&qcom_pinmux 68 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_LIGHTS_TOGGLE>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		dsl {
			label = "white:dsl";
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
		};

		usb {
			label = "white:usb";
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};

		lan {
			label = "white:lan";
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
		};

		wlan2g {
			label = "white:wlan2g";
			gpios = <&qcom_pinmux 16 GPIO_ACTIVE_HIGH>;
		};

		wlan5g {
			label = "white:wlan5g";
			gpios = <&qcom_pinmux 17 GPIO_ACTIVE_HIGH>;
		};

		power: power {
			label = "white:power";
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		phone {
			label = "white:phone";
			gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>;
		};

		wan {
			label = "white:wan";
			gpios = <&qcom_pinmux 56 GPIO_ACTIVE_HIGH>;
		};

		general: general {
			label = "white:general";
			gpios = <&qcom_pinmux 66 GPIO_ACTIVE_HIGH>;
		};
	};
};

&qcom_pinmux {
	led_pins: led_pins {
		mux {
			pins = "gpio7", "gpio8", "gpio9", "gpio16", "gpio17",
				"gpio26", "gpio53", "gpio56", "gpio66";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	button_pins: button_pins {
		mux {
			pins = "gpio54", "gpio64", "gpio65", "gpio67", "gpio68";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	spi_pins: spi_pins {
		mux {
			pins = "gpio18", "gpio19", "gpio21";
			function = "gsbi5";
			bias-pull-down;
		};

		data {
			pins = "gpio18", "gpio19";
			drive-strength = <10>;
		};

		cs {
			pins = "gpio20";
			drive-strength = <10>;
			bias-pull-up;
		};

		clk {
			pins = "gpio21";
			drive-strength = <12>;
		};
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi4: spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_HIGH>;

		flash@0 {
			compatible = "jedec,spi-nor";
			#address-cells = <1>;
			#size-cells = <1>;
			spi-max-frequency = <50000000>;
			reg = <0>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "SBL1";
					reg = <0x0 0x20000>;
					read-only;
				};

				partition@20000 {
					label = "MIBIB";
					reg = <0x20000 0x20000>;
					read-only;
				};

				partition@40000 {
					label = "SBL2";
					reg = <0x40000 0x40000>;
					read-only;
				};

				partition@80000 {
					label = "SBL3";
					reg = <0x80000 0x80000>;
					read-only;
				};

				partition@100000 {
					label = "DDRCONFIG";
					reg = <0x100000 0x10000>;
					read-only;
				};

				partition@110000 {
					label = "SSD";
					reg = <0x110000 0x10000>;
					read-only;
				};

				partition@120000 {
					label = "TZ";
					reg = <0x120000 0x80000>;
					read-only;
				};

				partition@1a0000 {
					label = "RPM";
					reg = <0x1a0000 0x80000>;
					read-only;
				};

				partition@220000 {
					label = "APPSBL";
					reg = <0x220000 0x80000>;
					read-only;
				};

				partition@2a0000 {
					label = "APPSBLENV";
					reg = <0x2a0000 0x40000>;
					read-only;
				};

				partition@2e0000 {
					label = "OLDART";
					reg = <0x2e0000 0x40000>;
					read-only;
				};

				partition@320000 {
					label = "firmware";
					reg = <0x320000 0xc60000>;
					compatible = "openwrt,uimage";
					openwrt,offset = <512>; /* account for pad-extra 512 */
				};

				/* hole 0xf80000 - 0xfaf100 */

				partition@faf100 {
					label = "default-mac";
					reg = <0xfaf100 0x00200>;
					read-only;

					compatible = "nvmem-cells";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_defaultmac_0: macaddr@0 {
						reg = <0x0 0x6>;
					};
				};

				partition@fc0000 {
					label = "ART";
					reg = <0xfc0000 0x40000>;
					read-only;

					compatible = "nvmem-cells";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_ART_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_ART_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
		};
	};
};

&usb3_0 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&pcie0 {
	status = "okay";

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "pci168c,0040";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_defaultmac_0>, <&precal_ART_1000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
			mac-address-increment = <(-1)>;
		};
	};
};

&pcie1 {
	status = "okay";
	max-link-speed = <1>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "pci168c,0040";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_defaultmac_0>, <&precal_ART_5000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
		};
	};
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	phy0: ethernet-phy@0 {
		reg = <0>;
		qca,ar8327-initvals = <
			0x00004 0x7600000   /* PAD0_MODE */
			0x00008 0x1000000   /* PAD5_MODE */
			0x0000c 0x80        /* PAD6_MODE */
			0x000e4 0x6a545     /* MAC_POWER_SEL */
			0x000e0 0xc74164de  /* SGMII_CTRL */
			0x0007c 0x4e        /* PORT0_STATUS */
			0x00094 0x4e        /* PORT6_STATUS */
			>;
	};

	phy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	nvmem-cells = <&macaddr_defaultmac_0>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <2>;

	nvmem-cells = <&macaddr_defaultmac_0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&adm_dma {
	status = "okay";
};
