From 69c4e53bdd055ecc27761f6971a50c631ff9072e Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Thu, 2 Dec 2021 15:16:27 -0800
Subject: [PATCH] ARM: dts: NSP: Fixed iProc PCIe MSI sub-node

Rename the msi controller unit name to 'msi' to avoid collisions with
the 'msi-controller' boolean property.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm-nsp.dtsi | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm/boot/dts/bcm-nsp.dtsi
+++ b/arch/arm/boot/dts/bcm-nsp.dtsi
@@ -587,7 +587,7 @@
 		status = "disabled";
 
 		msi-parent = <&msi0>;
-		msi0: msi-controller {
+		msi0: msi {
 			compatible = "brcm,iproc-msi";
 			msi-controller;
 			interrupt-parent = <&gic>;
@@ -624,7 +624,7 @@
 		status = "disabled";
 
 		msi-parent = <&msi1>;
-		msi1: msi-controller {
+		msi1: msi {
 			compatible = "brcm,iproc-msi";
 			msi-controller;
 			interrupt-parent = <&gic>;
@@ -661,7 +661,7 @@
 		status = "disabled";
 
 		msi-parent = <&msi2>;
-		msi2: msi-controller {
+		msi2: msi {
 			compatible = "brcm,iproc-msi";
 			msi-controller;
 			interrupt-parent = <&gic>;
