From 98feaf97bc64fc640a6c5b1394cd18fc7cd7dac8 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Sun, 28 Mar 2021 14:34:49 +0200
Subject: [PATCH] PCI: aardvark: Refactor unmasking summary MSI interrupt
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Refactor the masking of ISR0/1 Sources and unmasking of summary MSI interrupt
so that it corresponds to the comments:
- first mask all ISR0/1
- then unmask all MSIs
- then unmask summary MSI interrupt

Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/pci/controller/pci-aardvark.c | 10 ++++++----
 1 file changed, 6 insertions(+), 4 deletions(-)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -578,15 +578,17 @@ static void advk_pcie_setup_hw(struct ad
 	advk_writel(pcie, PCIE_IRQ_ALL_MASK, HOST_CTRL_INT_STATUS_REG);
 
 	/* Disable All ISR0/1 Sources */
-	reg = PCIE_ISR0_ALL_MASK;
-	reg &= ~PCIE_ISR0_MSI_INT_PENDING;
-	advk_writel(pcie, reg, PCIE_ISR0_MASK_REG);
-
+	advk_writel(pcie, PCIE_ISR0_ALL_MASK, PCIE_ISR0_MASK_REG);
 	advk_writel(pcie, PCIE_ISR1_ALL_MASK, PCIE_ISR1_MASK_REG);
 
 	/* Unmask all MSIs */
 	advk_writel(pcie, ~(u32)PCIE_MSI_ALL_MASK, PCIE_MSI_MASK_REG);
 
+	/* Unmask summary MSI interrupt */
+	reg = advk_readl(pcie, PCIE_ISR0_MASK_REG);
+	reg &= ~PCIE_ISR0_MSI_INT_PENDING;
+	advk_writel(pcie, reg, PCIE_ISR0_MASK_REG);
+
 	/* Enable summary interrupt for GIC SPI source */
 	reg = PCIE_IRQ_ALL_MASK & (~PCIE_IRQ_ENABLE_INTS_MASK);
 	advk_writel(pcie, reg, HOST_CTRL_INT_MASK_REG);
