From dccb22d078ebd098115e4f66bde1ee2249c8640b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 12 Nov 2020 16:08:30 +0100
Subject: [PATCH] arm64: add config for Broadcom BCM4908 SoCs
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add ARCH_BCM4908 config that can be used for compiling DTS files.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm64/Kconfig.platforms | 8 ++++++++
 arch/arm64/configs/defconfig | 1 +
 2 files changed, 9 insertions(+)

--- a/arch/arm64/Kconfig.platforms
+++ b/arch/arm64/Kconfig.platforms
@@ -43,6 +43,14 @@ config ARCH_BCM2835
 	  This enables support for the Broadcom BCM2837 and BCM2711 SoC.
 	  These SoCs are used in the Raspberry Pi 3 and 4 devices.
 
+config ARCH_BCM4908
+	bool "Broadcom BCM4908 family"
+	select GPIOLIB
+	help
+	  This enables support for the Broadcom BCM4906, BCM4908 and
+	  BCM49408 SoCs. These SoCs use Brahma-B53 cores and can be
+	  found in home routers.
+
 config ARCH_BCM_IPROC
 	bool "Broadcom iProc SoC Family"
 	select COMMON_CLK_IPROC
--- a/arch/arm64/configs/defconfig
+++ b/arch/arm64/configs/defconfig
@@ -32,6 +32,7 @@ CONFIG_ARCH_AGILEX=y
 CONFIG_ARCH_SUNXI=y
 CONFIG_ARCH_ALPINE=y
 CONFIG_ARCH_BCM2835=y
+CONFIG_ARCH_BCM4908=y
 CONFIG_ARCH_BCM_IPROC=y
 CONFIG_ARCH_BERLIN=y
 CONFIG_ARCH_BRCMSTB=y
