--- a/drivers/net/wireless/ath/ath5k/base.c
+++ b/drivers/net/wireless/ath/ath5k/base.c
@@ -2417,6 +2417,22 @@ ath5k_tx_complete_poll_work(struct work_
 * Initialization routines *
 \*************************/
 
+static const struct ieee80211_iface_limit if_limits[] = {
+	{ .max = 2048,	.types = BIT(NL80211_IFTYPE_STATION) },
+	{ .max = 4,	.types =
+#ifdef CONFIG_MAC80211_MESH
+				 BIT(NL80211_IFTYPE_MESH_POINT) |
+#endif
+				 BIT(NL80211_IFTYPE_AP) },
+};
+
+static const struct ieee80211_iface_combination if_comb = {
+	.limits = if_limits,
+	.n_limits = ARRAY_SIZE(if_limits),
+	.max_interfaces = 2048,
+	.num_different_channels = 1,
+};
+
 int __devinit
 ath5k_init_ah(struct ath5k_hw *ah, const struct ath_bus_ops *bus_ops)
 {
@@ -2438,6 +2454,9 @@ ath5k_init_ah(struct ath5k_hw *ah, const
 		BIT(NL80211_IFTYPE_ADHOC) |
 		BIT(NL80211_IFTYPE_MESH_POINT);
 
+	hw->wiphy->iface_combinations = &if_comb;
+	hw->wiphy->n_iface_combinations = 1;
+
 	/* SW support for IBSS_RSN is provided by mac80211 */
 	hw->wiphy->flags |= WIPHY_FLAG_IBSS_RSN;
 
--- a/net/mac80211/agg-rx.c
+++ b/net/mac80211/agg-rx.c
@@ -145,15 +145,20 @@ static void sta_rx_agg_session_timer_exp
 	struct tid_ampdu_rx *tid_rx;
 	unsigned long timeout;
 
+	rcu_read_lock();
 	tid_rx = rcu_dereference(sta->ampdu_mlme.tid_rx[*ptid]);
-	if (!tid_rx)
+	if (!tid_rx) {
+		rcu_read_unlock();
 		return;
+	}
 
 	timeout = tid_rx->last_rx + TU_TO_JIFFIES(tid_rx->timeout);
 	if (time_is_after_jiffies(timeout)) {
 		mod_timer(&tid_rx->session_timer, timeout);
+		rcu_read_unlock();
 		return;
 	}
+	rcu_read_unlock();
 
 #ifdef CONFIG_MAC80211_HT_DEBUG
 	printk(KERN_DEBUG "rx session timer expired on tid %d\n", (u16)*ptid);
@@ -200,6 +205,8 @@ static void ieee80211_send_addba_resp(st
 		memcpy(mgmt->bssid, sdata->u.mgd.bssid, ETH_ALEN);
 	else if (sdata->vif.type == NL80211_IFTYPE_ADHOC)
 		memcpy(mgmt->bssid, sdata->u.ibss.bssid, ETH_ALEN);
+	else if (sdata->vif.type == NL80211_IFTYPE_WDS)
+		memcpy(mgmt->bssid, da, ETH_ALEN);
 
 	mgmt->frame_control = cpu_to_le16(IEEE80211_FTYPE_MGMT |
 					  IEEE80211_STYPE_ACTION);
--- a/net/mac80211/agg-tx.c
+++ b/net/mac80211/agg-tx.c
@@ -81,7 +81,8 @@ static void ieee80211_send_addba_request
 	memcpy(mgmt->sa, sdata->vif.addr, ETH_ALEN);
 	if (sdata->vif.type == NL80211_IFTYPE_AP ||
 	    sdata->vif.type == NL80211_IFTYPE_AP_VLAN ||
-	    sdata->vif.type == NL80211_IFTYPE_MESH_POINT)
+	    sdata->vif.type == NL80211_IFTYPE_MESH_POINT ||
+	    sdata->vif.type == NL80211_IFTYPE_WDS)
 		memcpy(mgmt->bssid, sdata->vif.addr, ETH_ALEN);
 	else if (sdata->vif.type == NL80211_IFTYPE_STATION)
 		memcpy(mgmt->bssid, sdata->u.mgd.bssid, ETH_ALEN);
@@ -490,6 +491,7 @@ int ieee80211_start_tx_ba_session(struct
 	    sdata->vif.type != NL80211_IFTYPE_MESH_POINT &&
 	    sdata->vif.type != NL80211_IFTYPE_AP_VLAN &&
 	    sdata->vif.type != NL80211_IFTYPE_AP &&
+	    sdata->vif.type != NL80211_IFTYPE_WDS &&
 	    sdata->vif.type != NL80211_IFTYPE_ADHOC)
 		return -EINVAL;
 
--- a/net/mac80211/debugfs_sta.c
+++ b/net/mac80211/debugfs_sta.c
@@ -63,11 +63,11 @@ static ssize_t sta_flags_read(struct fil
 	test_sta_flag(sta, WLAN_STA_##flg) ? #flg "\n" : ""
 
 	int res = scnprintf(buf, sizeof(buf),
-			    "%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s",
+			    "%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s",
 			    TEST(AUTH), TEST(ASSOC), TEST(PS_STA),
 			    TEST(PS_DRIVER), TEST(AUTHORIZED),
 			    TEST(SHORT_PREAMBLE),
-			    TEST(WME), TEST(WDS), TEST(CLEAR_PS_FILT),
+			    TEST(WME), TEST(CLEAR_PS_FILT),
 			    TEST(MFP), TEST(BLOCK_BA), TEST(PSPOLL),
 			    TEST(UAPSD), TEST(SP), TEST(TDLS_PEER),
 			    TEST(TDLS_PEER_AUTH), TEST(4ADDR_EVENT),
--- a/net/mac80211/iface.c
+++ b/net/mac80211/iface.c
@@ -284,7 +284,6 @@ static int ieee80211_do_open(struct net_
 {
 	struct ieee80211_sub_if_data *sdata = IEEE80211_DEV_TO_SUB_IF(dev);
 	struct ieee80211_local *local = sdata->local;
-	struct sta_info *sta;
 	u32 changed = 0;
 	int res;
 	u32 hw_reconf_flags = 0;
@@ -430,28 +429,6 @@ static int ieee80211_do_open(struct net_
 
 	set_bit(SDATA_STATE_RUNNING, &sdata->state);
 
-	if (sdata->vif.type == NL80211_IFTYPE_WDS) {
-		/* Create STA entry for the WDS peer */
-		sta = sta_info_alloc(sdata, sdata->u.wds.remote_addr,
-				     GFP_KERNEL);
-		if (!sta) {
-			res = -ENOMEM;
-			goto err_del_interface;
-		}
-
-		sta_info_pre_move_state(sta, IEEE80211_STA_AUTH);
-		sta_info_pre_move_state(sta, IEEE80211_STA_ASSOC);
-		sta_info_pre_move_state(sta, IEEE80211_STA_AUTHORIZED);
-
-		res = sta_info_insert(sta);
-		if (res) {
-			/* STA has been freed */
-			goto err_del_interface;
-		}
-
-		rate_control_rate_init(sta);
-	}
-
 	/*
 	 * set_multicast_list will be invoked by the networking core
 	 * which will check whether any increments here were done in
@@ -642,6 +619,8 @@ static void ieee80211_do_stop(struct iee
 		ieee80211_configure_filter(local);
 		break;
 	default:
+		flush_work(&local->hw_roc_start);
+		flush_work(&local->hw_roc_done);
 		flush_work(&sdata->work);
 		/*
 		 * When we get here, the interface is marked down.
@@ -848,6 +827,72 @@ static void ieee80211_if_setup(struct ne
 	dev->destructor = free_netdev;
 }
 
+static void ieee80211_wds_rx_queued_mgmt(struct ieee80211_sub_if_data *sdata,
+					 struct sk_buff *skb)
+{
+	struct ieee80211_local *local = sdata->local;
+	struct ieee80211_rx_status *rx_status;
+	struct ieee802_11_elems elems;
+	struct ieee80211_mgmt *mgmt;
+	struct sta_info *sta;
+	size_t baselen;
+	u32 rates = 0;
+	u16 stype;
+	bool new = false;
+	enum ieee80211_band band = local->hw.conf.channel->band;
+	struct ieee80211_supported_band *sband = local->hw.wiphy->bands[band];
+
+	rx_status = IEEE80211_SKB_RXCB(skb);
+	mgmt = (struct ieee80211_mgmt *) skb->data;
+	stype = le16_to_cpu(mgmt->frame_control) & IEEE80211_FCTL_STYPE;
+
+	if (stype != IEEE80211_STYPE_BEACON)
+		return;
+
+	baselen = (u8 *) mgmt->u.probe_resp.variable - (u8 *) mgmt;
+	if (baselen > skb->len)
+		return;
+
+	ieee802_11_parse_elems(mgmt->u.probe_resp.variable,
+			       skb->len - baselen, &elems);
+
+	rates = ieee80211_sta_get_rates(local, &elems, band, NULL);
+
+	rcu_read_lock();
+
+	sta = sta_info_get(sdata, sdata->u.wds.remote_addr);
+
+	if (!sta) {
+		rcu_read_unlock();
+		sta = sta_info_alloc(sdata, sdata->u.wds.remote_addr,
+				     GFP_KERNEL);
+		if (!sta)
+			return;
+
+		new = true;
+	}
+
+	sta->last_rx = jiffies;
+	sta->sta.supp_rates[local->hw.conf.channel->band] = rates;
+
+	if (elems.ht_cap_elem)
+		ieee80211_ht_cap_ie_to_sta_ht_cap(sdata, sband,
+				elems.ht_cap_elem, &sta->sta.ht_cap);
+
+	if (elems.wmm_param)
+		set_sta_flag(sta, WLAN_STA_WME);
+
+	if (new) {
+		sta_info_pre_move_state(sta, IEEE80211_STA_AUTH);
+		sta_info_pre_move_state(sta, IEEE80211_STA_ASSOC);
+		sta_info_pre_move_state(sta, IEEE80211_STA_AUTHORIZED);
+		rate_control_rate_init(sta);
+		sta_info_insert_rcu(sta);
+	}
+
+	rcu_read_unlock();
+}
+
 static void ieee80211_iface_work(struct work_struct *work)
 {
 	struct ieee80211_sub_if_data *sdata =
@@ -952,6 +997,9 @@ static void ieee80211_iface_work(struct 
 				break;
 			ieee80211_mesh_rx_queued_mgmt(sdata, skb);
 			break;
+		case NL80211_IFTYPE_WDS:
+			ieee80211_wds_rx_queued_mgmt(sdata, skb);
+			break;
 		default:
 			WARN(1, "frame for unexpected interface type");
 			break;
--- a/net/mac80211/rx.c
+++ b/net/mac80211/rx.c
@@ -2284,6 +2284,7 @@ ieee80211_rx_h_action(struct ieee80211_r
 		    sdata->vif.type != NL80211_IFTYPE_MESH_POINT &&
 		    sdata->vif.type != NL80211_IFTYPE_AP_VLAN &&
 		    sdata->vif.type != NL80211_IFTYPE_AP &&
+		    sdata->vif.type != NL80211_IFTYPE_WDS &&
 		    sdata->vif.type != NL80211_IFTYPE_ADHOC)
 			break;
 
@@ -2498,14 +2499,15 @@ ieee80211_rx_h_mgmt(struct ieee80211_rx_
 
 	if (!ieee80211_vif_is_mesh(&sdata->vif) &&
 	    sdata->vif.type != NL80211_IFTYPE_ADHOC &&
-	    sdata->vif.type != NL80211_IFTYPE_STATION)
+	    sdata->vif.type != NL80211_IFTYPE_STATION &&
+	    sdata->vif.type != NL80211_IFTYPE_WDS)
 		return RX_DROP_MONITOR;
 
 	switch (stype) {
 	case cpu_to_le16(IEEE80211_STYPE_AUTH):
 	case cpu_to_le16(IEEE80211_STYPE_BEACON):
 	case cpu_to_le16(IEEE80211_STYPE_PROBE_RESP):
-		/* process for all: mesh, mlme, ibss */
+		/* process for all: mesh, mlme, ibss, wds */
 		break;
 	case cpu_to_le16(IEEE80211_STYPE_ASSOC_RESP):
 	case cpu_to_le16(IEEE80211_STYPE_REASSOC_RESP):
@@ -2839,10 +2841,16 @@ static int prepare_for_handlers(struct i
 		}
 		break;
 	case NL80211_IFTYPE_WDS:
-		if (bssid || !ieee80211_is_data(hdr->frame_control))
-			return 0;
 		if (compare_ether_addr(sdata->u.wds.remote_addr, hdr->addr2))
 			return 0;
+
+		if (ieee80211_is_data(hdr->frame_control) ||
+		    ieee80211_is_action(hdr->frame_control)) {
+			if (compare_ether_addr(sdata->vif.addr, hdr->addr1))
+				return 0;
+		} else if (!ieee80211_is_beacon(hdr->frame_control))
+			return 0;
+
 		break;
 	default:
 		/* should never get here */
--- a/net/mac80211/sta_info.h
+++ b/net/mac80211/sta_info.h
@@ -32,7 +32,6 @@
  * @WLAN_STA_SHORT_PREAMBLE: Station is capable of receiving short-preamble
  *	frames.
  * @WLAN_STA_WME: Station is a QoS-STA.
- * @WLAN_STA_WDS: Station is one of our WDS peers.
  * @WLAN_STA_CLEAR_PS_FILT: Clear PS filter in hardware (using the
  *	IEEE80211_TX_CTL_CLEAR_PS_FILT control flag) when the next
  *	frame to this station is transmitted.
@@ -64,7 +63,6 @@ enum ieee80211_sta_info_flags {
 	WLAN_STA_AUTHORIZED,
 	WLAN_STA_SHORT_PREAMBLE,
 	WLAN_STA_WME,
-	WLAN_STA_WDS,
 	WLAN_STA_CLEAR_PS_FILT,
 	WLAN_STA_MFP,
 	WLAN_STA_BLOCK_BA,
--- a/net/mac80211/util.c
+++ b/net/mac80211/util.c
@@ -804,7 +804,7 @@ void ieee80211_set_wmm_default(struct ie
 	struct ieee80211_local *local = sdata->local;
 	struct ieee80211_tx_queue_params qparam;
 	int ac;
-	bool use_11b;
+	bool use_11b, enable_qos;
 	int aCWmin, aCWmax;
 
 	if (!local->ops->conf_tx)
@@ -818,6 +818,13 @@ void ieee80211_set_wmm_default(struct ie
 	use_11b = (local->hw.conf.channel->band == IEEE80211_BAND_2GHZ) &&
 		 !(sdata->flags & IEEE80211_SDATA_OPERATING_GMODE);
 
+	/*
+	 * By default disable QoS in STA mode for old access points, which do
+	 * not support 802.11e. New APs will provide proper queue parameters,
+	 * that we will configure later.
+	 */
+	enable_qos = (sdata->vif.type != NL80211_IFTYPE_STATION);
+
 	for (ac = 0; ac < IEEE80211_NUM_ACS; ac++) {
 		/* Set defaults according to 802.11-2007 Table 7-37 */
 		aCWmax = 1023;
@@ -826,38 +833,47 @@ void ieee80211_set_wmm_default(struct ie
 		else
 			aCWmin = 15;
 
-		switch (ac) {
-		case IEEE80211_AC_BK:
-			qparam.cw_max = aCWmax;
-			qparam.cw_min = aCWmin;
-			qparam.txop = 0;
-			qparam.aifs = 7;
-			break;
-		default: /* never happens but let's not leave undefined */
-		case IEEE80211_AC_BE:
+		if (enable_qos) {
+			switch (ac) {
+			case IEEE80211_AC_BK:
+				qparam.cw_max = aCWmax;
+				qparam.cw_min = aCWmin;
+				qparam.txop = 0;
+				qparam.aifs = 7;
+				break;
+			/* never happens but let's not leave undefined */
+			default:
+			case IEEE80211_AC_BE:
+				qparam.cw_max = aCWmax;
+				qparam.cw_min = aCWmin;
+				qparam.txop = 0;
+				qparam.aifs = 3;
+				break;
+			case IEEE80211_AC_VI:
+				qparam.cw_max = aCWmin;
+				qparam.cw_min = (aCWmin + 1) / 2 - 1;
+				if (use_11b)
+					qparam.txop = 6016/32;
+				else
+					qparam.txop = 3008/32;
+				qparam.aifs = 2;
+				break;
+			case IEEE80211_AC_VO:
+				qparam.cw_max = (aCWmin + 1) / 2 - 1;
+				qparam.cw_min = (aCWmin + 1) / 4 - 1;
+				if (use_11b)
+					qparam.txop = 3264/32;
+				else
+					qparam.txop = 1504/32;
+				qparam.aifs = 2;
+				break;
+			}
+		} else {
+			/* Confiure old 802.11b/g medium access rules. */
 			qparam.cw_max = aCWmax;
 			qparam.cw_min = aCWmin;
 			qparam.txop = 0;
-			qparam.aifs = 3;
-			break;
-		case IEEE80211_AC_VI:
-			qparam.cw_max = aCWmin;
-			qparam.cw_min = (aCWmin + 1) / 2 - 1;
-			if (use_11b)
-				qparam.txop = 6016/32;
-			else
-				qparam.txop = 3008/32;
 			qparam.aifs = 2;
-			break;
-		case IEEE80211_AC_VO:
-			qparam.cw_max = (aCWmin + 1) / 2 - 1;
-			qparam.cw_min = (aCWmin + 1) / 4 - 1;
-			if (use_11b)
-				qparam.txop = 3264/32;
-			else
-				qparam.txop = 1504/32;
-			qparam.aifs = 2;
-			break;
 		}
 
 		qparam.uapsd = false;
@@ -866,12 +882,8 @@ void ieee80211_set_wmm_default(struct ie
 		drv_conf_tx(local, sdata, ac, &qparam);
 	}
 
-	/* after reinitialize QoS TX queues setting to default,
-	 * disable QoS at all */
-
 	if (sdata->vif.type != NL80211_IFTYPE_MONITOR) {
-		sdata->vif.bss_conf.qos =
-			sdata->vif.type != NL80211_IFTYPE_STATION;
+		sdata->vif.bss_conf.qos = enable_qos;
 		if (bss_notify)
 			ieee80211_bss_info_change_notify(sdata,
 							 BSS_CHANGED_QOS);
--- a/drivers/net/wireless/ath/ath9k/beacon.c
+++ b/drivers/net/wireless/ath/ath9k/beacon.c
@@ -48,7 +48,10 @@ int ath_beaconq_config(struct ath_softc 
 		txq = sc->tx.txq_map[WME_AC_BE];
 		ath9k_hw_get_txq_props(ah, txq->axq_qnum, &qi_be);
 		qi.tqi_aifs = qi_be.tqi_aifs;
-		qi.tqi_cwmin = 4*qi_be.tqi_cwmin;
+		if (ah->slottime == ATH9K_SLOT_TIME_20)
+			qi.tqi_cwmin = 2*qi_be.tqi_cwmin;
+		else
+			qi.tqi_cwmin = 4*qi_be.tqi_cwmin;
 		qi.tqi_cwmax = qi_be.tqi_cwmax;
 	}
 
--- a/net/mac80211/mlme.c
+++ b/net/mac80211/mlme.c
@@ -1220,6 +1220,22 @@ static void ieee80211_sta_wmm_params(str
 	sdata->vif.bss_conf.qos = true;
 }
 
+static void __ieee80211_stop_poll(struct ieee80211_sub_if_data *sdata)
+{
+	lockdep_assert_held(&sdata->local->mtx);
+
+	sdata->u.mgd.flags &= ~(IEEE80211_STA_CONNECTION_POLL |
+				IEEE80211_STA_BEACON_POLL);
+	ieee80211_run_deferred_scan(sdata->local);
+}
+
+static void ieee80211_stop_poll(struct ieee80211_sub_if_data *sdata)
+{
+	mutex_lock(&sdata->local->mtx);
+	__ieee80211_stop_poll(sdata);
+	mutex_unlock(&sdata->local->mtx);
+}
+
 static u32 ieee80211_handle_bss_capability(struct ieee80211_sub_if_data *sdata,
 					   u16 capab, bool erp_valid, u8 erp)
 {
@@ -1285,8 +1301,7 @@ static void ieee80211_set_associated(str
 	sdata->u.mgd.flags |= IEEE80211_STA_RESET_SIGNAL_AVE;
 
 	/* just to be sure */
-	sdata->u.mgd.flags &= ~(IEEE80211_STA_CONNECTION_POLL |
-				IEEE80211_STA_BEACON_POLL);
+	ieee80211_stop_poll(sdata);
 
 	ieee80211_led_assoc(local, 1);
 
@@ -1456,8 +1471,7 @@ static void ieee80211_reset_ap_probe(str
 		return;
 	}
 
-	ifmgd->flags &= ~(IEEE80211_STA_CONNECTION_POLL |
-			  IEEE80211_STA_BEACON_POLL);
+	__ieee80211_stop_poll(sdata);
 
 	mutex_lock(&local->iflist_mtx);
 	ieee80211_recalc_ps(local, -1);
@@ -1477,7 +1491,6 @@ static void ieee80211_reset_ap_probe(str
 		  round_jiffies_up(jiffies +
 				   IEEE80211_CONNECTION_IDLE_TIME));
 out:
-	ieee80211_run_deferred_scan(local);
 	mutex_unlock(&local->mtx);
 }
 
@@ -2413,7 +2426,11 @@ static void ieee80211_rx_mgmt_beacon(str
 			       "to a received beacon\n", sdata->name);
 		}
 #endif
+		mutex_lock(&local->mtx);
 		ifmgd->flags &= ~IEEE80211_STA_BEACON_POLL;
+		ieee80211_run_deferred_scan(local);
+		mutex_unlock(&local->mtx);
+
 		mutex_lock(&local->iflist_mtx);
 		ieee80211_recalc_ps(local, -1);
 		mutex_unlock(&local->iflist_mtx);
@@ -2600,8 +2617,7 @@ static void ieee80211_sta_connection_los
 	struct ieee80211_if_managed *ifmgd = &sdata->u.mgd;
 	u8 frame_buf[DEAUTH_DISASSOC_LEN];
 
-	ifmgd->flags &= ~(IEEE80211_STA_CONNECTION_POLL |
-			  IEEE80211_STA_BEACON_POLL);
+	ieee80211_stop_poll(sdata);
 
 	ieee80211_set_disassoc(sdata, IEEE80211_STYPE_DEAUTH, reason,
 			       false, frame_buf);
@@ -2879,8 +2895,7 @@ static void ieee80211_restart_sta_timer(
 	u32 flags;
 
 	if (sdata->vif.type == NL80211_IFTYPE_STATION) {
-		sdata->u.mgd.flags &= ~(IEEE80211_STA_BEACON_POLL |
-					IEEE80211_STA_CONNECTION_POLL);
+		__ieee80211_stop_poll(sdata);
 
 		/* let's probe the connection once */
 		flags = sdata->local->hw.flags;
@@ -2949,7 +2964,10 @@ void ieee80211_sta_restart(struct ieee80
 	if (test_and_clear_bit(TMR_RUNNING_CHANSW, &ifmgd->timers_running))
 		add_timer(&ifmgd->chswitch_timer);
 	ieee80211_sta_reset_beacon_monitor(sdata);
+
+	mutex_lock(&sdata->local->mtx);
 	ieee80211_restart_sta_timer(sdata);
+	mutex_unlock(&sdata->local->mtx);
 }
 #endif
 
