From cfcc8526e97bdcbfcbf945246b878262389b8842 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Wed, 25 Jan 2012 17:39:59 +0100
Subject: [PATCH 17/63] MIPS: BCM63XX: add RNG driver platform_device stub

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
 arch/mips/bcm63xx/Makefile   |    4 ++--
 arch/mips/bcm63xx/dev-trng.c |   40 ++++++++++++++++++++++++++++++++++++++++
 2 files changed, 42 insertions(+), 2 deletions(-)
 create mode 100644 arch/mips/bcm63xx/dev-trng.c

--- a/arch/mips/bcm63xx/Makefile
+++ b/arch/mips/bcm63xx/Makefile
@@ -1,6 +1,6 @@
 obj-y		+= clk.o cpu.o cs.o gpio.o irq.o prom.o setup.o timer.o \
-		   dev-dsp.o dev-enet.o dev-pcmcia.o dev-spi.o dev-uart.o \
-		   dev-wdt.o
+		   dev-dsp.o dev-enet.o dev-pcmcia.o dev-spi.o dev-trng.o \
+		   dev-uart.o dev-wdt.o
 obj-$(CONFIG_EARLY_PRINTK)	+= early_printk.o
 
 obj-y		+= boards/
--- /dev/null
+++ b/arch/mips/bcm63xx/dev-trng.c
@@ -0,0 +1,40 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 2011 Florian Fainelli <florian@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <linux/platform_device.h>
+#include <bcm63xx_cpu.h>
+
+static struct resource trng_resources[] = {
+	{
+		.start		= -1, /* filled at runtime */
+		.end		= -1, /* filled at runtime */
+		.flags		= IORESOURCE_MEM,
+	},
+};
+
+static struct platform_device bcm63xx_trng_device = {
+	.name		= "bcm63xx-trng",
+	.id		= -1,
+	.num_resources	= ARRAY_SIZE(trng_resources),
+	.resource	= trng_resources,
+};
+
+int __init bcm63xx_trng_register(void)
+{
+	if (!BCMCPU_IS_6368())
+		return -ENODEV;
+
+	trng_resources[0].start = bcm63xx_regset_address(RSET_TRNG);
+	trng_resources[0].end = trng_resources[0].start;
+	trng_resources[0].end += RSET_TRNG_SIZE - 1;
+
+	return platform_device_register(&bcm63xx_trng_device);
+}
+arch_initcall(bcm63xx_trng_register);
