--- a/drivers/net/wireless/brcm80211/brcmsmac/main.c
+++ b/drivers/net/wireless/brcm80211/brcmsmac/main.c
@@ -1943,7 +1943,8 @@ static bool brcms_b_radio_read_hwdisable
 		 * accesses phyreg throughput mac. This can be skipped since
 		 * only mac reg is accessed below
 		 */
-		flags |= SICF_PCLKE;
+		if (D11REV_GE(wlc_hw->corerev, 18))
+			flags |= SICF_PCLKE;
 
 		/*
 		 * TODO: test suspend/resume
@@ -2024,7 +2025,8 @@ void brcms_b_corereset(struct brcms_hard
 	 * phyreg throughput mac, AND phy_reset is skipped at early stage when
 	 * band->pi is invalid. need to enable PHY CLK
 	 */
-	flags |= SICF_PCLKE;
+	if (D11REV_GE(wlc_hw->corerev, 18))
+		flags |= SICF_PCLKE;
 
 	/*
 	 * reset the core
--- a/drivers/net/wireless/brcm80211/brcmsmac/phy/phy_n.c
+++ b/drivers/net/wireless/brcm80211/brcmsmac/phy/phy_n.c
@@ -17895,6 +17895,9 @@ static u32 *wlc_phy_get_ipa_gaintbl_nphy
 					nphy_tpc_txgain_ipa_2g_2057rev7;
 		} else if (NREV_IS(pi->pubpi.phy_rev, 6)) {
 			tx_pwrctrl_tbl = nphy_tpc_txgain_ipa_rev6;
+			if (pi->sh->chip == BCM47162_CHIP_ID) {
+				tx_pwrctrl_tbl = nphy_tpc_txgain_ipa_rev5;
+			}
 		} else if (NREV_IS(pi->pubpi.phy_rev, 5)) {
 			tx_pwrctrl_tbl = nphy_tpc_txgain_ipa_rev5;
 		} else {
@@ -19256,8 +19259,14 @@ static void wlc_phy_spurwar_nphy(struct
 			case 38:
 			case 102:
 			case 118:
-				nphy_adj_tone_id_buf[0] = 0;
-				nphy_adj_noise_var_buf[0] = 0x0;
+				if ((pi->sh->chip == BCM4716_CHIP_ID) &&
+				    (pi->sh->chippkg == BCM4717_PKG_ID)) {
+					nphy_adj_tone_id_buf[0] = 32;
+					nphy_adj_noise_var_buf[0] = 0x21f;
+				} else {
+					nphy_adj_tone_id_buf[0] = 0;
+					nphy_adj_noise_var_buf[0] = 0x0;
+				}
 				break;
 			case 134:
 				nphy_adj_tone_id_buf[0] = 32;
@@ -20697,12 +20706,22 @@ wlc_phy_chanspec_radio2056_setup(struct
 			write_radio_reg(pi, RADIO_2056_SYN_PLL_LOOPFILTER2 |
 					RADIO_2056_SYN, 0x1f);
 
-			write_radio_reg(pi,
-					RADIO_2056_SYN_PLL_LOOPFILTER4 |
-					RADIO_2056_SYN, 0xb);
-			write_radio_reg(pi,
-					RADIO_2056_SYN_PLL_CP2 |
-					RADIO_2056_SYN, 0x14);
+			if ((pi->sh->chip == BCM4716_CHIP_ID) ||
+			    (pi->sh->chip == BCM47162_CHIP_ID)) {
+				write_radio_reg(pi,
+						RADIO_2056_SYN_PLL_LOOPFILTER4 |
+						RADIO_2056_SYN, 0x14);
+				write_radio_reg(pi,
+						RADIO_2056_SYN_PLL_CP2 |
+						RADIO_2056_SYN, 0x00);
+			} else {
+				write_radio_reg(pi,
+						RADIO_2056_SYN_PLL_LOOPFILTER4 |
+						RADIO_2056_SYN, 0xb);
+				write_radio_reg(pi,
+						RADIO_2056_SYN_PLL_CP2 |
+						RADIO_2056_SYN, 0x14);
+			}
 		}
 	}
 
@@ -20749,24 +20768,33 @@ wlc_phy_chanspec_radio2056_setup(struct
 				WRITE_RADIO_REG2(pi, RADIO_2056, TX, core,
 						 PADG_IDAC, 0xcc);
 
-				bias = 0x25;
-				cascbias = 0x20;
+				if ((pi->sh->chip == BCM4716_CHIP_ID) ||
+				    (pi->sh->chip ==
+				     BCM47162_CHIP_ID)) {
+					bias = 0x40;
+					cascbias = 0x45;
+					pag_boost_tune = 0x5;
+					pgag_boost_tune = 0x33;
+					padg_boost_tune = 0x77;
+					mixg_boost_tune = 0x55;
+				} else {
+					bias = 0x25;
+					cascbias = 0x20;
 
-				if ((pi->sh->chip ==
-				     BCM43224_CHIP_ID)
-				    || (pi->sh->chip ==
-					BCM43225_CHIP_ID)) {
-					if (pi->sh->chippkg ==
-					    BCM43224_FAB_SMIC) {
-						bias = 0x2a;
-						cascbias = 0x38;
+					if ((pi->sh->chip == BCM43224_CHIP_ID)
+					    || (pi->sh->chip ==	BCM43225_CHIP_ID)) {
+						if (pi->sh->chippkg ==
+						    BCM43224_FAB_SMIC) {
+							bias = 0x2a;
+							cascbias = 0x38;
+						}
 					}
-				}
 
-				pag_boost_tune = 0x4;
-				pgag_boost_tune = 0x03;
-				padg_boost_tune = 0x77;
-				mixg_boost_tune = 0x65;
+					pag_boost_tune = 0x4;
+					pgag_boost_tune = 0x03;
+					padg_boost_tune = 0x77;
+					mixg_boost_tune = 0x65;
+				}
 
 				WRITE_RADIO_REG2(pi, RADIO_2056, TX, core,
 						 INTPAG_IMAIN_STAT, bias);
@@ -21180,19 +21208,27 @@ wlc_phy_chanspec_nphy_setup(struct brcms
 		} else if (NREV_GE(pi->pubpi.phy_rev, 7)) {
 			if (val == 54)
 				spuravoid = 1;
-		} else {
-			if (pi->nphy_aband_spurwar_en &&
-			    ((val == 38) || (val == 102)
-			     || (val == 118)))
+		} else if (pi->nphy_aband_spurwar_en &&
+			    ((val == 38) || (val == 102) || (val == 118))) {
+			if ((pi->sh->chip == BCM4716_CHIP_ID)
+			    && (pi->sh->chippkg == BCM4717_PKG_ID)) {
+				spuravoid = 0;
+			} else {
 				spuravoid = 1;
+			}
 		}
 
 		if (pi->phy_spuravoid == SPURAVOID_FORCEON)
 			spuravoid = 1;
 
-		wlapi_bmac_core_phypll_ctl(pi->sh->physhim, false);
-		si_pmu_spuravoid_pllupdate(pi->sh->sih, spuravoid);
-		wlapi_bmac_core_phypll_ctl(pi->sh->physhim, true);
+		if ((pi->sh->chip == BCM4716_CHIP_ID) ||
+		    (pi->sh->chip == BCM47162_CHIP_ID)) {
+			si_pmu_spuravoid_pllupdate(pi->sh->sih, spuravoid);
+		} else {
+			wlapi_bmac_core_phypll_ctl(pi->sh->physhim, false);
+			si_pmu_spuravoid_pllupdate(pi->sh->sih, spuravoid);
+			wlapi_bmac_core_phypll_ctl(pi->sh->physhim, true);
+		}
 
 		if ((pi->sh->chip == BCM43224_CHIP_ID) ||
 		    (pi->sh->chip == BCM43225_CHIP_ID)) {
@@ -21211,7 +21247,10 @@ wlc_phy_chanspec_nphy_setup(struct brcms
 			}
 		}
 
-		wlapi_bmac_core_phypll_reset(pi->sh->physhim);
+		if (!((pi->sh->chip == BCM4716_CHIP_ID) ||
+		      (pi->sh->chip == BCM47162_CHIP_ID))) {
+			wlapi_bmac_core_phypll_reset(pi->sh->physhim);
+		}
 
 		mod_phy_reg(pi, 0x01, (0x1 << 15),
 			    ((spuravoid > 0) ? (0x1 << 15) : 0));
@@ -24925,14 +24964,20 @@ wlc_phy_a2_nphy(struct brcms_phy *pi, st
 			if (txgains->useindex) {
 				phy_a4 = 15 - ((txgains->index) >> 3);
 				if (CHSPEC_IS2G(pi->radio_chanspec)) {
-					if (NREV_GE(pi->pubpi.phy_rev, 6))
+					if (NREV_GE(pi->pubpi.phy_rev, 6)) {
 						phy_a5 = 0x00f7 | (phy_a4 << 8);
-
-					else
-					if (NREV_IS(pi->pubpi.phy_rev, 5))
+						if (pi->sh->chip ==
+						    BCM47162_CHIP_ID) {
+							phy_a5 =
+							    0x10f7 | (phy_a4 <<
+								      8);
+						}
+					} else
+					if (NREV_IS(pi->pubpi.phy_rev, 5)) {
 						phy_a5 = 0x10f7 | (phy_a4 << 8);
-					else
+					} else {
 						phy_a5 = 0x50f7 | (phy_a4 << 8);
+					}
 				} else {
 					phy_a5 = 0x70f7 | (phy_a4 << 8);
 				}
