From 902b348cdddd4c858993e02aced615aa6caf04d0 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Wed, 14 Mar 2012 10:45:30 +0100
Subject: [PATCH 35/47] MIPS: ath79: add PCI registration code for AR934X

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
Acked-by: Luis R. Rodriguez <mcgrof@qca.qualcomm.com>
Cc: linux-mips@linux-mips.org
Cc: mcgrof@infradead.org
Patchwork: https://patchwork.linux-mips.org/patch/3516/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ath79/Kconfig |    2 ++
 arch/mips/ath79/pci.c   |   13 ++++++++++++-
 2 files changed, 14 insertions(+), 1 deletions(-)

--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -72,6 +72,8 @@ config SOC_AR933X
 
 config SOC_AR934X
 	select USB_ARCH_HAS_EHCI
+	select HW_HAS_PCI
+	select PCI_AR724X if PCI
 	def_bool n
 
 config PCI_AR724X
--- a/arch/mips/ath79/pci.c
+++ b/arch/mips/ath79/pci.c
@@ -14,6 +14,7 @@
 
 #include <linux/init.h>
 #include <linux/pci.h>
+#include <asm/mach-ath79/ar71xx_regs.h>
 #include <asm/mach-ath79/ath79.h>
 #include <asm/mach-ath79/irq.h>
 #include <asm/mach-ath79/pci.h>
@@ -57,7 +58,9 @@ int __init pcibios_map_irq(const struct
 		if (soc_is_ar71xx()) {
 			ath79_pci_irq_map = ar71xx_pci_irq_map;
 			ath79_pci_nr_irqs = ARRAY_SIZE(ar71xx_pci_irq_map);
-		} else if (soc_is_ar724x()) {
+		} else if (soc_is_ar724x() ||
+			   soc_is_ar9342() ||
+			   soc_is_ar9344()) {
 			ath79_pci_irq_map = ar724x_pci_irq_map;
 			ath79_pci_nr_irqs = ARRAY_SIZE(ar724x_pci_irq_map);
 		} else {
@@ -115,5 +118,13 @@ int __init ath79_register_pci(void)
 	if (soc_is_ar724x())
 		return ar724x_pcibios_init(ATH79_CPU_IRQ_IP2);
 
+	if (soc_is_ar9342() || soc_is_ar9344()) {
+		u32 bootstrap;
+
+		bootstrap = ath79_reset_rr(AR934X_RESET_REG_BOOTSTRAP);
+		if (bootstrap & AR934X_BOOTSTRAP_PCIE_RC)
+			return ar724x_pcibios_init(ATH79_IP2_IRQ(0));
+	}
+
 	return -ENODEV;
 }
