From c02c17b2d2bd9663ded7e9f59d6ef24fba239b33 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 12 Mar 2012 15:23:39 +0100
Subject: [PATCH 34/70] MIPS: lantiq: add additional soc ids

---
 .../mips/include/asm/mach-lantiq/xway/lantiq_soc.h |   38 +++++++++++++++----
 arch/mips/lantiq/xway/prom.c                       |   35 ++++++++++++++++--
 2 files changed, 61 insertions(+), 12 deletions(-)

--- a/arch/mips/include/asm/mach-lantiq/xway/lantiq_soc.h
+++ b/arch/mips/include/asm/mach-lantiq/xway/lantiq_soc.h
@@ -17,20 +17,32 @@
 #define SOC_ID_DANUBE1		0x129
 #define SOC_ID_DANUBE2		0x12B
 #define SOC_ID_TWINPASS		0x12D
-#define SOC_ID_AMAZON_SE	0x152
+#define SOC_ID_AMAZON_SE_1	0x152 /* 50601 */
+#define SOC_ID_AMAZON_SE_2	0x153 /* 50600 */
 #define SOC_ID_ARX188		0x16C
-#define SOC_ID_ARX168		0x16D
+#define SOC_ID_ARX168_1		0x16D
+#define SOC_ID_ARX168_2		0x16E
 #define SOC_ID_ARX182		0x16F
-#define SOC_ID_VRX288		0x1C0 /* VRX288 v1.1 */
-#define SOC_ID_VRX268		0x1C2 /* VRX268 v1.1 */
-#define SOC_ID_GRX288		0x1C9 /* GRX288 v1.1 */
+#define SOC_ID_GRX188		0x170
+#define SOC_ID_GRX168		0x171
+
+#define SOC_ID_VRX288		0x1C0 /* v1.1 */
+#define SOC_ID_VRX282		0x1C1 /* v1.1 */
+#define SOC_ID_VRX268		0x1C2 /* v1.1 */
+#define SOC_ID_GRX268		0x1C8 /* v1.1 */
+#define SOC_ID_GRX288		0x1C9 /* v1.1 */
+#define SOC_ID_VRX288_2		0x00B /* v1.2 */
+#define SOC_ID_VRX268_2		0x00C /* v1.2 */
+#define SOC_ID_GRX288_2		0x00D /* v1.2 */
+#define SOC_ID_GRX282_2		0x00E /* v1.2 */
 
 /* SoC Types */
 #define SOC_TYPE_DANUBE		0x01
 #define SOC_TYPE_TWINPASS	0x02
 #define SOC_TYPE_AR9		0x03
-#define SOC_TYPE_VR9		0x04
-#define SOC_TYPE_AMAZON_SE	0x05
+#define SOC_TYPE_VR9_1		0x04 /* v1.1 */
+#define SOC_TYPE_VR9_2		0x05 /* v1.2 */
+#define SOC_TYPE_AMAZON_SE	0x06
 
 /* ASC0/1 - serial port */
 #define LTQ_ASC0_BASE_ADDR	0x1E100400
@@ -149,9 +161,19 @@ static inline int ltq_is_ar9(void)
 	return (ltq_get_soc_type() == SOC_TYPE_AR9);
 }
 
+static inline int ltq_is_vr9_1(void)
+{
+	return (ltq_get_soc_type() == SOC_TYPE_VR9_1);
+}
+
+static inline int ltq_is_vr9_2(void)
+{
+	return (ltq_get_soc_type() == SOC_TYPE_VR9_2);
+}
+
 static inline int ltq_is_vr9(void)
 {
-	return (ltq_get_soc_type() == SOC_TYPE_VR9);
+	return (ltq_is_vr9_1() || ltq_is_vr9_2());
 }
 
 static inline int ltq_is_falcon(void)
--- a/arch/mips/lantiq/xway/prom.c
+++ b/arch/mips/lantiq/xway/prom.c
@@ -18,7 +18,9 @@
 
 #define SOC_DANUBE	"Danube"
 #define SOC_TWINPASS	"Twinpass"
+#define SOC_AMAZON_SE	"Amazon_SE"
 #define SOC_AR9		"AR9"
+#define SOC_GR9		"GR9"
 #define SOC_VR9		"VR9"
 
 #define PART_SHIFT	12
@@ -26,7 +28,6 @@
 #define REV_SHIFT	28
 #define REV_MASK	0xF0000000
 
-#define SOC_AMAZON_SE	"Amazon_SE"
 
 void __init ltq_soc_detect(struct ltq_soc_info *i)
 {
@@ -46,13 +47,21 @@ void __init ltq_soc_detect(struct ltq_so
 		break;
 
 	case SOC_ID_ARX188:
-	case SOC_ID_ARX168:
+	case SOC_ID_ARX168_1:
+	case SOC_ID_ARX168_2:
 	case SOC_ID_ARX182:
 		i->name = SOC_AR9;
 		i->type = SOC_TYPE_AR9;
 		break;
 
-	case SOC_ID_AMAZON_SE:
+	case SOC_ID_GRX188:
+	case SOC_ID_GRX168:
+		i->name = SOC_GR9;
+		i->type = SOC_TYPE_AR9;
+		break;
+
+	case SOC_ID_AMAZON_SE_1:
+	case SOC_ID_AMAZON_SE_2:
 		i->name = SOC_AMAZON_SE;
 		i->type = SOC_TYPE_AMAZON_SE;
 #ifdef CONFIG_PCI
@@ -60,12 +69,30 @@ void __init ltq_soc_detect(struct ltq_so
 #endif
 		break;
 
+	case SOC_ID_VRX282:
 	case SOC_ID_VRX268:
 	case SOC_ID_VRX288:
 		i->name = SOC_VR9;
-		i->type = SOC_TYPE_VR9;
+		i->type = SOC_TYPE_VR9_1;
 		break;
 
+	case SOC_ID_GRX268:
+	case SOC_ID_GRX288:
+		i->name = SOC_GR9;
+		i->type = SOC_TYPE_VR9_1;
+		break;
+
+	case SOC_ID_VRX268_2:
+	case SOC_ID_VRX288_2:
+		i->name = SOC_VR9;
+		i->type = SOC_TYPE_VR9_2;
+		break;
+
+	case SOC_ID_GRX282_2:
+	case SOC_ID_GRX288_2:
+		i->name = SOC_GR9;
+		i->type = SOC_TYPE_VR9_2;
+
 	default:
 		unreachable();
 		break;
