From 79b1ef832e3e73af4ec6c506ce01f8666d4c92bb Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 19 Aug 2016 11:12:28 +0100
Subject: [PATCH] BCM270X_DT: Add audio_pins to CM dtb

Bring the CM .dtb in line with other others.
---
 arch/arm/boot/dts/bcm2708-rpi-cm.dts | 5 +++++
 1 file changed, 5 insertions(+)

--- a/arch/arm/boot/dts/bcm2708-rpi-cm.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dts
@@ -35,6 +35,11 @@
 		brcm,pins = <18 19 20 21>;
 		brcm,function = <4>; /* alt0 */
 	};
+
+	audio_pins: audio_pins {
+		brcm,pins;
+		brcm,function;
+	};
 };
 
 &spi0 {
