From 57d949256241fb79b669bbca0426c2d74a3dfc6e Mon Sep 17 00:00:00 2001
From: Shaohui Xie <Shaohui.Xie@freescale.com>
Date: Fri, 8 Jul 2016 10:27:39 +0800
Subject: [PATCH 02/70] dts/ls1043a: add LS1043ARDB board support

commit 9a6fce16a82d3412c9350b9f08eacebaa81c0a3d
[context adjustment]

Signed-off-by: Shaohui Xie <Shaohui.Xie@freescale.com>
Signed-off-by: Mingkai Hu <Mingkai.Hu@freescale.com>
Signed-off-by: Wenbin Song <Wenbin.Song@freescale.com>
Signed-off-by: Hou Zhiqiang <B48286@freescale.com>
Signed-off-by: Mingkai Hu <mingkai.hu@nxp.com>
Integrated-by: Zhao Qiang <qiang.zhao@nxp.com>
---
 arch/arm64/boot/dts/freescale/Makefile            |    1 +
 arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts |  117 +++++++++++++++++++++
 2 files changed, 118 insertions(+)
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts

--- a/arch/arm64/boot/dts/freescale/Makefile
+++ b/arch/arm64/boot/dts/freescale/Makefile
@@ -1,6 +1,7 @@
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2080a-qds.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2080a-rdb.dtb
 dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls2080a-simu.dtb
+dtb-$(CONFIG_ARCH_LAYERSCAPE) += fsl-ls1043a-rdb.dtb
  
 always		:= $(dtb-y)
 subdir-y	:= $(dts-dirs)
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
@@ -0,0 +1,117 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1043A family SoC.
+ *
+ * Copyright 2014-2015, Freescale Semiconductor
+ *
+ * Mingkai Hu <Mingkai.hu@freescale.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "fsl-ls1043a.dtsi"
+
+/ {
+	model = "LS1043A RDB Board";
+	compatible = "fsl,ls1043a-rdb", "fsl,ls1043a";
+};
+
+&i2c0 {
+	status = "okay";
+	ina220@40 {
+		compatible = "ti,ina220";
+		reg = <0x40>;
+		shunt-resistor = <1000>;
+	};
+	adt7461a@4c {
+		compatible = "adi,adt7461";
+		reg = <0x4c>;
+	};
+	eeprom@56 {
+		compatible = "at24,24c512";
+		reg = <0x52>;
+	};
+	eeprom@57 {
+		compatible = "at24,24c512";
+		reg = <0x53>;
+	};
+	rtc@68 {
+		compatible = "pericom,pt7c4338";
+		reg = <0x68>;
+	};
+};
+
+&ifc {
+	status = "okay";
+	#address-cells = <2>;
+	#size-cells = <1>;
+	/* NOR, NAND Flashes and FPGA on board */
+	ranges = <0x0 0x0 0x0 0x60000000 0x08000000
+		  0x1 0x0 0x0 0x7e800000 0x00010000
+		  0x2 0x0 0x0 0x7fb00000 0x00000100>;
+
+		nor@0,0 {
+			compatible = "cfi-flash";
+			#address-cells = <1>;
+			#size-cells = <1>;
+			reg = <0x0 0x0 0x8000000>;
+			bank-width = <2>;
+			device-width = <1>;
+		};
+
+		nand@1,0 {
+			compatible = "fsl,ifc-nand";
+			#address-cells = <1>;
+			#size-cells = <1>;
+			reg = <0x1 0x0 0x10000>;
+		};
+
+		cpld: board-control@2,0 {
+			compatible = "fsl,ls1043ardb-cpld";
+			reg = <0x2 0x0 0x0000100>;
+		};
+};
+
+&duart0 {
+	status = "okay";
+};
+
+&duart1 {
+	status = "okay";
+};
