From c1ff5519a7fd849da5d169036d8175383f807962 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 11 Apr 2016 06:00:23 +0200
Subject: [PATCH 102/102] net: mediatek: v4.4 backports

---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |   13 ++++++++-----
 1 file changed, 8 insertions(+), 5 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -217,7 +217,7 @@ static int mtk_phy_connect_node(struct m
 
 	dev_info(eth->dev,
 		 "connected mac %d to PHY at %s [uid=%08x, driver=%s]\n",
-		 mac->id, phydev_name(phydev), phydev->phy_id,
+		 mac->id, dev_name(&phydev->dev), phydev->phy_id,
 		 phydev->drv->name);
 
 	mac->phy_dev = phydev;
@@ -1396,6 +1396,7 @@ static int mtk_stop(struct net_device *d
 	struct mtk_mac *mac = netdev_priv(dev);
 	struct mtk_eth *eth = mac->hw;
 
+	netif_carrier_off(dev);
 	netif_tx_disable(dev);
 	phy_stop(mac->phy_dev);
 
@@ -1595,11 +1596,13 @@ static int mtk_set_settings(struct net_d
 {
 	struct mtk_mac *mac = netdev_priv(dev);
 
-	if (cmd->phy_address != mac->phy_dev->mdio.addr) {
-		mac->phy_dev = mdiobus_get_phy(mac->hw->mii_bus,
-					       cmd->phy_address);
-		if (!mac->phy_dev)
+	if (cmd->phy_address != mac->phy_dev->addr) {
+		if (mac->hw->mii_bus->phy_map[cmd->phy_address]) {
+			mac->phy_dev =
+				mac->hw->mii_bus->phy_map[cmd->phy_address];
+		} else {
 			return -ENODEV;
+		}
 	}
 
 	return phy_ethtool_sset(mac->phy_dev, cmd);
