#!/bin/sh
#
# Copyright (C) 2011-2015 OpenWrt.org
#

. /lib/functions/system.sh
. /lib/functions/uci-defaults.sh
. /lib/ar71xx.sh

ar71xx_setup_interfaces()
{
	local board="$1"

	case "$board" in
	airgatewaypro)
		ucidef_add_switch "switch0" \
			"0@eth0" "4:lan" "5:wan"
		;;
	airrouter|\
	ap121|\
	ap121-mini|\
	ap96|\
	dir-600-a1|\
	dir-615-c1|\
	dir-615-e1|\
	dir-615-e4|\
	hiwifi-hc6361|\
	ja76pf|\
	mc-mac1200r|\
	minibox-v1|\
	mynet-n600|\
	oolite|\
	qihoo-c301|\
	rb-750|\
	rb-751|\
	som9331|\
	tew-632brp|\
	tew-712br|\
	tew-732br|\
	tl-mr3220|\
	tl-mr3220-v2|\
	tl-mr3420|\
	tl-wdr3320-v2|\
	tl-wdr3500|\
	tl-wr741nd-v4|\
	tl-wr841n-v11|\
	tl-wr841n-v9|\
	tl-wr842n-v3|\
	whr-g301n|\
	whr-hp-g300n|\
	whr-hp-gn|\
	wzr-hp-ag300h|\
	zbt-we1526)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	alfa-ap120c|\
	all0305|\
	antminer-s1|\
	antminer-s3|\
	antrouter-r1|\
	ap121f|\
	aw-nr580|\
	bullet-m|\
	c-55|\
	cap4200ag|\
	cf-e380ac-v1|\
	cf-e380ac-v2|\
	eap120|\
	eap300v2|\
	eap7660d|\
	el-mini|\
	loco-m-xw|\
	mr12|\
	mr16|\
	mr1750|\
	mr1750v2|\
	mr18|\
	mr600|\
	mr600v2|\
	mr900|\
	mr900v2|\
	mynet-rext|\
	rb-411|\
	rb-411u|\
	rb-911g-2hpnd|\
	rb-911g-5hpacd|\
	rb-911g-5hpnd|\
	rb-912uag-2hpnd|\
	rb-912uag-5hpnd|\
	rb-sxt2n|\
	rb-sxt5n|\
	re450|\
	rocket-m-xw|\
	tl-mr10u|\
	tl-mr11u|\
	tl-mr12u|\
	tl-mr13u|\
	tl-mr3020|\
	tl-mr3040|\
	tl-mr3040-v2|\
	tl-wa701nd-v2|\
	tl-wa7210n-v2|\
	tl-wa750re|\
	tl-wa801nd-v2|\
	tl-wa830re-v2|\
	tl-wa850re|\
	tl-wa901nd|\
	tl-wa901nd-v2|\
	tl-wa901nd-v3|\
	tl-wa901nd-v4|\
	tl-wr703n|\
	tl-wr802n-v1|\
	tube2h|\
	unifiac-lite|\
	wndap360|\
	wp543)
		ucidef_set_interface_lan "eth0"
		;;
	a40|\
	a60|\
	alfa-ap96|\
	alfa-nx|\
	dr344|\
	gl-ar150|\
	gl-ar300m|\
	gl-domino|\
	gl-inet|\
	gl-mifi|\
	jwap003|\
	om2pv4|\
	om2p-hsv4|\
	pb42|\
	pb44|\
	rb-951ui-2hnd|\
	routerstation|\
	tl-wr710n|\
	tl-wr720n-v3|\
	tl-wr810n|\
	wpe72|\
	wrtnode2q)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		;;
	rb-750-r2|\
	rb-750up-r2)
		ucidef_set_interfaces_lan_wan "eth1.1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	all0258n|\
	all0315n|\
	dlan-hotspot|\
	dlan-pro-500-wp|\
	ja76pf2|\
	rocket-m-ti|\
	ubnt-unifi-outdoor)
		ucidef_set_interface_lan "eth0 eth1"
		;;
	wzr-hp-g300nh2)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "3:lan:2" "4:lan:3" "5:lan:4" "2:wan"
		;;
	ap132|\
	ap136|\
	ap152|\
	rb-750gl|\
	rb-751g|\
	rb-951g-2hnd|\
	wlr8100|\
	wzr-hp-g450h)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan" "5:lan" "1:wan"
		;;
	ap135-020|\
	ap136-020|\
	bhr-4grv2|\
	tew-823dru|\
	tl-wr1043nd-v2|\
	wzr-450hp2)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan" "6@eth0"
		;;
	ap136-010|\
	ap147-010|\
	nbg6616|\
	nbg6716)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan" "6@eth1"
		;;
	ap143|\
	rb-433|\
	rb-433u)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "5@eth1"
		;;
	archer-c5|\
	archer-c7|\
	tl-wdr4900-v2)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "2:lan" "3:lan" "4:lan" "5:lan" "6@eth0" "1:wan"
		;;
	arduino-yun|\
	dir-505-a1|\
	tl-wa801nd-v3)
		ucidef_set_interface_lan "eth1"
		;;
	bsb)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan" "3:lan"
		;;
	c-60)
		ucidef_add_switch "switch0" \
			"0@eth0" "3:wan" "4:lan"
		;;
	cap324)
		ucidef_set_interface_lan "eth0" "dhcp"
		;;
	cpe210|\
	cpe510|\
	wbs210|\
	wbs510)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:lan" "4:wan"
		;;
	cr3000)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:4" "3:lan:3" "4:lan:2"
		;;
	cr5000|\
	dgl-5500-a1|\
	dhp-1565-a1|\
	dir-825-c1|\
	dir-835-a1|\
	esr900|\
	mynet-n750|\
	sr3200|\
	wndr3700v4|\
	wndr4300)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan"
		;;
	dap-2695-a1)
		ucidef_add_switch "switch0" "0@eth0" "2:lan" "3:wan" "6@eth1"
		;;
	rb-941-2nd)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:wan:1"
	;;
	db120|\
	rb-2011l|\
	rb-2011uas|\
	rb-2011uas-2hnd|\
	rb-2011uias|\
	rb-2011uias-2hnd)
		case "$board" in
		rb-2011uas*|\
		rb-2011uias|\
		rb-2011uias-2hnd)
			ucidef_add_switch "switch0" \
				"0@eth0" "2:lan" "3:lan" "4:lan" "5:lan" "1:wan" "6:sfp"
		;;
		*)
			ucidef_add_switch "switch0" \
				"0@eth0" "2:lan" "3:lan" "4:lan" "5:lan" "1:wan"
		;;
		esac

		ucidef_add_switch "switch1" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan" "5:lan"
		;;
	dir-615-i1|\
	omy-g1|\
	r6100|\
	smart-300|\
	tl-mr3420-v2|\
	tl-wdr6500-v2|\
	tl-wr841n-v8|\
	tl-wr940n-v4|\
	tl-wr941nd-v5|\
	tl-wr941nd-v6|\
	wnr1000-v2|\
	wnr2000-v4|\
	wnr2200|\
	wnr612-v2|\
	wpn824n)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "4@eth1"
		;;
	dir-825-b1|\
	nbg460n_550n_550nh|\
	tew-673gru|\
	wzr-hp-g300nh)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "5@eth0"
		;;
	dlan-pro-1200-ac)
		ucidef_set_interface_lan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan"
		ucidef_add_switch_attr "switch0" "enable" "false"
		;;
	el-m150)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "3@eth1"
		;;
	dir-869-a1|\
	epg5000|\
	esr1750|\
	tl-wr1043nd-v4)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan"
		;;
	ew-dorin)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:wan"
		;;
	ew-dorin-router)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan"
		;;
	dw33d|\
	f9k1115v2)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"2:lan" "3:lan" "4:lan" "5:lan" "6@eth1" "0@eth0" "1:wan"
		;;
	gl-ar300|\
	wnr2000-v3)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan"
		;;
	jwap230)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "5:wan" "6@eth1"
		;;
	nanostation-m-xw)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:lan" "1:wan"
		;;
	onion-omega)
		ucidef_set_interface_lan "wlan0"
		;;
	rb-435g)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan" "2:lan"
		;;
	rb-450)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5@eth1"
		;;
	rb-450g)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:1" "2:lan:4" "3:lan:3" "4:lan:2"
		;;
	routerstation-pro)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	rb-493g)
		ucidef_set_interfaces_lan_wan "eth0 eth1.1" "eth1.2"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan"
		ucidef_add_switch "switch1" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan"
		;;
	tellstick-znet-lite)
		ucidef_set_interface_wan "eth0"
		ucidef_set_interface_raw "wlan" "wlan0" "dhcp"
		;;
	tl-wdr4300|\
	tl-wr1041n-v2)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:2" "4:lan:3" "5:lan:4" "1:wan"
		;;
	tl-wpa8630)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:3" "3:lan:2" "4:lan:1" "5:lan:4"
		;;
	tl-wr1043nd)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "5@eth0"
		;;
	tl-wr2543n)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "9@eth0"
		;;
	tl-wr841n-v1|\
	tl-wr941nd)
		ucidef_set_interface_raw "eth" "eth0"
		ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "wan"
		;;
	tl-wr741nd|\
	tl-wr841n-v7)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:2" "3:lan:3" "4:lan:4"
		;;
	tl-wr842n-v2)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:1" "3:lan:2" "4:lan:3"
		;;
	uap-pro|\
	wpj342)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:wan"
		;;
	unifiac-pro|\
	xd3200)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:wan"
		;;
	wndr3700|\
	wndr3700v2|\
	wndr3800|\
	wndr3800ch)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5@eth0"

		ucidef_add_switch_attr "switch0" "blinkrate" 2
		ucidef_add_switch_port_attr "switch0" 1 led 6
		ucidef_add_switch_port_attr "switch0" 2 led 9
		ucidef_add_switch_port_attr "switch0" 5 led 2
		;;
	wpj344)
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan" "2:wan"
		;;
	wpj558)
		ucidef_add_switch "switch0" \
			"5:lan" "1:wan" "6@eth0"
		;;
	wrt160nl)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "4@eth0"
		;;
	wzr-hp-g450h)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1 3:lan:2 4:lan:3 5:lan:4" "1:wan"
		;;
	z1)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:2" "3:lan:3" "4:lan:4" "5:wan"
		;;
	*)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		;;
	esac
}

ar71xx_setup_macs()
{
	local board="$1"
	local lan_mac=""
	local wan_mac=""

	case $board in
	dgl-5500-a1|\
	dir-825-c1)
		wan_mac=$(mtd_get_mac_ascii nvram "wan_mac")
		;;
	dhp-1565-a1|\
	dir-835-a1|\
	wndr3700v4|\
	wndr4300)
		lan_mac=$(mtd_get_mac_binary caldata 0)
		wan_mac=$(mtd_get_mac_binary caldata 6)
		;;
	tl-wr1043nd-v4)
		lan_mac=$(mtd_get_mac_binary product-info 8)
		wan_mac=$(macaddr_add "$lan_mac" 1)
		;;
	esr900)
		wan_mac=$(mtd_get_mac_ascii u-boot-env "wanaddr")
		;;
	dir-869-a1|\
	mynet-n750)
		wan_mac=$(mtd_get_mac_ascii devdata "wanmac")
		;;
	esac

	[ -n "$lan_mac" ] && ucidef_set_interface_macaddr "lan" $lan_mac
	[ -n "$wan_mac" ] && ucidef_set_interface_macaddr "wan" $wan_mac
}

board_config_update
board=$(ar71xx_board_name)
ar71xx_setup_interfaces $board
ar71xx_setup_macs $board
board_config_flush

exit 0
