From 3526403353c2a1b94c3181f900582626d23c339b Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Thu, 18 Aug 2016 20:40:45 +0200
Subject: mfd: qcom_rpm: Handle message RAM clock
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The MSM8660, APQ8060, IPQ806x and MSM8960 have a GCC clock
to the message RAM used by the RPM. This needs to be enabled
for messages to pass through. This is a crude solution that
simply prepare/enable at probe() and disable/unprepare
at remove(). More elaborate PM is probably possible to
add later.

The construction uses IS_ERR() to gracefully handle the
platforms that do not provide a message RAM clock. It will
bail out of probe only if the clock is hitting a probe
deferral situation.

Of course this requires the proper device tree set-up:

rpm: rpm@104000 {
    compatible = "qcom,rpm-msm8660";
    clocks = <&gcc RPM_MSG_RAM_H_CLK>;
    clock-names = "ram";
    ...
};

I have provided this in the MSM8660 device tree, and will
provide patches for the other targets.

Cc: Björn Andersson <bjorn.andersson@linaro.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Signed-off-by: Lee Jones <lee.jones@linaro.org>
---
 drivers/mfd/qcom_rpm.c | 20 ++++++++++++++++++++
 1 file changed, 20 insertions(+)

--- a/drivers/mfd/qcom_rpm.c
+++ b/drivers/mfd/qcom_rpm.c
@@ -21,6 +21,7 @@
 #include <linux/mfd/qcom_rpm.h>
 #include <linux/mfd/syscon.h>
 #include <linux/regmap.h>
+#include <linux/clk.h>
 
 #include <dt-bindings/mfd/qcom-rpm.h>
 
@@ -48,6 +49,7 @@ struct qcom_rpm {
 	struct regmap *ipc_regmap;
 	unsigned ipc_offset;
 	unsigned ipc_bit;
+	struct clk *ramclk;
 
 	struct completion ack;
 	struct mutex lock;
@@ -503,6 +505,20 @@ static int qcom_rpm_probe(struct platfor
 	mutex_init(&rpm->lock);
 	init_completion(&rpm->ack);
 
+	/* Enable message RAM clock */
+	rpm->ramclk = devm_clk_get(&pdev->dev, "ram");
+	if (IS_ERR(rpm->ramclk)) {
+		ret = PTR_ERR(rpm->ramclk);
+		if (ret == -EPROBE_DEFER)
+			return ret;
+		/*
+		 * Fall through in all other cases, as the clock is
+		 * optional. (Does not exist on all platforms.)
+		 */
+		rpm->ramclk = NULL;
+	}
+	clk_prepare_enable(rpm->ramclk); /* Accepts NULL */
+
 	irq_ack = platform_get_irq_byname(pdev, "ack");
 	if (irq_ack < 0) {
 		dev_err(&pdev->dev, "required ack interrupt missing\n");
@@ -621,7 +637,11 @@ static int qcom_rpm_probe(struct platfor
 
 static int qcom_rpm_remove(struct platform_device *pdev)
 {
+	struct qcom_rpm *rpm = dev_get_drvdata(&pdev->dev);
+
 	of_platform_depopulate(&pdev->dev);
+	clk_disable_unprepare(rpm->ramclk);
+
 	return 0;
 }
 
