From 5c4ad318de3b8e8680d654c82a254c4b65243739 Mon Sep 17 00:00:00 2001
From: Felipe Balbi <balbi@kernel.org>
Date: Mon, 11 Apr 2016 17:12:34 +0300
Subject: usb: dwc3: core: fix PHY handling during suspend

we need to power off the PHY during suspend and
power it back on during resume.

Signed-off-by: Felipe Balbi <balbi@kernel.org>
[nsekhar@ti.com: fix call to usb_phy_set_suspend() in dwc3_suspend()]
Signed-off-by: Sekhar Nori <nsekhar@ti.com>
Signed-off-by: Roger Quadros <rogerq@ti.com>
Signed-off-by: Felipe Balbi <felipe.balbi@linux.intel.com>
---
 drivers/usb/dwc3/core.c | 23 ++++++++++++++++++++++-
 1 file changed, 22 insertions(+), 1 deletion(-)

--- a/drivers/usb/dwc3/core.c
+++ b/drivers/usb/dwc3/core.c
@@ -1124,6 +1124,11 @@ static int dwc3_suspend(struct device *d
 	phy_exit(dwc->usb2_generic_phy);
 	phy_exit(dwc->usb3_generic_phy);
 
+	usb_phy_set_suspend(dwc->usb2_phy, 1);
+	usb_phy_set_suspend(dwc->usb3_phy, 1);
+	WARN_ON(phy_power_off(dwc->usb2_generic_phy) < 0);
+	WARN_ON(phy_power_off(dwc->usb3_generic_phy) < 0);
+
 	pinctrl_pm_select_sleep_state(dev);
 
 	return 0;
@@ -1137,11 +1142,21 @@ static int dwc3_resume(struct device *de
 
 	pinctrl_pm_select_default_state(dev);
 
+	usb_phy_set_suspend(dwc->usb2_phy, 0);
+	usb_phy_set_suspend(dwc->usb3_phy, 0);
+	ret = phy_power_on(dwc->usb2_generic_phy);
+	if (ret < 0)
+		return ret;
+
+	ret = phy_power_on(dwc->usb3_generic_phy);
+	if (ret < 0)
+		goto err_usb2phy_power;
+
 	usb_phy_init(dwc->usb3_phy);
 	usb_phy_init(dwc->usb2_phy);
 	ret = phy_init(dwc->usb2_generic_phy);
 	if (ret < 0)
-		return ret;
+		goto err_usb3phy_power;
 
 	ret = phy_init(dwc->usb3_generic_phy);
 	if (ret < 0)
@@ -1174,6 +1189,12 @@ static int dwc3_resume(struct device *de
 err_usb2phy_init:
 	phy_exit(dwc->usb2_generic_phy);
 
+err_usb3phy_power:
+	phy_power_off(dwc->usb3_generic_phy);
+
+err_usb2phy_power:
+	phy_power_off(dwc->usb2_generic_phy);
+
 	return ret;
 }
 
