--- a/arch/arm/boot/dts/imx6qdl-gw51xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw51xx.dtsi
@@ -158,6 +158,11 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&pinctrl_i2c2>;
 	status = "okay";
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &i2c3 {
--- a/arch/arm/boot/dts/imx6qdl-gw52xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw52xx.dtsi
@@ -233,6 +233,11 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&pinctrl_i2c2>;
 	status = "okay";
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &i2c3 {
--- a/arch/arm/boot/dts/imx6qdl-gw53xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw53xx.dtsi
@@ -226,6 +226,11 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&pinctrl_i2c2>;
 	status = "okay";
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &i2c3 {
--- a/arch/arm/boot/dts/imx6qdl-gw54xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw54xx.dtsi
@@ -317,6 +317,11 @@
 			};
 		};
 	};
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &i2c3 {
