From 59aafd667d2880c90776931b6102b8252214d93c Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sun, 21 Feb 2016 13:52:12 +0100
Subject: [PATCH 026/102] scpsys: various fixes

---
 drivers/clk/mediatek/clk-mt2701.c        |    2 ++
 drivers/soc/mediatek/mtk-scpsys-mt2701.c |    8 --------
 include/dt-bindings/power/mt2701-power.h |    4 ++--
 3 files changed, 4 insertions(+), 10 deletions(-)

--- a/drivers/clk/mediatek/clk-mt2701.c
+++ b/drivers/clk/mediatek/clk-mt2701.c
@@ -1043,6 +1043,8 @@ static void __init mtk_ethsys_init(struc
 	if (r)
 		pr_err("%s(): could not register clock provider: %d\n",
 			__func__, r);
+
+	mtk_register_reset_controller(node, 1, 0x34);
 }
 CLK_OF_DECLARE(mtk_ethsys, "mediatek,mt2701-ethsys", mtk_ethsys_init);
 
--- a/drivers/soc/mediatek/mtk-scpsys-mt2701.c
+++ b/drivers/soc/mediatek/mtk-scpsys-mt2701.c
@@ -61,14 +61,6 @@ static const struct scp_domain_data scp_
 		.bus_prot_mask = MT2701_TOP_AXI_PROT_EN_DISP,
 		.active_wakeup = true,
 	},
-	[MT2701_POWER_DOMAIN_MFG] = {
-		.name = "mfg",
-		.sta_mask = MFG_PWR_STA_MASK,
-		.ctl_offs = SPM_MFG_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(12, 12),
-		.active_wakeup = true,
-	},
 	[MT2701_POWER_DOMAIN_VDEC] = {
 		.name = "vdec",
 		.sta_mask = VDE_PWR_STA_MASK,
--- a/include/dt-bindings/power/mt2701-power.h
+++ b/include/dt-bindings/power/mt2701-power.h
@@ -16,12 +16,12 @@
 
 #define MT2701_POWER_DOMAIN_CONN	0
 #define MT2701_POWER_DOMAIN_DISP	1
-#define MT2701_POWER_DOMAIN_MFG		2
+//#define MT2701_POWER_DOMAIN_MFG		2
 #define MT2701_POWER_DOMAIN_VDEC	3
 #define MT2701_POWER_DOMAIN_ISP		4
 #define MT2701_POWER_DOMAIN_BDP		5
 #define MT2701_POWER_DOMAIN_ETH		6
 #define MT2701_POWER_DOMAIN_HIF		7
-#define MT2701_POWER_DOMAIN_IFR_MSC	8
+#define MT2701_POWER_DOMAIN_IFR_MSC	2
 
 #endif /* _DT_BINDINGS_POWER_MT2701_POWER_H */
