From 3ce895cbe3469bfcaa84674ec4f1b2d60e8b370b Mon Sep 17 00:00:00 2001
From: Mingkai Hu <Mingkai.Hu@freescale.com>
Date: Mon, 21 Jul 2014 14:48:42 +0800
Subject: [PATCH 01/70] arm64/ls1043a: add DTS for Freescale LS1043A SoC

LS1043a is an SoC with 4 ARMv8 A53 cores and most other IP blocks
similar to LS1021a which complies to Chassis 2.1 spec.

Following levels of DTSI/DTS files have been created for the
LS1043A SoC family:

- fsl-ls1043a.dtsi:
  DTS-Include file for FSL LS1043A SoC.

Signed-off-by: Li Yang <leoli@freescale.com>
Signed-off-by: Hou Zhiqiang <B48286@freescale.com>
Signed-off-by: Mingkai Hu <Mingkai.Hu@freescale.com>
Signed-off-by: Wenbin Song <Wenbin.Song@freescale.com>
Signed-off-by: Mingkai Hu <mingkai.hu@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi |  525 ++++++++++++++++++++++++
 1 file changed, 525 insertions(+)
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi

--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -0,0 +1,525 @@
+/*
+ * Device Tree Include file for Freescale Layerscape-1043A family SoC.
+ *
+ * Copyright 2014-2015, Freescale Semiconductor
+ *
+ * Mingkai Hu <Mingkai.hu@freescale.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPLv2 or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This library is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This library is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/ {
+	compatible = "fsl,ls1043a";
+	interrupt-parent = <&gic>;
+	#address-cells = <2>;
+	#size-cells = <2>;
+
+	cpus {
+		#address-cells = <2>;
+		#size-cells = <0>;
+
+		/*
+		 * We expect the enable-method for cpu's to be "psci", but this
+		 * is dependent on the SoC FW, which will fill this in.
+		 *
+		 * Currently supported enable-method is psci v0.2
+		 */
+		cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x0 0x0>;
+			clocks = <&clockgen 1 0>;
+		};
+
+		cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x0 0x1>;
+			clocks = <&clockgen 1 0>;
+		};
+
+		cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x0 0x2>;
+			clocks = <&clockgen 1 0>;
+		};
+
+		cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a53";
+			reg = <0x0 0x3>;
+			clocks = <&clockgen 1 0>;
+		};
+	};
+
+	memory@80000000 {
+		device_type = "memory";
+		reg = <0x0 0x80000000 0 0x80000000>;
+		      /* DRAM space 1, size: 2GiB DRAM */
+	};
+
+	sysclk: sysclk {
+		compatible = "fixed-clock";
+		#clock-cells = <0>;
+		clock-frequency = <100000000>;
+		clock-output-names = "sysclk";
+	};
+
+	timer {
+		compatible = "arm,armv8-timer";
+		interrupts = <1 13 0x1>, /* Physical Secure PPI */
+			     <1 14 0x1>, /* Physical Non-Secure PPI */
+			     <1 11 0x1>, /* Virtual PPI */
+			     <1 10 0x1>; /* Hypervisor PPI */
+	};
+
+	pmu {
+		compatible = "arm,armv8-pmuv3";
+		interrupts = <0 106 0x4>,
+			     <0 107 0x4>,
+			     <0 95 0x4>,
+			     <0 97 0x4>;
+		interrupt-affinity = <&cpu0>,
+				     <&cpu1>,
+				     <&cpu2>,
+				     <&cpu3>;
+	};
+
+	gic: interrupt-controller@1400000 {
+		compatible = "arm,gic-400";
+		#interrupt-cells = <3>;
+		interrupt-controller;
+		reg = <0x0 0x1401000 0 0x1000>, /* GICD */
+		      <0x0 0x1402000 0 0x2000>, /* GICC */
+		      <0x0 0x1404000 0 0x2000>, /* GICH */
+		      <0x0 0x1406000 0 0x2000>; /* GICV */
+		interrupts = <1 9 0xf08>;
+	};
+
+	soc {
+		compatible = "simple-bus";
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		clockgen: clocking@1ee1000 {
+			compatible = "fsl,ls1043a-clockgen";
+			reg = <0x0 0x1ee1000 0x0 0x1000>;
+			#clock-cells = <2>;
+			clocks = <&sysclk>;
+		};
+
+		scfg: scfg@1570000 {
+			compatible = "fsl,ls1043a-scfg", "syscon";
+			reg = <0x0 0x1570000 0x0 0x10000>;
+			big-endian;
+		};
+
+		dcfg: dcfg@1ee0000 {
+			compatible = "fsl,ls1043a-dcfg", "syscon";
+			reg = <0x0 0x1ee0000 0x0 0x10000>;
+		};
+
+		ifc: ifc@1530000 {
+			compatible = "fsl,ifc", "simple-bus";
+			reg = <0x0 0x1530000 0x0 0x10000>;
+			interrupts = <0 43 0x4>;
+		};
+
+		esdhc: esdhc@1560000 {
+			compatible = "fsl,ls1043a-esdhc", "fsl,esdhc";
+			reg = <0x0 0x1560000 0x0 0x10000>;
+			interrupts = <0 62 0x4>;
+			clock-frequency = <0>;
+			voltage-ranges = <1800 1800 3300 3300>;
+			sdhci,auto-cmd12;
+			big-endian;
+			bus-width = <4>;
+		};
+
+		dspi0: dspi@2100000 {
+			compatible = "fsl,ls1043a-dspi", "fsl,ls1021a-v1.0-dspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2100000 0x0 0x10000>;
+			interrupts = <0 64 0x4>;
+			clock-names = "dspi";
+			clocks = <&clockgen 4 0>;
+			spi-num-chipselects = <5>;
+			big-endian;
+			status = "disabled";
+		};
+
+		dspi1: dspi@2110000 {
+			compatible = "fsl,ls1043a-dspi", "fsl,ls1021a-v1.0-dspi";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2110000 0x0 0x10000>;
+			interrupts = <0 65 0x4>;
+			clock-names = "dspi";
+			clocks = <&clockgen 4 0>;
+			spi-num-chipselects = <5>;
+			big-endian;
+			status = "disabled";
+		};
+
+		i2c0: i2c@2180000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2180000 0x0 0x10000>;
+			interrupts = <0 56 0x4>;
+			clock-names = "i2c";
+			clocks = <&clockgen 4 0>;
+			dmas = <&edma0 1 39>,
+			       <&edma0 1 38>;
+			dma-names = "tx", "rx";
+			status = "disabled";
+		};
+
+		i2c1: i2c@2190000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x2190000 0x0 0x10000>;
+			interrupts = <0 57 0x4>;
+			clock-names = "i2c";
+			clocks = <&clockgen 4 0>;
+			status = "disabled";
+		};
+
+		i2c2: i2c@21a0000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x21a0000 0x0 0x10000>;
+			interrupts = <0 58 0x4>;
+			clock-names = "i2c";
+			clocks = <&clockgen 4 0>;
+			status = "disabled";
+		};
+
+		i2c3: i2c@21b0000 {
+			compatible = "fsl,vf610-i2c";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			reg = <0x0 0x21b0000 0x0 0x10000>;
+			interrupts = <0 59 0x4>;
+			clock-names = "i2c";
+			clocks = <&clockgen 4 0>;
+			status = "disabled";
+		};
+
+		duart0: serial@21c0500 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x00 0x21c0500 0x0 0x100>;
+			interrupts = <0 54 0x4>;
+			clocks = <&clockgen 4 0>;
+		};
+
+		duart1: serial@21c0600 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x00 0x21c0600 0x0 0x100>;
+			interrupts = <0 54 0x4>;
+			clocks = <&clockgen 4 0>;
+		};
+
+		duart2: serial@21d0500 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21d0500 0x0 0x100>;
+			interrupts = <0 55 0x4>;
+			clocks = <&clockgen 4 0>;
+		};
+
+		duart3: serial@21d0600 {
+			compatible = "fsl,ns16550", "ns16550a";
+			reg = <0x0 0x21d0600 0x0 0x100>;
+			interrupts = <0 55 0x4>;
+			clocks = <&clockgen 4 0>;
+		};
+
+		gpio1: gpio@2300000 {
+			compatible = "fsl,ls1043a-gpio";
+			reg = <0x0 0x2300000 0x0 0x10000>;
+			interrupts = <0 66 0x4>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio2: gpio@2310000 {
+			compatible = "fsl,ls1043a-gpio";
+			reg = <0x0 0x2310000 0x0 0x10000>;
+			interrupts = <0 67 0x4>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio3: gpio@2320000 {
+			compatible = "fsl,ls1043a-gpio";
+			reg = <0x0 0x2320000 0x0 0x10000>;
+			interrupts = <0 68 0x4>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		gpio4: gpio@2330000 {
+			compatible = "fsl,ls1043a-gpio";
+			reg = <0x0 0x2330000 0x0 0x10000>;
+			interrupts = <0 134 0x4>;
+			gpio-controller;
+			#gpio-cells = <2>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		lpuart0: serial@2950000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2950000 0x0 0x1000>;
+			interrupts = <0 48 0x4>;
+			clocks = <&clockgen 0 0>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart1: serial@2960000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2960000 0x0 0x1000>;
+			interrupts = <0 49 0x4>;
+			clocks = <&clockgen 4 0>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart2: serial@2970000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2970000 0x0 0x1000>;
+			interrupts = <0 50 0x4>;
+			clocks = <&clockgen 4 0>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart3: serial@2980000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2980000 0x0 0x1000>;
+			interrupts = <0 51 0x4>;
+			clocks = <&clockgen 4 0>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart4: serial@2990000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x2990000 0x0 0x1000>;
+			interrupts = <0 52 0x4>;
+			clocks = <&clockgen 4 0>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		lpuart5: serial@29a0000 {
+			compatible = "fsl,ls1021a-lpuart";
+			reg = <0x0 0x29a0000 0x0 0x1000>;
+			interrupts = <0 53 0x4>;
+			clocks = <&clockgen 4 0>;
+			clock-names = "ipg";
+			status = "disabled";
+		};
+
+		wdog0: wdog@2ad0000 {
+			compatible = "fsl,ls1043a-wdt", "fsl,imx21-wdt";
+			reg = <0x0 0x2ad0000 0x0 0x10000>;
+			interrupts = <0 83 0x4>;
+			clocks = <&clockgen 4 0>;
+			clock-names = "wdog";
+			big-endian;
+		};
+
+		edma0: edma@2c00000 {
+			#dma-cells = <2>;
+			compatible = "fsl,vf610-edma";
+			reg = <0x0 0x2c00000 0x0 0x10000>,
+			      <0x0 0x2c10000 0x0 0x10000>,
+			      <0x0 0x2c20000 0x0 0x10000>;
+			interrupts = <0 103 0x4>,
+				     <0 103 0x4>;
+			interrupt-names = "edma-tx", "edma-err";
+			dma-channels = <32>;
+			big-endian;
+			clock-names = "dmamux0", "dmamux1";
+			clocks = <&clockgen 4 0>,
+				 <&clockgen 4 0>;
+		};
+
+		usb0: usb3@2f00000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x2f00000 0x0 0x10000>;
+			interrupts = <0 60 0x4>;
+			dr_mode = "host";
+		};
+
+		usb1: usb3@3000000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3000000 0x0 0x10000>;
+			interrupts = <0 61 0x4>;
+			dr_mode = "host";
+		};
+
+		usb2: usb3@3100000 {
+			compatible = "snps,dwc3";
+			reg = <0x0 0x3100000 0x0 0x10000>;
+			interrupts = <0 63 0x4>;
+			dr_mode = "host";
+		};
+
+		sata: sata@3200000 {
+			compatible = "fsl,ls1043a-ahci";
+			reg = <0x0 0x3200000 0x0 0x10000>;
+			interrupts = <0 69 0x4>;
+			clocks = <&clockgen 4 0>;
+		};
+
+		msi1: msi-controller1@1571000 {
+			compatible = "fsl,1s1043a-msi";
+			reg = <0x0 0x1571000 0x0 0x4>,
+			      <0x0 0x1571004 0x0 0x4>;
+			reg-names = "msiir", "msir";
+			msi-controller;
+			interrupts = <0 116 0x4>;
+		};
+
+		msi2: msi-controller2@1572000 {
+			compatible = "fsl,1s1043a-msi";
+			reg = <0x0 0x1572000 0x0 0x4>,
+			      <0x0 0x1572004 0x0 0x4>;
+			reg-names = "msiir", "msir";
+			msi-controller;
+			interrupts = <0 126 0x4>;
+		};
+
+		msi3: msi-controller3@1573000 {
+			compatible = "fsl,1s1043a-msi";
+			reg = <0x0 0x1573000 0x0 0x4>,
+			      <0x0 0x1573004 0x0 0x4>;
+			reg-names = "msiir", "msir";
+			msi-controller;
+			interrupts = <0 160 0x4>;
+		};
+
+		pcie@3400000 {
+			compatible = "fsl,ls1043a-pcie", "snps,dw-pcie";
+			reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
+			       0x40 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <0 118 0x4>, /* controller interrupt */
+				     <0 117 0x4>; /* PME interrupt */
+			interrupt-names = "intr", "pme";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			num-lanes = <4>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x40 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x40 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&msi1>;
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 110 0x4>,
+					<0000 0 0 2 &gic 0 111 0x4>,
+					<0000 0 0 3 &gic 0 112 0x4>,
+					<0000 0 0 4 &gic 0 113 0x4>;
+		};
+
+		pcie@3500000 {
+			compatible = "fsl,ls1043a-pcie", "snps,dw-pcie";
+			reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
+			       0x48 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <0 128 0x4>,
+				     <0 127 0x4>;
+			interrupt-names = "intr", "pme";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			num-lanes = <2>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x48 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x48 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&msi2>;
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 120  0x4>,
+					<0000 0 0 2 &gic 0 121 0x4>,
+					<0000 0 0 3 &gic 0 122 0x4>,
+					<0000 0 0 4 &gic 0 123 0x4>;
+		};
+
+		pcie@3600000 {
+			compatible = "fsl,ls1043a-pcie", "snps,dw-pcie";
+			reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
+			       0x50 0x00000000 0x0 0x00002000>; /* configuration space */
+			reg-names = "regs", "config";
+			interrupts = <0 162 0x4>,
+				     <0 161 0x4>;
+			interrupt-names = "intr", "pme";
+			#address-cells = <3>;
+			#size-cells = <2>;
+			device_type = "pci";
+			num-lanes = <2>;
+			bus-range = <0x0 0xff>;
+			ranges = <0x81000000 0x0 0x00000000 0x50 0x00010000 0x0 0x00010000   /* downstream I/O */
+				  0x82000000 0x0 0x40000000 0x50 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
+			msi-parent = <&msi3>;
+			#interrupt-cells = <1>;
+			interrupt-map-mask = <0 0 0 7>;
+			interrupt-map = <0000 0 0 1 &gic 0 154 0x4>,
+					<0000 0 0 2 &gic 0 155 0x4>,
+					<0000 0 0 3 &gic 0 156 0x4>,
+					<0000 0 0 4 &gic 0 157 0x4>;
+		};
+	};
+
+};
