From 77eff1bfa410edc8c6cc2fb5441aaac2054ebb5c Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 12 May 2016 08:52:06 +0100
Subject: [PATCH] BCM270X_DT: Include address override for pca9542

Omitted from "BCM270X_DT: Add umbrella I2C Mux overlay i2c-mux".

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/i2c-mux-overlay.dts | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/i2c-mux-overlay.dts
+++ b/arch/arm/boot/dts/overlays/i2c-mux-overlay.dts
@@ -132,7 +132,8 @@
 		pca9545 = <0>, "+1";
 		pca9548 = <0>, "+2";
 
-		addr =  <&pca9545>,"reg:0",
+		addr =  <&pca9542>,"reg:0",
+			<&pca9545>,"reg:0",
 			<&pca9548>,"reg:0";
 	};
 };
