From 37faf877fc9db93893b313190f688c56f51ea1fd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Noralf=20Tr=C3=B8nnes?= <noralf@tronnes.org>
Date: Fri, 26 Jun 2015 14:21:20 +0200
Subject: [PATCH] firmware: bcm2835: Add missing property tags
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Noralf Trønnes <noralf@tronnes.org>
---
 include/soc/bcm2835/raspberrypi-firmware.h | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/include/soc/bcm2835/raspberrypi-firmware.h
+++ b/include/soc/bcm2835/raspberrypi-firmware.h
@@ -63,6 +63,7 @@ enum rpi_firmware_property_tag {
 	RPI_FIRMWARE_GET_MIN_VOLTAGE =                        0x00030008,
 	RPI_FIRMWARE_GET_TURBO =                              0x00030009,
 	RPI_FIRMWARE_GET_MAX_TEMPERATURE =                    0x0003000a,
+	RPI_FIRMWARE_GET_STC =                                0x0003000b,
 	RPI_FIRMWARE_ALLOCATE_MEMORY =                        0x0003000c,
 	RPI_FIRMWARE_LOCK_MEMORY =                            0x0003000d,
 	RPI_FIRMWARE_UNLOCK_MEMORY =                          0x0003000e,
@@ -72,10 +73,12 @@ enum rpi_firmware_property_tag {
 	RPI_FIRMWARE_SET_ENABLE_QPU =                         0x00030012,
 	RPI_FIRMWARE_GET_DISPMANX_RESOURCE_MEM_HANDLE =       0x00030014,
 	RPI_FIRMWARE_GET_EDID_BLOCK =                         0x00030020,
+	RPI_FIRMWARE_GET_CUSTOMER_OTP =                       0x00030021,
 	RPI_FIRMWARE_SET_CLOCK_STATE =                        0x00038001,
 	RPI_FIRMWARE_SET_CLOCK_RATE =                         0x00038002,
 	RPI_FIRMWARE_SET_VOLTAGE =                            0x00038003,
 	RPI_FIRMWARE_SET_TURBO =                              0x00038009,
+	RPI_FIRMWARE_SET_CUSTOMER_OTP =                       0x00038021,
 
 	/* Dispmanx TAGS */
 	RPI_FIRMWARE_FRAMEBUFFER_ALLOCATE =                   0x00040001,
@@ -89,6 +92,7 @@ enum rpi_firmware_property_tag {
 	RPI_FIRMWARE_FRAMEBUFFER_GET_VIRTUAL_OFFSET =         0x00040009,
 	RPI_FIRMWARE_FRAMEBUFFER_GET_OVERSCAN =               0x0004000a,
 	RPI_FIRMWARE_FRAMEBUFFER_GET_PALETTE =                0x0004000b,
+	RPI_FIRMWARE_FRAMEBUFFER_GET_TOUCHBUF =               0x0004000f,
 	RPI_FIRMWARE_FRAMEBUFFER_RELEASE =                    0x00048001,
 	RPI_FIRMWARE_FRAMEBUFFER_TEST_PHYSICAL_WIDTH_HEIGHT = 0x00044003,
 	RPI_FIRMWARE_FRAMEBUFFER_TEST_VIRTUAL_WIDTH_HEIGHT =  0x00044004,
@@ -98,6 +102,7 @@ enum rpi_firmware_property_tag {
 	RPI_FIRMWARE_FRAMEBUFFER_TEST_VIRTUAL_OFFSET =        0x00044009,
 	RPI_FIRMWARE_FRAMEBUFFER_TEST_OVERSCAN =              0x0004400a,
 	RPI_FIRMWARE_FRAMEBUFFER_TEST_PALETTE =               0x0004400b,
+	RPI_FIRMWARE_FRAMEBUFFER_TEST_VSYNC =                 0x0004400e,
 	RPI_FIRMWARE_FRAMEBUFFER_SET_PHYSICAL_WIDTH_HEIGHT =  0x00048003,
 	RPI_FIRMWARE_FRAMEBUFFER_SET_VIRTUAL_WIDTH_HEIGHT =   0x00048004,
 	RPI_FIRMWARE_FRAMEBUFFER_SET_DEPTH =                  0x00048005,
@@ -106,6 +111,9 @@ enum rpi_firmware_property_tag {
 	RPI_FIRMWARE_FRAMEBUFFER_SET_VIRTUAL_OFFSET =         0x00048009,
 	RPI_FIRMWARE_FRAMEBUFFER_SET_OVERSCAN =               0x0004800a,
 	RPI_FIRMWARE_FRAMEBUFFER_SET_PALETTE =                0x0004800b,
+	RPI_FIRMWARE_FRAMEBUFFER_SET_VSYNC =                  0x0004800e,
+
+	RPI_FIRMWARE_VCHIQ_INIT =                             0x00048010,
 
 	RPI_FIRMWARE_GET_COMMAND_LINE =                       0x00050001,
 	RPI_FIRMWARE_GET_DMA_CHANNELS =                       0x00060001,
