From 5ab1a37c6027c114a87a1ae32cfc5ef303d643c5 Mon Sep 17 00:00:00 2001
From: Boris Brezillon <boris.brezillon@free-electrons.com>
Date: Fri, 2 Dec 2016 14:48:13 +0100
Subject: [PATCH] ARM: dts: bcm283x: Enable the VEC IP on all RaspberryPi
 boards

Enable the VEC IP on all RaspberryPi boards.

Signed-off-by: Boris Brezillon <boris.brezillon@free-electrons.com>
Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm2835-rpi.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

--- a/arch/arm/boot/dts/bcm2835-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2835-rpi.dtsi
@@ -87,3 +87,8 @@
 	power-domains = <&power RPI_POWER_DOMAIN_HDMI>;
 	status = "okay";
 };
+
+&vec {
+	power-domains = <&power RPI_POWER_DOMAIN_VEC>;
+	status = "okay";
+};
